(footprint "MOSFET-N-2CH-DMT3020-SO-8"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SO, 8 Pin (https://www.ti.com/lit/ml/msop001a/msop001a.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "SO SO")
	(property "Reference" "REF**"
		(at 0 -4.05 0)
		(layer "F.SilkS")
		(uuid "4cc14baa-3def-4b49-a9a3-68085445d04d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "MOSFET-N-2CH-DMT3020-SO-8"
		(at 0 4.05 0)
		(layer "F.Fab")
		(uuid "28b74d9f-3781-449f-be99-8cb9b73c0f33")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "93e2d15a-53b4-481f-b8de-16280bf221f1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "42103509-512b-44a2-97e1-65c85d44b383")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7d09ef97-947c-4492-9ffb-a7c787687f4b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.76 -3.21)
		(end -2.76 -2.465)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "15003fa0-f48d-40a7-939d-9b7630521fe1")
	)
	(fp_line
		(start -2.76 3.21)
		(end -2.76 2.465)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b566c35f-bd8f-42e2-96c7-ba03d80b5532")
	)
	(fp_line
		(start 0 -3.21)
		(end -2.76 -3.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d534bcd5-df85-44df-8348-fb4856c5bae1")
	)
	(fp_line
		(start 0 -3.21)
		(end 2.76 -3.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c0502cfd-fc2f-4b77-814b-f09cc49cba6b")
	)
	(fp_line
		(start 0 3.21)
		(end -2.76 3.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "97922497-e836-4c2f-943c-1fea2658a945")
	)
	(fp_line
		(start 0 3.21)
		(end 2.76 3.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c2df4492-7637-40aa-aba2-dbae222386ef")
	)
	(fp_line
		(start 2.76 -3.21)
		(end 2.76 -2.465)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "bc46b0e6-a61f-4ca8-a49b-b1c8fd1d3530")
	)
	(fp_line
		(start 2.76 3.21)
		(end 2.76 2.465)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6384290d-4723-4b4f-9706-8813537121e9")
	)
	(fp_poly
		(pts
			(xy -3.55 -2.465) (xy -3.79 -2.795) (xy -3.31 -2.795) (xy -3.55 -2.465)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "33ac3011-7895-4484-9336-fa9f2de9404b")
	)
	(fp_line
		(start -4.7 -3.35)
		(end -4.7 3.35)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "44383ba6-383b-462d-8d46-cd7616fb134c")
	)
	(fp_line
		(start -4.7 3.35)
		(end 4.7 3.35)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4401ef1c-bea4-4b14-aa0b-840e54c24f91")
	)
	(fp_line
		(start 4.7 -3.35)
		(end -4.7 -3.35)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "eb3729a7-6484-4c24-b1cc-e630c872c7eb")
	)
	(fp_line
		(start 4.7 3.35)
		(end 4.7 -3.35)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "47cc2593-7a3e-4f79-8d6d-7b6bf60e9d55")
	)
	(fp_line
		(start -2.65 -2.1)
		(end -1.65 -3.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0bf121d7-ceba-44d6-b0a9-25691ddb0c83")
	)
	(fp_line
		(start -2.65 3.1)
		(end -2.65 -2.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "90c29bd7-506b-4639-b8e3-d33d771a2e55")
	)
	(fp_line
		(start -1.65 -3.1)
		(end 2.65 -3.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8571f730-a775-4338-9da9-1ebf3d0912b1")
	)
	(fp_line
		(start 2.65 -3.1)
		(end 2.65 3.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "13c085cd-a79e-4e36-bc49-355c8ca1a2d9")
	)
	(fp_line
		(start 2.65 3.1)
		(end -2.65 3.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "43afea7c-3d02-411b-93e9-3a33d1973485")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "4f23a516-d8fe-4dbb-8598-e7876c3336a6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.5 -1.905)
		(size 1.9 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "e114aa41-c8b2-4ecd-9d04-9fab82308e30")
	)
	(pad "2" smd roundrect
		(at -3.5 -0.635)
		(size 1.9 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "c3ecaa29-40bf-48cb-8cf4-4992c7c4cffb")
	)
	(pad "3" smd roundrect
		(at -3.5 0.635)
		(size 1.9 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "2515847e-4a9f-4b8d-ad93-24c796183357")
	)
	(pad "4" smd roundrect
		(at -3.5 1.905)
		(size 1.9 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "694037ec-f4eb-4cd0-87e3-b5c0d2fdc3b2")
	)
	(pad "5" smd roundrect
		(at 3.5 1.905)
		(size 1.9 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "ce4bba4d-649c-460f-981c-5695ba9a7023")
	)
	(pad "6" smd roundrect
		(at 3.5 0.635)
		(size 1.9 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "74a85224-ca81-40fc-baff-2bc4a5fdabb3")
	)
	(pad "7" smd roundrect
		(at 3.5 -0.635)
		(size 1.9 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "07adabc5-aaaf-4645-8c79-928cebb69273")
	)
	(pad "8" smd roundrect
		(at 3.5 -1.905)
		(size 1.9 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "b8eab1f2-7583-4cd6-b172-2f861e1beaa6")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_5.3x6.2mm_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
