(footprint "ESP32-S3-WROOM-2-N32R8V"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -6.575 -14.135 0)
		(layer "F.SilkS")
		(uuid "0b32be73-f918-40f8-b24a-b4d1876e8fe9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "ESP32-S3-WROOM-2-N32R8V"
		(at 8.03 14.365 0)
		(layer "F.Fab")
		(uuid "9969f794-560e-4ebc-afd9-c55f51dfcad4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "ee392990-c044-485e-a493-c3f42c7214f8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2e61eba2-1377-4120-833c-51e6b3132a90")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "68751851-cbaf-45e9-9e50-22dc4135a40e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -9 -12.75)
		(end 9 -12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a3bba1e3-4a35-4547-8bd6-83fd65970c44")
	)
	(fp_line
		(start -9 -6.03)
		(end -9 -12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c5f054d6-9b38-4eb7-a5b5-a108b3b515b4")
	)
	(fp_line
		(start -9 12.02)
		(end -9 12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c04ae80c-cb1a-4373-87bc-dd53bc2f5561")
	)
	(fp_line
		(start -9 12.75)
		(end -7.755 12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "981b0b1f-3fc7-4fed-92f1-c72dd9d399cc")
	)
	(fp_line
		(start 9 -12.75)
		(end 9 -6.03)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b52dd884-8c3e-4fa1-9ba4-7c441f424a2d")
	)
	(fp_line
		(start 9 12.02)
		(end 9 12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2e10571f-80c4-4d85-902c-690eb29bc204")
	)
	(fp_line
		(start 9 12.75)
		(end 7.755 12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f2cb9a29-4094-46ad-84e1-2d09c0cd52db")
	)
	(fp_circle
		(center -10.2 -5.26)
		(end -10.1 -5.26)
		(stroke
			(width 0.2)
			(type solid)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "b30beda7-8caf-4ed2-8b21-f6817373f2b7")
	)
	(fp_line
		(start -9.75 -13)
		(end 9.75 -13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c5fd7943-434b-4db3-85c0-c064c318d953")
	)
	(fp_line
		(start -9.75 13.5)
		(end -9.75 -13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fb2f25b4-6d85-4c0a-a89a-05dda7a2cfce")
	)
	(fp_line
		(start -9.75 13.5)
		(end 9.75 13.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7d8bcec6-19c8-45eb-9d2f-18e6d4e563ac")
	)
	(fp_line
		(start 9.75 -13)
		(end 9.75 13.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fd4b9d9e-1725-4f42-8b2f-4e19f9ec99ab")
	)
	(fp_line
		(start -9 -12.75)
		(end 9 -12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d4e87384-b016-49d1-a12f-1642b268b55d")
	)
	(fp_line
		(start -9 -6.75)
		(end -9 -12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5694ecfb-4c40-467a-acf3-d77aaf2b0635")
	)
	(fp_line
		(start -9 -6.75)
		(end 9 -6.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1209d15e-6138-41c2-8b5b-68a6bfcd8ef3")
	)
	(fp_line
		(start -9 12.75)
		(end -9 -6.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "11974dde-f86a-477a-a291-46942fe8b875")
	)
	(fp_line
		(start 9 -12.75)
		(end 9 -6.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7dd82a66-0832-45bc-8dfd-32e1f4febaf0")
	)
	(fp_line
		(start 9 -6.75)
		(end 9 12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "697defde-8a59-4aa1-9dd2-02b8f7c198a3")
	)
	(fp_line
		(start 9 12.75)
		(end -9 12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "aec9b56f-81bc-4533-9a13-1ee78343fb81")
	)
	(fp_circle
		(center -10.2 -5.26)
		(end -10.1 -5.26)
		(stroke
			(width 0.2)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "79db4b67-30bd-4812-818c-38e73ecb3f25")
	)
	(fp_text user "ANTENNA"
		(at -4.5 -9.5 0)
		(layer "F.Fab")
		(uuid "6c5d7a7e-9f38-4d74-bcdd-fd0e8fbe6b08")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -8.75 -5.26)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "a7b36064-e425-4292-a84d-36f1fb4bcaa4")
	)
	(pad "2" smd rect
		(at -8.75 -3.99)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "31c67fc4-b452-48c6-bac3-c5ea30998bda")
	)
	(pad "3" smd rect
		(at -8.75 -2.72)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "c230c7a7-1f1c-4fc3-91df-ce02d692ebb9")
	)
	(pad "4" smd rect
		(at -8.75 -1.45)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "306109ee-c6d1-4db9-91c9-2ab97ec18e20")
	)
	(pad "5" smd rect
		(at -8.75 -0.18)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "d3e9f717-03b9-4d0d-8722-19e9571057d9")
	)
	(pad "6" smd rect
		(at -8.75 1.09)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "fb691635-0d6d-45d4-b3fb-9d7cc443d13f")
	)
	(pad "7" smd rect
		(at -8.75 2.36)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "ccd08626-04a2-40da-92f5-4898f7b6da64")
	)
	(pad "8" smd rect
		(at -8.75 3.63)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "5d3114bb-fca4-4098-ba3b-58507c9a6d3c")
	)
	(pad "9" smd rect
		(at -8.75 4.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "a06ad093-73fc-4c39-8725-a5908bf1e70e")
	)
	(pad "10" smd rect
		(at -8.75 6.17)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "7f911e9c-d39a-41b3-8841-45fd5e5693d7")
	)
	(pad "11" smd rect
		(at -8.75 7.44)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "2befa670-bc07-44a7-90b3-3b6f756d505f")
	)
	(pad "12" smd rect
		(at -8.75 8.71)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "a7273328-4130-4423-9fa6-af13321e344d")
	)
	(pad "13" smd rect
		(at -8.75 9.98)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "137de360-6ed4-472c-95dd-ce041117f8e3")
	)
	(pad "14" smd rect
		(at -8.75 11.25)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "fe422d42-a1d6-43c1-ae33-e7a8f5e21046")
	)
	(pad "15" smd rect
		(at -6.985 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "c1eecd55-9987-4233-97df-c4006503035d")
	)
	(pad "16" smd rect
		(at -5.715 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "8c9ee5f4-93c9-49cc-98c9-905038580dc9")
	)
	(pad "17" smd rect
		(at -4.445 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "55fd4e3d-a6f9-4e76-8936-b72932d81d42")
	)
	(pad "18" smd rect
		(at -3.175 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "a5e9e6f8-6414-46ad-a1f6-aaa593f3822a")
	)
	(pad "19" smd rect
		(at -1.905 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "f20283d8-f578-4cca-b6fe-41e396884925")
	)
	(pad "20" smd rect
		(at -0.635 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "5e1b2f86-4bfb-48a0-a667-04c3acb9603b")
	)
	(pad "21" smd rect
		(at 0.635 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "b5e1638c-71d6-4cca-b5a5-acd29691c3e0")
	)
	(pad "22" smd rect
		(at 1.905 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "8b932f76-54b7-497f-ac9a-55c96d97caa2")
	)
	(pad "23" smd rect
		(at 3.175 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "42075176-49bc-4251-a1c0-a9096f3797a5")
	)
	(pad "24" smd rect
		(at 4.445 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "045b724f-d98b-429e-b0a8-e142759dc750")
	)
	(pad "25" smd rect
		(at 5.715 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "f1b4ec06-20a5-48ba-a4f3-074f84612eb6")
	)
	(pad "26" smd rect
		(at 6.985 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "f8ecb135-132d-406a-b523-a0c88d8c2123")
	)
	(pad "27" smd rect
		(at 8.75 11.25)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "a6635e3c-354a-438c-8e2c-4c8f2a1c211d")
	)
	(pad "28" smd rect
		(at 8.75 9.98)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "74edfc41-8c80-45b4-b213-066032c78ed9")
	)
	(pad "29" smd rect
		(at 8.75 8.71)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "895d97d0-9a50-4d75-bf4b-a4a7c70b45b0")
	)
	(pad "30" smd rect
		(at 8.75 7.44)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "161b7d67-d419-477e-8a4b-7c8c6bf8a2b3")
	)
	(pad "31" smd rect
		(at 8.75 6.17)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "e06b9ceb-5ce7-45f9-b46c-0f6e2e7fd9d6")
	)
	(pad "32" smd rect
		(at 8.75 4.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "c791a750-bf1e-4aff-85a2-fac3cf2eaf5c")
	)
	(pad "33" smd rect
		(at 8.75 3.63)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "1aec4caf-1f42-44a3-bb80-0b4694ebc867")
	)
	(pad "34" smd rect
		(at 8.75 2.36)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "00222089-beb9-4b55-b65d-0a2f7caf07c9")
	)
	(pad "35" smd rect
		(at 8.75 1.09)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "8fc8bb18-6c06-45e3-8e0f-1ed00a0f581b")
	)
	(pad "36" smd rect
		(at 8.75 -0.18)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "52d3abb1-e88a-463c-a99a-1cf3c44510da")
	)
	(pad "37" smd rect
		(at 8.75 -1.45)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "165bfc24-7c9c-468d-bd20-405284db8ba9")
	)
	(pad "38" smd rect
		(at 8.75 -2.72)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "7cb9798a-e03c-4720-ba29-d066643741f4")
	)
	(pad "39" smd rect
		(at 8.75 -3.99)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "ee6f5813-5679-4a15-aa78-f6754033da8f")
	)
	(pad "40" smd rect
		(at 8.75 -5.26)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "2e7dd0bc-cfc1-4961-b471-3432a42c63b7")
	)
	(pad "41_1" smd rect
		(at -1.36 0.09)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "9a709bdc-b7fd-4163-a4b1-628148102795")
	)
	(pad "41_2" smd rect
		(at -2.86 0.09)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "eb9b4fb4-5756-4cd0-9e46-e20b88c9e09e")
	)
	(pad "41_3" smd rect
		(at 0.14 0.09)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "fc65e9ba-5eab-4ca6-a00a-0994bae5fe3c")
	)
	(pad "41_4" smd rect
		(at -2.86 1.59)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "7fd25ece-1de4-4112-ae48-b4fd84eabc46")
	)
	(pad "41_5" smd rect
		(at -1.36 1.59)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "76f0fa04-9d9b-4cff-b7f8-a9b308b1ba44")
	)
	(pad "41_6" smd rect
		(at 0.14 1.59)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "1f914697-2939-4343-b2cb-28c8c10a20ab")
	)
	(pad "41_7" smd rect
		(at -2.86 -1.41)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "cf0ee777-50e2-48fc-b28e-dd184abc9ac1")
	)
	(pad "41_8" smd rect
		(at -1.36 -1.41)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "126dc226-c33f-4639-9fce-2cd6e951c916")
	)
	(pad "41_9" smd rect
		(at 0.14 -1.41)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "4e93900d-7568-4f6d-91e9-1541586e654e")
	)
	(pad "41_10" thru_hole circle
		(at -1.36 -0.66)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "edb07115-ee8b-45a9-bcb0-468d374393d8")
	)
	(pad "41_11" thru_hole circle
		(at -2.86 -0.66)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "7b975aba-9439-492a-b5f8-65f3ccdbf3c6")
	)
	(pad "41_12" thru_hole circle
		(at 0.14 -0.66)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "cfdfb755-a53f-4ffe-8807-5a7ce9834468")
	)
	(pad "41_13" thru_hole circle
		(at -2.86 0.84)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "f543f2f2-2b20-4411-b1ca-b1d69ce95100")
	)
	(pad "41_14" thru_hole circle
		(at -1.36 0.84)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "cc7fa5ea-e2fb-43d8-8b32-d8cd3eec0128")
	)
	(pad "41_15" thru_hole circle
		(at 0.14 0.84)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "758d5d80-be6a-4e68-a56c-398e71fe1a2f")
	)
	(pad "41_16" thru_hole circle
		(at -2.11 -1.41)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "6c241e00-d195-49aa-88fc-9fa68a2ca02e")
	)
	(pad "41_17" thru_hole circle
		(at -0.61 -1.41)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "1daf1337-1a49-46e5-929c-02b4993aabe4")
	)
	(pad "41_18" thru_hole circle
		(at -2.11 0.09)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "52af196b-9660-4251-8369-fc569474b206")
	)
	(pad "41_19" thru_hole circle
		(at -0.61 0.09)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "573e30f5-a702-4e0c-8a85-9f02c722214d")
	)
	(pad "41_20" thru_hole circle
		(at -2.11 1.59)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "d5d96e7c-e833-4e1c-9e5d-8ff9493e27c8")
	)
	(pad "41_21" thru_hole circle
		(at -0.61 1.59)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "8558a9cd-4341-44f3-a235-e9fd7da5d376")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "1c7de16c-4437-4030-88a5-1fc0a336918e")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9 -12.75) (xy 9 -12.75) (xy 9 -6.75) (xy -9 -6.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu")
		(uuid "2ce1f9ae-a02d-4b98-a73d-029f6d25d0f7")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9 -12.75) (xy 9 -12.75) (xy 9 -6.75) (xy -9 -6.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(uuid "d2c30f4a-92b7-4031-89cc-5f671610c639")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9 -12.75) (xy 9 -12.75) (xy 9 -6.75) (xy -9 -6.75)
			)
		)
	)
	(model "/home/alex/Development/KiCAD-Libraries/ESP32-S3-WROOM-1-N8R2.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
