(footprint "BreadBoard-PowerAdapter-ESP32C3_v2"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Universal Power Adapter for Bread Board")
	(tags "Power Adapter Bread Board")
	(property "Reference" "BRD**"
		(at 0 -26.67 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "eb28b312-ccf5-4086-af96-2dc70b08668c")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "BreadBoard-PowerAdapter-ESP32C3_v2"
		(at 0 -22.86 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "888916df-9240-4a4a-89c5-e9dfd3a3a042")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4415cf11-8b03-453d-b470-bd69b1668e9e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4c604028-9ca3-49a9-b9fc-74314460e477")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Universal Power Adapter for Bread Board"
		(at 0 -21.59 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1b138117-f25c-4fd1-aa6a-34918751937f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -25.4 12.7)
		(end -25.4 -22.86)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "0e6acb05-95e5-4e13-839e-37d9995055dd")
	)
	(fp_line
		(start -24.13 13.97)
		(end 24.13 13.97)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "e7907f39-4c29-473a-bf4f-84a6cf15db5c")
	)
	(fp_line
		(start -22.86 -25.4)
		(end 22.86 -25.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "023b62d1-3240-4d02-ad95-5fc2644b4cc9")
	)
	(fp_line
		(start 27.94 -22.86)
		(end 27.94 12.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "bba8f151-42a4-4c0d-9f52-46a8221205cf")
	)
	(fp_arc
		(start -25.4 -22.86)
		(mid -24.656051 -24.656051)
		(end -22.86 -25.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "85febc22-b321-4619-ab24-efc5309a888e")
	)
	(fp_arc
		(start -24.13 13.97)
		(mid -25.028026 13.598026)
		(end -25.4 12.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "7bd351ec-26a8-403f-ba04-efdfe75dc255")
	)
	(fp_arc
		(start 25.4 -25.4)
		(mid 27.196051 -24.656051)
		(end 27.94 -22.86)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "fd37a84e-9b29-40d9-970b-53d7f7d4115d")
	)
	(fp_arc
		(start 27.94 12.7)
		(mid 27.568026 13.598026)
		(end 26.67 13.97)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "9669b8e2-70e8-409b-bb30-a00f3e46cd29")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -19.05 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "d9c00428-0a29-4dcf-80d0-e165eb51ae8a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(uuid "60d6bf8e-8a76-4aee-b400-e687b2bdf105")
		(pts
			(xy -24.130001 12.700001) (xy 26.67 12.7)
		)
		(height 12.619364)
		(gr_text "50.8000 mm"
			(at 1.27 24.169364 2.255739275e-06)
			(layer "Dwgs.User")
			(uuid "60d6bf8e-8a76-4aee-b400-e687b2bdf105")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(uuid "954e0d4d-05a1-44a0-ab24-6b9e96a929a7")
		(pts
			(xy 24.13 12.7) (xy 24.13 2.54)
		)
		(height 7.62)
		(gr_text "10.1600 mm"
			(at 30.6 7.62 90)
			(layer "Dwgs.User")
			(uuid "954e0d4d-05a1-44a0-ab24-6b9e96a929a7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(uuid "9c805382-387d-4767-82b3-661053141c02")
		(pts
			(xy -24.13 12.7) (xy -21.59 12.7)
		)
		(height 5.08)
		(gr_text "2.5400 mm"
			(at -22.86 16.63 0)
			(layer "Dwgs.User")
			(uuid "9c805382-387d-4767-82b3-661053141c02")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(uuid "bf43eb57-e208-4a86-b6f6-7c965f6983ee")
		(pts
			(xy 19.05 13.97) (xy 19.05 -25.4)
		)
		(height 38.1)
		(gr_text "39.3700 mm"
			(at 56 -5.715 90)
			(layer "Dwgs.User")
			(uuid "bf43eb57-e208-4a86-b6f6-7c965f6983ee")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(uuid "caad2e59-348c-41e5-b247-7467d9cdb62b")
		(pts
			(xy -25.4 12.7) (xy 27.94 12.7)
		)
		(height 20.32)
		(gr_text "53.3400 mm"
			(at 1.27 31.87 0)
			(layer "Dwgs.User")
			(uuid "caad2e59-348c-41e5-b247-7467d9cdb62b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(uuid "d58aa933-0683-4650-a144-611372583b0d")
		(pts
			(xy -22.86 -22.86) (xy 25.4 -22.86)
		)
		(height -8.89)
		(gr_text "48.2600 mm"
			(at 1.27 -32.9 0)
			(layer "Dwgs.User")
			(uuid "d58aa933-0683-4650-a144-611372583b0d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(pad "1" thru_hole circle
		(at -12.7 8.89)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f054de3d-cfb0-4259-bf30-fa878d7c0c95")
	)
	(pad "2" thru_hole circle
		(at -12.7 11.43)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0356299a-6d16-4607-b4db-eca387598c80")
	)
	(pad "3" thru_hole circle
		(at -10.16 8.89)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c9417135-0f98-4d03-a2d5-269935932f4e")
	)
	(pad "4" thru_hole circle
		(at -10.16 11.43)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6c35e06d-66da-4ce1-ba01-291040984ff5")
	)
	(pad "5" thru_hole circle
		(at -5.08 8.89)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ab1a136d-e4ae-4da4-a385-1e81584e4356")
	)
	(pad "6" thru_hole circle
		(at -5.08 11.43)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ee42b3c4-ea0d-4721-82db-093c64427502")
	)
	(pad "7" thru_hole circle
		(at -2.54 8.89)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "897a9567-45bd-41aa-92ca-7a510930bcc5")
	)
	(pad "8" thru_hole circle
		(at -2.54 11.43)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2733f22c-4e26-4ce2-bded-70dc5c23ff7e")
	)
	(pad "9" thru_hole circle
		(at 2.54 8.89)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c001dd4d-3589-4315-ba00-152fb4775355")
	)
	(pad "10" thru_hole circle
		(at 2.54 11.43)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ec2ebef9-0bbc-4c42-8601-f2316a60474e")
	)
	(pad "11" thru_hole circle
		(at 5.08 8.89)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "be6e010c-cd22-44e1-b0fa-505183c01a14")
	)
	(pad "12" thru_hole circle
		(at 5.08 11.43)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "86030f50-742f-4e8d-af03-89e6bb273de6")
	)
	(pad "13" thru_hole circle
		(at 10.16 8.89)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a4e91997-ae44-4a5f-968f-7ffc49b2485a")
	)
	(pad "14" thru_hole circle
		(at 10.16 11.43)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c01568b5-9db6-49c4-b97b-ba17da6b6134")
	)
	(pad "15" thru_hole circle
		(at 12.7 8.89)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "860e3ed8-a3d6-49a5-ac23-4d8b9e604762")
	)
	(pad "16" thru_hole circle
		(at 12.7 11.43)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7796d7d1-49c5-4571-b454-8eb706f20b05")
	)
	(pad "G1" thru_hole circle
		(at -21.59 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "537627d7-3e02-46b2-9e21-b3338d271c30")
	)
	(pad "G1" thru_hole circle
		(at -21.59 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "20a48552-fce3-40de-9514-7c5d4cac591b")
	)
	(pad "G2" thru_hole circle
		(at 26.67 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c155bf40-e9b8-4596-aefd-bb9b3c6afa14")
	)
	(pad "G2" thru_hole circle
		(at 26.67 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "72fc9726-3025-4d46-a43a-0c2889e34d93")
	)
	(pad "GND" thru_hole circle
		(at -22.86 -22.86)
		(size 5 5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ffc6e70c-23eb-4f6a-a87b-3a1743e277d6")
	)
	(pad "GND" thru_hole circle
		(at 25.4 -22.86)
		(size 5 5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f6a4cd44-802e-4d9b-b5ff-5310503cbc3b")
	)
	(pad "V1" thru_hole circle
		(at -24.13 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "08f81879-3e87-4fab-ac3e-55077bf0ae5f")
	)
	(pad "V1" thru_hole circle
		(at -24.13 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "30102978-7b4c-43a5-aa33-617ba8eb1a3f")
	)
	(pad "V2" thru_hole circle
		(at 24.13 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b5fe58a7-f301-4174-b9d3-7b9255d0c4b5")
	)
	(pad "V2" thru_hole circle
		(at 24.13 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "20a9449a-19a3-47e1-a0a7-1f2ad5559aac")
	)
)
