(footprint "RP2040-Zero"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "RP2040W Pico Zero")
	(tags "RP2040W Pico Zero")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "119935da-4c55-4506-8926-a2976de3cf50")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "RP2040-Zero"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "ea4c00b4-299a-4561-a6c1-7d89c0327a3a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "82b9af0c-69ed-4ab1-a14e-53c451565dde")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a2ed462d-b18c-46fb-8fb7-43e4730a5b82")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "RP2040W Pico Zero"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "418951af-7250-42fd-9736-2743baca03ce")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "409abbbf-e2fa-4f31-9eaa-76b9824f27b5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at -7.62 -22.86 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "06ac80ec-6eee-4907-98c0-9186c2628ba3")
	)
	(pad "2" thru_hole oval
		(at -7.62 -20.32 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e82bde82-581b-4ba7-945b-d231448a8acd")
	)
	(pad "3" thru_hole oval
		(at -7.62 -17.78 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ac907607-57a6-453c-940b-6d8364b97894")
	)
	(pad "4" thru_hole oval
		(at -7.62 -15.24 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8470707d-95b1-477f-8198-15c60869d7e8")
	)
	(pad "5" thru_hole oval
		(at -7.62 -12.7 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "272d45c6-afc3-4030-b3ce-6186c73a9223")
	)
	(pad "6" thru_hole oval
		(at -7.62 -10.16 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c1dcf4c3-e96b-42c9-9f5c-0dbb056f635a")
	)
	(pad "7" thru_hole oval
		(at -7.62 -7.62 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ad4c458a-8e0c-4076-9e82-8c8881ee28da")
	)
	(pad "8" thru_hole oval
		(at -7.62 -5.08 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "da1de3e2-28de-4fd2-ba7f-7096b8d0c227")
	)
	(pad "9" thru_hole oval
		(at -7.62 -2.54 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8bdeca76-e387-4efb-a59f-d83122972d48")
	)
	(pad "10" thru_hole oval
		(at -5.08 -2.54 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7709a60a-fa1a-4221-8039-0496b800876b")
	)
	(pad "11" thru_hole oval
		(at -2.54 -2.54 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6218e298-006f-4148-a6ab-316955371047")
	)
	(pad "12" thru_hole oval
		(at 0 -2.54 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1c14b3c4-6583-4708-b978-76bd322c81fc")
	)
	(pad "13" thru_hole oval
		(at 2.54 -2.54 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ac35088c-a238-40fd-b710-0c348aea22ea")
	)
	(pad "14" thru_hole oval
		(at 5.08 -2.54 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1b056c5a-b688-4bfe-a773-0fe6bd0f0472")
	)
	(pad "15" thru_hole oval
		(at 7.62 -2.54 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a86cff29-881b-4675-90a9-3d5f54aa4612")
	)
	(pad "16" thru_hole oval
		(at 7.62 -5.08 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "80c6f987-858f-4d1e-8f46-17251d953a77")
	)
	(pad "17" thru_hole oval
		(at 7.62 -7.62 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f18073d4-08a9-458c-896c-43a0ea2aa0f4")
	)
	(pad "18" thru_hole oval
		(at 7.62 -10.16 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "eafec1f4-ead6-40cf-9f53-5793cdaaa4ee")
	)
	(pad "19" thru_hole oval
		(at 7.62 -12.7 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7cc141df-d469-4985-af19-42f4e16b08fb")
	)
	(pad "20" thru_hole oval
		(at 7.62 -15.24 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9922587d-733d-462a-a34e-2a50082ef8d9")
	)
	(pad "21" thru_hole oval
		(at 7.62 -17.78 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "82c1cd2d-2f73-4616-ab07-ec065cb27441")
	)
	(pad "22" thru_hole oval
		(at 7.62 -20.32 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "92fcd8b8-d739-41fd-a3b5-fbea177d344e")
	)
	(pad "23" thru_hole oval
		(at 7.62 -22.86 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d75de787-f618-4355-bc3a-017c8c82be0e")
	)
)