(footprint "PinSocket_1x01_P2.54"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5e1403aa-0d62-459b-897f-8756eca026e5")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "PinSocket_1x01_P2.54"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "f2a9e1eb-308f-4035-bb26-aea054e2d6d5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5433eafd-fdba-4f21-8dbd-d3e3c908cb66")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "89bcbbe6-2da0-4ade-b337-b071f7d8fe78")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "89600bac-db47-4ed3-a7c1-8ef89229b0ce")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_circle
		(center 0 -2.54)
		(end 0 -3.81)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "50c6d507-5e24-4c47-a1de-a553fed1d3d6")
	)
	(fp_circle
		(center 0 -2.54)
		(end 0 -3.81)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "4d34a7d5-927d-4dd3-adde-967968231c6b")
	)
	(fp_line
		(start -0.06 -5.08)
		(end -0.06 -5.08)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e0c637cc-e96d-4403-ac15-84c514a7628e")
	)
	(fp_circle
		(center 0 -2.54)
		(end 0 -3.81)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "2a364f4d-c5b8-4e78-bd19-0ff35b44235d")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "1fafa1bc-1e59-4f3f-bd93-4879d3c80f32")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole oval
		(at 0 -2.57)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "856af50b-1830-4709-9f6b-48298035b569")
	)
)