(footprint "ESP32-C3-WROOM-02-Socket"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -9.035 -14.585 0)
		(layer "F.SilkS")
		(uuid "c1ef7f4f-d8a5-44f4-ad1d-4b2aec7eccf5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "ESP32-C3-WROOM-02-Socket"
		(at 0 20.32 0)
		(layer "F.Fab")
		(uuid "b181fa74-d9b4-4804-9bc1-b081e6bde4bb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at -2.46 -3.5 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "15536f93-f33c-4864-9d98-6e178b43b039")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at -2.46 -3.5 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7dfa6719-3fd2-4897-bc0d-ec5e75a775dd")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at -2.46 -3.5 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "9a131e6a-a466-4751-94ad-e5721b8264e5")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -11.46 -13.5)
		(end -11.46 -7.17)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0076f9b1-81b5-4285-abb4-62faf899b121")
	)
	(fp_line
		(start -11.46 6.5)
		(end -11.46 6.37)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "193a1fe4-1544-4f0a-a331-baad59e749fc")
	)
	(fp_line
		(start -11.46 6.5)
		(end 6.54 6.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e3d811e3-865c-4318-9fe1-1cba1633accd")
	)
	(fp_line
		(start 6.54 -13.5)
		(end -11.46 -13.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2f7ccea0-b14d-4f41-9967-771d65b5ea14")
	)
	(fp_line
		(start 6.54 -7.17)
		(end 6.54 -13.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "34a1d457-851b-4c77-b352-0988e5fbe50d")
	)
	(fp_line
		(start 6.54 6.5)
		(end 6.54 6.37)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "999f0b2b-d2bd-44aa-8d78-3240b5b1c47b")
	)
	(fp_line
		(start -17.78 15.24)
		(end -17.78 -5.08)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "dc0a399e-86b7-4726-a038-1e7730e7ae22")
	)
	(fp_line
		(start -15.24 -7.62)
		(end 10.16 -7.62)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "b1751c00-b900-4b60-91a0-bce747457d36")
	)
	(fp_line
		(start 10.16 17.78)
		(end -15.24 17.78)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "2a50c0b5-62e8-4153-a44e-58b5bab18ebe")
	)
	(fp_line
		(start 12.7 -5.08)
		(end 12.7 15.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "9d82ace1-7e1d-408e-a12b-aeebf47444b8")
	)
	(fp_arc
		(start -17.78 -5.08)
		(mid -17.036051 -6.876051)
		(end -15.24 -7.62)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "65a3d21f-c77e-40a3-b422-39e8b720edd5")
	)
	(fp_arc
		(start -15.24 17.78)
		(mid -17.036051 17.036051)
		(end -17.78 15.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "9840c1a7-2040-4d6e-854d-cb28239d748c")
	)
	(fp_arc
		(start 10.16 -7.62)
		(mid 11.956051 -6.876051)
		(end 12.7 -5.08)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "28231675-c752-460a-91ab-d51cf7dbf7dd")
	)
	(fp_arc
		(start 12.7 15.24)
		(mid 11.956051 17.036051)
		(end 10.16 17.78)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "1eaa7d5e-f35f-40bc-b477-7c8cf2f081e6")
	)
	(fp_line
		(start -12.21 -13.75)
		(end -12.21 6.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "172387b9-ba7a-4395-a875-36d8319536fa")
	)
	(fp_line
		(start -12.21 6.75)
		(end 7.29 6.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "07a472d3-b3b4-48a8-92c5-11b84169a55b")
	)
	(fp_line
		(start 7.29 -13.75)
		(end -12.21 -13.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2af17463-a6d8-4a6a-85bf-7a4abc35fe63")
	)
	(fp_line
		(start 7.29 6.75)
		(end 7.29 -13.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4c08169c-2bb8-4f43-8692-d32e478139b3")
	)
	(fp_line
		(start -11.46 -13.5)
		(end -11.46 -7.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "81588b9a-c83a-4bc7-ba7a-167b90fc3fdd")
	)
	(fp_line
		(start -11.46 -7.5)
		(end -11.46 6.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "67974f64-51a9-4e67-9a68-00e668e6c344")
	)
	(fp_line
		(start -11.46 6.5)
		(end 6.54 6.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5c37b9a1-b972-4c2b-a47c-76444bfcece7")
	)
	(fp_line
		(start 6.54 -13.5)
		(end -11.46 -13.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e78db179-c8bb-4496-8101-cb63044d88f9")
	)
	(fp_line
		(start 6.54 -7.5)
		(end -11.46 -7.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "41282e0d-9a18-4120-b9bd-655e8effafd8")
	)
	(fp_line
		(start 6.54 -7.5)
		(end 6.54 -13.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "91151eb1-8a2c-498f-bb58-b95a6358faa4")
	)
	(fp_line
		(start 6.54 6.5)
		(end 6.54 -7.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "22f16326-4c43-4f12-97bd-c64200effc3c")
	)
	(fp_circle
		(center -12.96 -6.4)
		(end -12.86 -6.4)
		(stroke
			(width 0.2)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "cc470171-7a85-46f0-942b-31d5aac30266")
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(uuid "36c075c2-27a0-4fb3-bed3-b03d913725de")
		(pts
			(xy 10.16 17.78) (xy 10.16 -7.62)
		)
		(height 15.24)
		(gr_text "25.4000 mm"
			(at 24.25 5.08 90)
			(layer "Cmts.User")
			(uuid "36c075c2-27a0-4fb3-bed3-b03d913725de")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(uuid "5cda490b-8368-4605-99a9-6bf898d6235b")
		(pts
			(xy -15.24 -5.08) (xy 10.16 -5.08)
		)
		(height -20.32)
		(gr_text "25.4000 mm"
			(at -2.54 -26.55 0)
			(layer "Cmts.User")
			(uuid "5cda490b-8368-4605-99a9-6bf898d6235b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(uuid "e2f57b15-561b-4cc4-a3e4-2a6e23c062fa")
		(pts
			(xy -17.78 15.24) (xy 12.7 15.24)
		)
		(height 12.7)
		(gr_text "30.4800 mm"
			(at -2.54 26.79 0)
			(layer "Cmts.User")
			(uuid "e2f57b15-561b-4cc4-a3e4-2a6e23c062fa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(pad "1" thru_hole rect
		(at -15.24 -5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1fc9f2e5-39c7-426e-b123-548378da993a")
	)
	(pad "1" smd rect
		(at -11.21 -6.4)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "4f2cf8cd-63a0-4c4d-a2fc-30401d4d579d")
	)
	(pad "2" thru_hole circle
		(at -15.24 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6774307e-1ae8-4563-a337-105bbc7e0497")
	)
	(pad "2" smd rect
		(at -11.21 -4.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "2d7bde91-885b-4e75-96aa-3a220aea7933")
	)
	(pad "3" thru_hole circle
		(at -15.24 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5d64747d-a852-42e6-b321-385dd43d0959")
	)
	(pad "3" smd rect
		(at -11.21 -3.4)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "f71a33f4-b981-4849-a326-fe0eb98aa681")
	)
	(pad "4" thru_hole circle
		(at -15.24 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "51d4b505-3fa6-47e7-aab5-47bf622cd946")
	)
	(pad "4" smd rect
		(at -11.21 -1.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "1b987018-93b0-4de0-8271-a4673148f422")
	)
	(pad "5" thru_hole circle
		(at -15.24 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4da34b95-ba12-41a8-b201-9026c516407c")
	)
	(pad "5" smd rect
		(at -11.21 -0.4)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "0a1b99dc-6f53-4dae-93f8-c1c147265d2f")
	)
	(pad "6" thru_hole circle
		(at -15.24 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5a056539-f712-4018-8e26-7fb3d287f69c")
	)
	(pad "6" smd rect
		(at -11.21 1.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "d9ba1da5-7148-4d31-bf5c-683c0bd8595a")
	)
	(pad "7" thru_hole circle
		(at -15.24 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cd777b65-609a-464f-a49e-4890fd059058")
	)
	(pad "7" smd rect
		(at -11.21 2.6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "3cf28dcf-d765-4dbe-8bf3-7bca177e725b")
	)
	(pad "8" thru_hole circle
		(at -15.24 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4fee6c49-0bdd-44fb-80ce-58a1f7b9d8e6")
	)
	(pad "8" smd rect
		(at -11.21 4.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "df872d06-3e39-4375-bc22-ef3bb3d1b1b6")
	)
	(pad "9" thru_hole roundrect
		(at -15.24 15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0)
		(chamfer_ratio 0.3)
		(chamfer top_left bottom_right)
		(uuid "f6c3d963-487a-4e0e-b670-4b0433679f97")
	)
	(pad "9" smd rect
		(at -11.21 5.6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "19431822-d50b-4e77-a015-065108c192f0")
	)
	(pad "10" smd rect
		(at 6.29 5.6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "9f193b3b-31f5-404c-bf3c-70e85a9dffde")
	)
	(pad "10" thru_hole circle
		(at 10.16 15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "edab94a2-f3bc-438a-b3c2-aca260e231bd")
	)
	(pad "11" smd rect
		(at 6.29 4.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "06bd1478-6895-4d06-9e7c-f38386483dc7")
	)
	(pad "11" thru_hole circle
		(at 10.16 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9b9d0460-b01f-4d5d-8f38-61e52eb2ca93")
	)
	(pad "12" smd rect
		(at 6.29 2.6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "b61ccca8-29cd-479e-93e0-82b8fc376640")
	)
	(pad "12" thru_hole circle
		(at 10.16 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f55b6177-83ad-45d4-8abc-316506e463ab")
	)
	(pad "13" smd rect
		(at 6.29 1.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "5e26cebb-1376-4f2d-85a0-663e3d89c305")
	)
	(pad "13" thru_hole circle
		(at 10.16 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "af34ec01-ae4e-40fc-99f4-97654eb3e89b")
	)
	(pad "14" smd rect
		(at 6.29 -0.4)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "051e7207-9b08-4f18-bf50-d3eb8d8a0eaf")
	)
	(pad "14" thru_hole circle
		(at 10.16 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f9aae237-f5e9-47e8-9be4-7eb18ef51010")
	)
	(pad "15" smd rect
		(at 6.29 -1.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "6de2f8c7-78a2-4f9f-86bf-44bc3d928dbb")
	)
	(pad "15" thru_hole circle
		(at 10.16 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1b9e7da7-379d-4543-add7-65ed2a1b5475")
	)
	(pad "16" smd rect
		(at 6.29 -3.4)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "36396bbc-12de-4a0e-964d-54fb454c4e00")
	)
	(pad "16" thru_hole circle
		(at 10.16 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "899b639f-b0b5-499e-a3e6-5a76f0a3cd9d")
	)
	(pad "17" smd rect
		(at 6.29 -4.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "915268c9-6d26-4efe-9a23-a01ec54b2d33")
	)
	(pad "17" thru_hole circle
		(at 10.16 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f49b1057-0d1b-4c88-a911-6e285f4844ea")
	)
	(pad "18" smd rect
		(at 6.29 -6.4)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "ca71375e-d35c-4f9e-9aae-637df1a557c2")
	)
	(pad "18" thru_hole circle
		(at 10.16 -5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a192418f-dfe2-4b90-87fc-c77ddb8982c7")
	)
	(pad "19" smd rect
		(at -2.6 -1.3)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "385b5496-6d73-41a6-af62-a1475a34a52f")
	)
	(pad "20" smd rect
		(at -1.5 -1.3)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "8fafad51-c486-44eb-8e9f-1c70644eeaa3")
	)
	(pad "21" smd rect
		(at -0.4 -1.3)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "89f4dcce-d1b6-47ed-a960-49ee0ea49182")
	)
	(pad "22" smd rect
		(at -2.6 -0.2)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "cf5f9572-6ac2-4561-a9e9-38441368ff44")
	)
	(pad "23" smd rect
		(at -1.5 -0.2)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "dd536341-59e7-4ec1-b803-5207f361bdd3")
	)
	(pad "24" smd rect
		(at -0.4 -0.2)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "7f4a1e09-9261-40e2-9e68-a32b10a467e7")
	)
	(pad "25" smd rect
		(at -2.6 0.9)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "8733727d-1033-49d3-af6e-2f32f6d3a3d5")
	)
	(pad "26" smd rect
		(at -1.5 0.9)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "24de7862-16fc-4700-aa17-48387ff3c2e1")
	)
	(pad "27" smd rect
		(at -0.4 0.9)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "e08912de-8924-4b1b-9ef5-8acffb9f1eb7")
	)
	(pad "28" thru_hole circle
		(at -2.05 -1.3)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "e92f3fbd-680c-404a-9731-81d18b0d1160")
	)
	(pad "29" thru_hole circle
		(at -0.95 -1.3)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "76f7b757-fea9-4212-a976-bfb2e8e6ad7d")
	)
	(pad "30" thru_hole circle
		(at -2.6 -0.75)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "ff4649c9-87af-40f8-857c-ce33a08cebc9")
	)
	(pad "31" thru_hole circle
		(at -1.5 -0.75)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "78c7a6ee-6de2-4034-8333-107691cb871e")
	)
	(pad "32" thru_hole circle
		(at -0.4 -0.75)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "36c35b0c-23ef-47f7-b22f-13a0a2a03658")
	)
	(pad "33" thru_hole circle
		(at -2.05 -0.2)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "1db95e42-0600-4c5f-89fe-895929074861")
	)
	(pad "34" thru_hole circle
		(at -0.95 -0.2)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "93aa8f8f-dc4a-4913-a4ac-27ec72a30846")
	)
	(pad "35" thru_hole circle
		(at -2.6 0.35)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "629decbb-bf92-41dc-aeab-d7f59202750a")
	)
	(pad "36" thru_hole circle
		(at -1.5 0.35)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "1fa7fe60-609e-4366-926d-91f44ba27f58")
	)
	(pad "37" thru_hole circle
		(at -0.4 0.35)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "bc3acfb6-52b0-45ca-81b6-2d184b9afe85")
	)
	(pad "38" thru_hole circle
		(at -2.05 0.9)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "3f7d3459-139d-4fdb-8e48-0c7e980d52b5")
	)
	(pad "39" thru_hole circle
		(at -0.95 0.9)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "34f87634-3531-4b8b-8137-238797db8d16")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "862083ce-f31d-451b-b600-797268f6d971")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -11.46 -13.5) (xy 6.54 -13.5) (xy 6.54 -7.5) (xy -11.46 -7.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu")
		(uuid "23faee98-3437-4126-b9e6-da16c18b2d7e")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -11.46 -13.5) (xy 6.54 -13.5) (xy 6.54 -7.5) (xy -11.46 -7.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(uuid "a1808f18-e0f9-4b1a-a307-741746e8d492")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -11.46 -13.5) (xy 6.54 -13.5) (xy 6.54 -7.5) (xy -11.46 -7.5)
			)
		)
	)
	(model "C:/Users/alex/github/KiCAD-Libraries/ESP32-C3-WROOM-02-N4.step"
		(offset
			(xyz -2.5 3.51 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
