(footprint "Conn_Terminal_2_Large" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 8060404d-7584-4986-83fc-8fdc66016fdb)
  )
  (fp_text value "Conn_Terminal_2_Large" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ba0e9860-90bb-4e1f-9729-155a34948ea8)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 66068ab2-a7ec-4899-a895-f04295fcf364)
  )
  (fp_line (start -3 10) (end 4 10)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 58c96ccf-2e65-46f7-a580-fdc1fba04009))
  (fp_line (start 4 5) (end 4 15)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 803ba2df-c4b4-4afc-be73-af6a530fc545))
  (fp_rect (start -3 5) (end 5 15)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp 127b6667-ed23-4f0c-a983-55f4a5763015))
  (fp_line (start -3 5) (end 5 5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a3c13091-5090-4ed0-9092-dcc69345d08b))
  (fp_line (start -3 15) (end -3 5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1c1f1ed1-f239-4c8a-b60d-2133f212ec65))
  (fp_line (start 5 5) (end 5 15)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 308541fa-6ace-43e6-8ed7-47a47bc184bb))
  (fp_line (start 5 15) (end -3 15)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 912fabba-6618-46eb-b7a9-440bc8420c4b))
  (pad "1" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 7deaf4b0-9f9c-440a-bcb5-1900acd78b92))
  (pad "2" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 3d0dcfe7-db10-4e33-8630-f6a8dc26a2b8))
)
