(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "AST50147-xx" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -9.525 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AST50147-xx" (at 6.985 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:Astrocast_AST50147-00" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://docs.astrocast.com/dl/0532-DOC-M2M-ASTRO-Astronode_S-Datasheet.pdf" (at 2.54 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "RF module Astrocast radio Astronode " (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "L-band satellite communication Astronode S module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Astrocast*AST50147*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AST50147-xx_0_1"
      (rectangle (start -10.16 10.16) (end 10.16 -10.16)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "AST50147-xx_1_1"
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 5.08 0) (length 2.54)
        (name "TXD" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -12.7 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 2.54)
        (name "RXD" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -12.7 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "GND_RF" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -12.7 90) (length 2.54) hide
        (name "GND_RF" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 7.62 180) (length 2.54)
        (name "ANTN_RF" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -12.7 90) (length 2.54) hide
        (name "GND_RF" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -12.7 90) (length 2.54) hide
        (name "GND_RF" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 12.7 270) (length 2.54) hide
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 10.16 270) (length 2.54) hide
        (name "RSVD" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -5.08 10.16 270) (length 2.54) hide
        (name "RSVD" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 10.16 270) (length 2.54) hide
        (name "RSVD" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -12.7 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 0 0) (length 2.54) hide
        (name "N.C." (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -12.7 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 -10.16 90) (length 2.54) hide
        (name "N.C." (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -12.7 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 5.08 -10.16 90) (length 2.54) hide
        (name "N.C." (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -12.7 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 -10.16 90) (length 2.54) hide
        (name "N.C." (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -12.7 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 10.16 270) (length 2.54) hide
        (name "N.C." (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -12.7 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 -7.62 0) (length 2.54) hide
        (name "N.C." (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 -2.54 180) (length 2.54) hide
        (name "N.C." (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -12.7 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 10.16 270) (length 2.54) hide
        (name "RSVD" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 5.08 10.16 270) (length 2.54) hide
        (name "RSVD" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 2.54 180) (length 2.54)
        (name "EVENT_NOTIF" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -12.7 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 2.54)
        (name "ANTN_USE" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -12.7 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.54 0) (length 2.54)
        (name "WAKEUP" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 -12.7 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ATSAMR21G18-MR210UA_NoRFPads" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -11.43 29.21 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "ATSAMR21G18-MR210UA_NoRFPads" (at 1.27 29.21 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "RF_Module:Atmel_ATSAMR21G18-MR210UA_NoRFPads" (at 2.54 0 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/atmel-42475-atsamr21g18-mr210ua_datasheet.pdf" (at 0 -38.1 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Wireless Zigbee 802.15.4 ATSAMR21G18 AT45DB041E TECC508A" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "RF Module, ATSAMR21, Zigbee 802.15.4, external antenna, SMD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Atmel*ATSAMR21G18*MR210UA*NoRFPads*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ATSAMR21G18-MR210UA_NoRFPads_1_1"
      (rectangle (start -10.16 27.94) (end 10.16 -25.4)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin power_in line (at 0 -27.94 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -17.78 180) (length 2.54)
        (name "PA28" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 15.24 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -27.94 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 17.78 180) (length 2.54)
        (name "PA07" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 15.24 180) (length 2.54)
        (name "PA08" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 12.7 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 10.16 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 10.16 180) (length 2.54)
        (name "PA13" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 12.7 180) (length 2.54)
        (name "PA12" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -12.7 180) (length 2.54)
        (name "PA24" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -27.94 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -15.24 180) (length 2.54)
        (name "PA25" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 5.08 180) (length 2.54)
        (name "PA15" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 7.62 180) (length 2.54)
        (name "PA14" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 25.4 180) (length 2.54)
        (name "PA4" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 22.86 180) (length 2.54)
        (name "PA5" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 20.32 180) (length 2.54)
        (name "PA6" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 5.08 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -27.94 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 30.48 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -20.32 180) (length 2.54)
        (name "PA30" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -22.86 180) (length 2.54)
        (name "PA31" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 0 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 20.32 0) (length 2.54)
        (name "ATECC508_GPIO" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 -2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 -5.08 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -10.16 180) (length 2.54)
        (name "PA23" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -7.62 180) (length 2.54)
        (name "PA22" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 -7.62 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 -10.16 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 30.48 270) (length 2.54) hide
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 -12.7 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -27.94 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -27.94 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 25.4 0) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 0 180) (length 2.54)
        (name "PA17" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
        (name "PA18" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 2.54 180) (length 2.54)
        (name "PA16" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -5.08 180) (length 2.54)
        (name "PA19" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "AX-SIP-SFEU" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -13.97 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AX-SIP-SFEU" (at 8.89 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:OnSemi_SIP-38-6EP-9x7mm_P0.65mm_EP1.2x1.2mm" (at 2.54 -24.13 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/AX-SIP-SFEU-D.PDF" (at -24.13 -31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Sigfox SIP 868Mhz" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Ultra low power, Sigfox or custom, system in package transceiver, 868Mhz" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "OnSemi*SIP*6EP*9x7mm*P0.65mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AX-SIP-SFEU_0_1"
      (rectangle (start -15.24 22.86) (end 15.24 -22.86)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "AX-SIP-SFEU_1_1"
      (pin power_in line (at 0 -25.4 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -12.7 180) (length 2.54)
        (name "GPIO11/PC6" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -10.16 180) (length 2.54)
        (name "GPIO10/PC5" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -5.08 180) (length 2.54)
        (name "GPIO8/PC4" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -2.54 180) (length 2.54)
        (name "GPIO7/PC3" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 0 180) (length 2.54)
        (name "GPIO6/PC2" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 2.54 180) (length 2.54)
        (name "GPIO5/PC1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 5.08 180) (length 2.54)
        (name "GPIO4/PC0" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -17.78 -7.62 0) (length 2.54)
        (name "CPULED" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -17.78 -10.16 0) (length 2.54)
        (name "RADIOLED" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -7.62 180) (length 2.54)
        (name "GPIO9/PB3" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -17.78 15.24 0) (length 2.54)
        (name "UART_TX" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -17.78 12.7 0) (length 2.54)
        (name "UART_RX" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -17.78 0 0) (length 2.54)
        (name "RX_LED" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -17.78 -2.54 0) (length 2.54)
        (name "TX_LED" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -15.24 2.54 0) (length 2.54) hide
        (name "NC24" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -17.78 7.62 0) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 25.4 270) (length 2.54)
        (name "VDD_IO" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 15.24 180) (length 2.54)
        (name "GPIO0/PA0" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 12.7 180) (length 2.54)
        (name "GPIO1/PA1" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 17.78 20.32 180) (length 2.54)
        (name "ANT" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 10.16 180) (length 2.54)
        (name "GPIO2/PA2" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 5.08 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 7.62 180) (length 2.54)
        (name "GPIO3/PA5" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -15.24 180) (length 2.54)
        (name "GPIO12/PA6" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -17.78 180) (length 2.54)
        (name "GPIO13/PA7" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -20.32 180) (length 2.54)
        (name "GPIO14/PC7" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -5.08 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "AX-SIP-SFEU-API" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -13.97 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AX-SIP-SFEU-API" (at 10.16 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:OnSemi_SIP-38-6EP-9x7mm_P0.65mm_EP1.2x1.2mm" (at 2.54 -24.13 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/AX-SIP-SFEU-D.PDF" (at -24.13 -31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Sigfox SIP 868Mhz" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Ultra low power, Sigfox or custom, programmable system in package, 868Mhz" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "OnSemi*SIP*6EP*9x7mm*P0.65mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AX-SIP-SFEU-API_0_1"
      (rectangle (start -15.24 22.86) (end 15.24 -22.86)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "AX-SIP-SFEU-API_1_1"
      (pin power_in line (at 0 -25.4 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -12.7 180) (length 2.54)
        (name "GPIO11/PC6" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -10.16 180) (length 2.54)
        (name "GPIO10/PC5" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -5.08 180) (length 2.54)
        (name "GPIO8/PC4" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -2.54 180) (length 2.54)
        (name "GPIO7/PC3" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 0 180) (length 2.54)
        (name "GPIO6/PC2" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 2.54 180) (length 2.54)
        (name "GPIO5/PC1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 5.08 180) (length 2.54)
        (name "GPIO4/PC0" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -17.78 -7.62 0) (length 2.54)
        (name "CPULED/PB0" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -17.78 -10.16 0) (length 2.54)
        (name "RADIOLED/PB1" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -7.62 180) (length 2.54)
        (name "GPIO9/PB3" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -17.78 15.24 0) (length 2.54)
        (name "UART_TX/PB4" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -17.78 12.7 0) (length 2.54)
        (name "UART_RX/PB5" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 0 0) (length 2.54)
        (name "DBG_DATA/PB6" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -17.78 -2.54 0) (length 2.54)
        (name "DBG_CLK/PB7" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -17.78 2.54 0) (length 2.54)
        (name "DBG_EN" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -17.78 7.62 0) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 25.4 270) (length 2.54)
        (name "VDD_IO" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 15.24 180) (length 2.54)
        (name "GPIO0/PA0" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 12.7 180) (length 2.54)
        (name "GPIO1/PA1" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 17.78 20.32 180) (length 2.54)
        (name "ANT" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 10.16 180) (length 2.54)
        (name "GPIO2/PA2" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 2.54 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 5.08 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 7.62 180) (length 2.54)
        (name "GPIO3/PA5" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -15.24 180) (length 2.54)
        (name "GPIO12/PA6" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -17.78 180) (length 2.54)
        (name "GPIO13/PA7" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -20.32 180) (length 2.54)
        (name "GPIO14/PC7" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -7.62 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -5.08 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 22.86 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Ai-Thinker-Ra-01" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 17.78 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Ai-Thinker-Ra-01" (at 13.97 -15.24 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:Ai-Thinker-Ra-01-LoRa" (at 25.4 -10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://wiki.ai-thinker.com/_media/lora/docs/c047ps01a1_ra-01_product_specification_v1.1.pdf" (at 2.54 17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Ra-01 LoRa" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Ai-Thinker Ra-01 410-525 MHz LoRa Module, SPI interface, external antenna" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Ai?Thinker?Ra?01*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Ai-Thinker-Ra-01_0_1"
      (rectangle (start -7.62 12.7) (end 7.62 -12.7)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "Ai-Thinker-Ra-01_1_1"
      (pin passive line (at 10.16 10.16 180) (length 2.54)
        (name "ANT" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -5.08 180) (length 2.54)
        (name "DIO4" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -7.62 180) (length 2.54)
        (name "DIO5" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "SCK" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 2.54 0) (length 2.54)
        (name "MISO" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "MOSI" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "~{NSS}" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -15.24 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 15.24 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -7.62 0) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 5.08 180) (length 2.54)
        (name "DIO0" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 2.54 180) (length 2.54)
        (name "DIO1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 0 180) (length 2.54)
        (name "DIO2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -2.54 180) (length 2.54)
        (name "DIO3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Ai-Thinker-Ra-02" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 2.54 19.05 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Ai-Thinker-Ra-02" (at 13.97 -15.24 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:Ai-Thinker-Ra-01-LoRa" (at 25.4 -10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://wiki.ai-thinker.com/_media/lora/docs/c048ps01a1_ra-02_product_specification_v1.1.pdf" (at 2.54 19.05 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Ra-02 LoRa" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Ai-Thinker Ra-02 410-525 MHz LoRa Module, SPI interface, U.FL antenna connector" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Ai?Thinker?Ra?01*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Ai-Thinker-Ra-02_0_1"
      (rectangle (start -7.62 12.7) (end 7.62 -12.7)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "Ai-Thinker-Ra-02_1_1"
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -5.08 180) (length 2.54)
        (name "DIO4" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -7.62 180) (length 2.54)
        (name "DIO5" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "SCK" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 2.54 0) (length 2.54)
        (name "MISO" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "MOSI" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "~{NSS}" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -15.24 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 17.78 270) (length 5.08)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -7.62 0) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 5.08 180) (length 2.54)
        (name "DIO0" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 2.54 180) (length 2.54)
        (name "DIO1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 0 180) (length 2.54)
        (name "DIO2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -2.54 180) (length 2.54)
        (name "DIO3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "CMWX1ZZABZ-078" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -17.78 36.83 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "CMWX1ZZABZ-078" (at 16.51 36.83 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:CMWX1ZZABZ" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://wireless.murata.com/RFM/data/type_abz.pdf" (at 62.23 -38.1 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "iot lora sigfox" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LoRa/SigFox Module, STM32L082 MCU, Murata CMWX1ZZABZ" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "CMWX1ZZABZ*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "CMWX1ZZABZ-078_0_1"
      (rectangle (start -20.32 35.56) (end 20.32 -35.56)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "CMWX1ZZABZ-078_1_1"
      (pin bidirectional line (at -22.86 0 0) (length 2.54)
        (name "PA12/USB_DP" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -25.4 180) (length 2.54)
        (name "SX1276_DIO4" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -27.94 180) (length 2.54)
        (name "DBG_SX1276_DIO5" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -17.78 180) (length 2.54)
        (name "DBG_SX1276_DIO1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -15.24 180) (length 2.54)
        (name "DBG_SX1276_DIO0" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 0 180) (length 2.54)
        (name "PB15/SPI2_MOSI" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 2.54 180) (length 2.54)
        (name "PB14/SPI2_MISO" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 5.08 180) (length 2.54)
        (name "PB13/SPI2_SCK" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 7.62 180) (length 2.54)
        (name "PB12/SPI2_NSS" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 5.08 0) (length 2.54)
        (name "PA10/USART1_RX" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 7.62 0) (length 2.54)
        (name "PA9/USART1_TX" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 2.54 0) (length 2.54)
        (name "PA11/USB_DM" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 10.16 0) (length 2.54)
        (name "PA8/MCO" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 12.7 0) (length 2.54)
        (name "PA5/ADC5/DAC2" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 15.24 0) (length 2.54)
        (name "PA4/ADC4/DAC1" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 17.78 0) (length 2.54)
        (name "PA3/ADC3" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 20.32 0) (length 2.54)
        (name "PA2/ADC2" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 22.86 -33.02 180) (length 2.54)
        (name "ANT" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 22.86 -5.08 180) (length 2.54)
        (name "DBG_CRF1" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 22.86 -10.16 180) (length 2.54)
        (name "DBG_CRF3" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -38.1 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 22.86 -7.62 180) (length 2.54)
        (name "DGB_CRF2" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -22.86 -27.94 0) (length 2.54)
        (name "~{STSAFE_RST}" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 38.1 270) (length 2.54)
        (name "VREF+" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 22.86 0) (length 2.54)
        (name "PA0/WKUP1" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -10.16 0) (length 2.54)
        (name "~{MCU_RST}" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 12.7 180) (length 2.54)
        (name "PB8/I2C1_SCL" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 10.16 180) (length 2.54)
        (name "PB9/I2C1_SDA" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 22.86 180) (length 2.54)
        (name "PB2/LPTIM1_OUT" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 15.24 180) (length 2.54)
        (name "PB7/LPTIM1_IN2" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 17.78 180) (length 2.54)
        (name "PB6/LPTIM1_ETR" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 38.1 270) (length 2.54)
        (name "VDD_USB" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 20.32 180) (length 2.54)
        (name "PB5/LPTIM1_IN1" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -2.54 0) (length 2.54)
        (name "PA13/SWDIO" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -5.08 0) (length 2.54)
        (name "PA14/SWCLK" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -33.02 0) (length 2.54)
        (name "BOOT0" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -22.86 0) (length 2.54)
        (name "PH1/OSC_OUT" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -20.32 0) (length 2.54)
        (name "PH0/OSC_IN" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -22.86 -15.24 0) (length 2.54)
        (name "TCXO_OUT" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 38.1 270) (length 2.54)
        (name "VDD_TCXO" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 38.1 270) (length 2.54)
        (name "VDD_MCU" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 38.1 270) (length 2.54)
        (name "VDD_RF" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -20.32 180) (length 2.54)
        (name "DBG_SX1276_DIO2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -22.86 180) (length 2.54)
        (name "DBG_SX1276_DI03" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "CMWX1ZZABZ-091" (extends "CMWX1ZZABZ-078")
    (property "Reference" "U" (at -17.78 36.83 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "CMWX1ZZABZ-091" (at 16.51 36.83 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:CMWX1ZZABZ" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://wireless.murata.com/RFM/data/type_abz.pdf" (at 62.23 -38.1 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "iot lora sigfox" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LoRa/SigFox Module, STM32L072 MCU, Murata CMWX1ZZABZ" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "CMWX1ZZABZ*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "D52MxxM8" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -11.43 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "D52MxxM8" (at 7.62 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:Garmin_M8-35_9.8x14.0mm_Layout6x6_P1.5mm" (at 0 -29.21 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.thisisant.com/assets/resources/D00001687_D52_Module_Datasheet.v.2.3_(Garmin).pdf" (at 2.54 -21.59 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "RF Radio ANT Bluetooth BLE D52 nRF52 Garmin Canada Dynastream Nordic" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "D52M Module, nRF52832 SoC, ARM Cortex-M4F, 64kB RAM, 512kB Flash, 1.7-3.6V, M8-35" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Garmin*M8*9.8x14.0mm*Layout6x6*P1.5mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "D52MxxM8_0_1"
      (rectangle (start -12.7 22.86) (end 12.7 -22.86)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "D52MxxM8_1_1"
      (pin power_in line (at 0 -25.4 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "A2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "A3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "A4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "A5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -25.4 90) (length 2.54) hide
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "A6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 17.78 0) (length 2.54)
        (name "SWDIO" (effects (font (size 1.27 1.27))))
        (number "B1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 5.08 0) (length 2.54)
        (name "P012" (effects (font (size 1.27 1.27))))
        (number "B2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -2.54 0) (length 2.54)
        (name "P015" (effects (font (size 1.27 1.27))))
        (number "B3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -10.16 0) (length 2.54)
        (name "P020" (effects (font (size 1.27 1.27))))
        (number "B4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 25.4 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "B5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 25.4 270) (length 2.54) hide
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "B6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 15.24 0) (length 2.54)
        (name "SWDCLK" (effects (font (size 1.27 1.27))))
        (number "C1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
        (name "NFC1/P009" (effects (font (size 1.27 1.27))))
        (number "C2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
        (name "NFC2/P010" (effects (font (size 1.27 1.27))))
        (number "C3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -5.08 0) (length 2.54)
        (name "P016" (effects (font (size 1.27 1.27))))
        (number "C4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 25.4 270) (length 2.54) hide
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "C5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 25.4 270) (length 2.54) hide
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "C6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
        (name "P008" (effects (font (size 1.27 1.27))))
        (number "D1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 0 0) (length 2.54)
        (name "P014" (effects (font (size 1.27 1.27))))
        (number "D2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 2.54 0) (length 2.54)
        (name "P013" (effects (font (size 1.27 1.27))))
        (number "D3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -12.7 0) (length 2.54)
        (name "P022" (effects (font (size 1.27 1.27))))
        (number "D4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -7.62 0) (length 2.54)
        (name "P018" (effects (font (size 1.27 1.27))))
        (number "D5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -15.24 0) (length 2.54)
        (name "P024" (effects (font (size 1.27 1.27))))
        (number "D6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
        (name "P006" (effects (font (size 1.27 1.27))))
        (number "E1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
        (name "AIN3/P005" (effects (font (size 1.27 1.27))))
        (number "E2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
        (name "AIN1/P003" (effects (font (size 1.27 1.27))))
        (number "E3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
        (name "AIN2/P004" (effects (font (size 1.27 1.27))))
        (number "E4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 0 180) (length 2.54)
        (name "AIN0/P002" (effects (font (size 1.27 1.27))))
        (number "E5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 12.7 0) (length 2.54)
        (name "P021/RESET" (effects (font (size 1.27 1.27))))
        (number "E6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -17.78 0) (length 2.54)
        (name "P025" (effects (font (size 1.27 1.27))))
        (number "F1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -17.78 180) (length 2.54)
        (name "AIN7/P031" (effects (font (size 1.27 1.27))))
        (number "F2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
        (name "AIN6/P030" (effects (font (size 1.27 1.27))))
        (number "F3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
        (name "AIN5/P029" (effects (font (size 1.27 1.27))))
        (number "F4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
        (name "AIN4/P028" (effects (font (size 1.27 1.27))))
        (number "F5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 7.62 0) (length 2.54)
        (name "P011" (effects (font (size 1.27 1.27))))
        (number "F6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "DWM1000" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "DWM" (at 7.62 25.4 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "DWM1000" (at 1.27 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:DWM1000" (at 17.78 -25.4 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.decawave.com/sites/default/files/resources/dwm1000-datasheet-v1.3.pdf" (at 60.96 -27.94 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "DWM1000,Decawave,RF,ranging,UWB" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Ultra wide band RF module With ranging location capabilities" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "*DWM1000*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "DWM1000_0_1"
      (rectangle (start 17.78 22.86) (end -17.78 -22.86)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "DWM1000_1_1"
      (pin output line (at -22.86 5.08 0) (length 5.08)
        (name "EXTON" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -12.7 180) (length 5.08)
        (name "GPIO5/EXTTXE/SPIPOL" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -10.16 180) (length 5.08)
        (name "GPIO4/EXTPA" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -7.62 180) (length 5.08)
        (name "GPIO3/TXLED" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -5.08 180) (length 5.08)
        (name "GPIO2/RXLED" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -2.54 180) (length 5.08)
        (name "GPIO1/SFDLED" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 0 180) (length 5.08)
        (name "GPIO0/RXOKLED" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -27.94 90) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 10.16 180) (length 5.08)
        (name "SPICSn" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 12.7 180) (length 5.08)
        (name "SPIMOSI" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 15.24 180) (length 5.08)
        (name "SPIMISO" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 2.54 0) (length 5.08)
        (name "WAKEUP" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 17.78 180) (length 5.08)
        (name "SPICLK" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -27.94 90) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 20.32 180) (length 5.08)
        (name "IRQ/GPIO8" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -27.94 90) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -27.94 90) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 0 0) (length 5.08)
        (name "RSTn" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -2.54 0) (length 5.08)
        (name "GPIO7" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 27.94 270) (length 5.08)
        (name "VDDAON" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 27.94 270) (length 5.08)
        (name "VDD3V3" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 27.94 270) (length 5.08)
        (name "VDD3V3" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -27.94 90) (length 5.08)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -15.24 180) (length 5.08)
        (name "GPIO6/EXTRXE/SPIHA" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "DWM1001" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -12.7 27.94 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "DWM1001" (at -12.7 25.4 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "RF_Module:DecaWave_DWM1001" (at 17.78 -24.13 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.decawave.com/sites/default/files/dwm1001_datasheet.pdf" (at 22.86 -20.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "DWM1000  DecaWave RF ranging UWB" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" " Ultra wide band RF module With ranging location capabilities, I2C, UART, SPI, +2.8V to +3.6V VCC" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "*DWM1001*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "DWM1001_0_1"
      (rectangle (start 15.24 22.86) (end -15.24 -22.86)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "DWM1001_1_1"
      (pin power_in line (at 0 -27.94 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -17.78 180) (length 5.08)
        (name "GPIO_30" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -27.94 90) (length 5.08) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 27.94 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -15.24 180) (length 5.08)
        (name "GPIO_27" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 12.7 0) (length 5.08)
        (name "I2C_SDA" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -20.32 10.16 0) (length 5.08)
        (name "I2C_SCL" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -12.7 180) (length 5.08)
        (name "GPIO_23" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -2.54 180) (length 5.08)
        (name "GPIO_13" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 -2.54 0) (length 5.08)
        (name "UART_RX" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 20.32 20.32 180) (length 5.08)
        (name "READY" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 5.08 0) (length 5.08)
        (name "SWD_CLK" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -20.32 -5.08 0) (length 5.08)
        (name "UART_TX" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 15.24 180) (length 5.08)
        (name "GPIO_1" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 17.78 180) (length 5.08)
        (name "GPIO_0" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -7.62 180) (length 5.08)
        (name "GPIO_15" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -27.94 90) (length 5.08) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 7.62 180) (length 5.08)
        (name "GPIO_8" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -20.32 -10.16 0) (length 5.08)
        (name "SPIS_MISO" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -20.32 -12.7 0) (length 5.08)
        (name "SPIS_MOSI" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 -15.24 0) (length 5.08)
        (name "SPIS_CLK" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 -17.78 0) (length 5.08)
        (name "~{SPIS_CS}" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 2.54 0) (length 5.08)
        (name "SWD_DIO" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 10.16 180) (length 5.08)
        (name "GPIO_3" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 12.7 180) (length 5.08)
        (name "GPIO_2" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 20.32 0) (length 5.08)
        (name "BT_WAKE_UP" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 17.78 0) (length 5.08)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -27.94 90) (length 5.08) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 2.54 180) (length 5.08)
        (name "GPIO_10" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 5.08 180) (length 5.08)
        (name "GPIO_9" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 0 180) (length 5.08)
        (name "GPIO_12" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -5.08 180) (length 5.08)
        (name "GPIO_14" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -10.16 180) (length 5.08)
        (name "GPIO_22" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -20.32 180) (length 5.08)
        (name "GPIO_31" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "E18-MS1-PCB" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -2.54 21.59 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "E18-MS1-PCB" (at -2.54 19.05 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "RF_Module:E18-MS1-PCB" (at -5.08 5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.cdebyte.com/en/downpdf.aspx?id=122" (at -5.08 5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Zigbee, RF, 802.15.4" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Zigbee RF Module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "E18-MS1-PCB*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "E18-MS1-PCB_0_1"
      (rectangle (start -10.16 17.78) (end 10.16 -15.24)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "E18-MS1-PCB_1_1"
      (pin power_in line (at 0 -17.78 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 2.54 180) (length 2.54)
        (name "P1.5" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 5.08 180) (length 2.54)
        (name "P1.4" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 7.62 180) (length 2.54)
        (name "P1.3" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 10.16 180) (length 2.54)
        (name "P1.2" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 12.7 180) (length 2.54)
        (name "P1.1" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 15.24 180) (length 2.54)
        (name "P1.0" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -7.62 0) (length 2.54)
        (name "P0.7" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -5.08 0) (length 2.54)
        (name "P0.6" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -2.54 0) (length 2.54)
        (name "P0.5" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 0 0) (length 2.54)
        (name "P0.4" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 20.32 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 2.54 0) (length 2.54)
        (name "P0.3" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 5.08 0) (length 2.54)
        (name "P0.2" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 7.62 0) (length 2.54)
        (name "P0.1" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 10.16 0) (length 2.54)
        (name "P0.0" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 15.24 0) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -12.7 180) (length 2.54)
        (name "P2.2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -10.16 180) (length 2.54)
        (name "P2.1" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -7.62 180) (length 2.54)
        (name "P2.0" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
        (name "P1.7" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 0 180) (length 2.54)
        (name "P1.6" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 -10.16 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 -12.7 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "E73-2G4M04S-52832" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "E73-2G4M04S-52832" (at 0 -1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:E73-2G4M04S" (at 0 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.cdebyte.com/en/downpdf.aspx?id=243" (at 0 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "BLE5, BLE, nRF52832" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "nRF52832 BLE5 Module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "E73*2G4M04S*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "E73-2G4M04S-52832_0_1"
      (rectangle (start 20.32 38.1) (end -20.32 -38.1)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "E73-2G4M04S-52832_1_1"
      (pin power_in line (at 0 -40.64 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "0" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -40.64 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -33.02 180) (length 2.54)
        (name "AIN6/P0.30" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -35.56 180) (length 2.54)
        (name "AIN7/P0.31" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 40.64 270) (length 2.54)
        (name "DEC4" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 5.08 40.64 270) (length 2.54)
        (name "DCC" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 40.64 270) (length 2.54)
        (name "DEC1" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -40.64 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 40.64 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 35.56 180) (length 2.54)
        (name "AIN0/P0.02" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 33.02 180) (length 2.54)
        (name "AIN1/P0.03" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 30.48 180) (length 2.54)
        (name "AIN2/P0.04" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -40.64 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 27.94 180) (length 2.54)
        (name "AIN3/P0.05" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 25.4 180) (length 2.54)
        (name "P0.06" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 22.86 180) (length 2.54)
        (name "P0.07" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 20.32 180) (length 2.54)
        (name "P0.08" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 17.78 180) (length 2.54)
        (name "NFC1/P0.09" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 15.24 180) (length 2.54)
        (name "NFC2/P0.10" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 12.7 180) (length 2.54)
        (name "P0.11" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 10.16 180) (length 2.54)
        (name "P0.12" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 7.62 180) (length 2.54)
        (name "P0.13" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 5.08 180) (length 2.54)
        (name "P0.14" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -10.16 40.64 270) (length 2.54)
        (name "DEC2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 2.54 180) (length 2.54)
        (name "P0.15" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 0 180) (length 2.54)
        (name "P0.16" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -2.54 180) (length 2.54)
        (name "P0.17" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -5.08 180) (length 2.54)
        (name "SWO/P0.18" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -7.62 180) (length 2.54)
        (name "P0.19" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -10.16 180) (length 2.54)
        (name "P0.20" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -12.7 0) (length 2.54)
        (name "P0.21/~{RESET}" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -15.24 0) (length 2.54)
        (name "SWDCLK" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -17.78 0) (length 2.54)
        (name "SWDIO" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -12.7 180) (length 2.54)
        (name "P0.22" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -7.62 40.64 270) (length 2.54)
        (name "DEC3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -15.24 180) (length 2.54)
        (name "P0.23" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -17.78 180) (length 2.54)
        (name "P0.24" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -40.64 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -40.64 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -20.32 180) (length 2.54)
        (name "P0.25" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -22.86 180) (length 2.54)
        (name "P0.26" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -25.4 180) (length 2.54)
        (name "P0.27" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -27.94 180) (length 2.54)
        (name "AIN4/P0.28" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -30.48 180) (length 2.54)
        (name "AIN5/P0.29" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "E73-2G4M04S-52810" (extends "E73-2G4M04S-52832")
    (property "Reference" "U" (at 0 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "E73-2G4M04S-52810" (at 0 -1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:E73-2G4M04S" (at 0 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.cdebyte.com/en/downpdf.aspx?id=243" (at 0 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "BLE5, BLE, nRF52810" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "nRF52810 BLE5 Module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "E73*2G4M04S*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "ESP-07" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -12.7 19.05 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "ESP-07" (at 12.7 19.05 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "RF_Module:ESP-07" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://wiki.ai-thinker.com/_media/esp8266/esp8266_series_modules_user_manual_v1.1.pdf" (at -8.89 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "802.11 Wi-Fi" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "802.11 b/g/n Wi-Fi Module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "ESP?07*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP-07_0_1"
      (rectangle (start -12.7 17.78) (end 12.7 -15.24)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "ESP-07_1_1"
      (pin input line (at -15.24 15.24 0) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
        (name "GPIO15" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
        (name "GPIO2" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
        (name "GPIO0" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
        (name "GPIO4" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
        (name "GPIO5" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
        (name "GPIO3/RXD" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
        (name "GPIO1/TXD" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 5.08 0) (length 2.54)
        (name "ADC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 10.16 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
        (name "GPIO16" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
        (name "GPIO14" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 0 180) (length 2.54)
        (name "GPIO12" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
        (name "GPIO13" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 20.32 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -17.78 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP-12E" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -12.7 19.05 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "ESP-12E" (at 12.7 19.05 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "RF_Module:ESP-12E" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://wiki.ai-thinker.com/_media/esp8266/esp8266_series_modules_user_manual_v1.1.pdf" (at -8.89 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "802.11 Wi-Fi" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "802.11 b/g/n Wi-Fi Module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "ESP?12*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP-12E_0_1"
      (rectangle (start -12.7 17.78) (end 12.7 -15.24)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "ESP-12E_1_1"
      (pin input line (at -15.24 15.24 0) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -2.54 0) (length 2.54)
        (name "MISO" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -5.08 0) (length 2.54)
        (name "GPIO9" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -7.62 0) (length 2.54)
        (name "GPIO10" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -10.16 0) (length 2.54)
        (name "MOSI" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -12.7 0) (length 2.54)
        (name "SCLK" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -17.78 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
        (name "GPIO15" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
        (name "GPIO2" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
        (name "GPIO0" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
        (name "GPIO4" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 5.08 0) (length 2.54)
        (name "ADC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
        (name "GPIO5" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
        (name "GPIO3/RXD" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
        (name "GPIO1/TXD" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 10.16 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
        (name "GPIO16" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
        (name "GPIO14" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 0 180) (length 2.54)
        (name "GPIO12" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
        (name "GPIO13" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 20.32 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 0 0) (length 2.54)
        (name "CS0" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP-12F" (extends "ESP-12E")
    (property "Reference" "U" (at -12.7 19.05 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "ESP-12F" (at 12.7 19.05 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "RF_Module:ESP-12E" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://wiki.ai-thinker.com/_media/esp8266/esp8266_series_modules_user_manual_v1.1.pdf" (at -8.89 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "802.11 Wi-Fi" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "802.11 b/g/n Wi-Fi Module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "ESP?12*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "ESP-WROOM-02" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -7.62 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP-WROOM-02" (at 10.16 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:ESP-WROOM-02" (at 15.24 -13.97 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/0c-esp-wroom-02_datasheet_en.pdf" (at 1.27 38.1 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "RF Radio ESP Espressif" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Wi-Fi Module, ESP8266EX SoC, 32-bit, 802.11b/g/n, WPA/WPA2, 2.7-3.6V, SMD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "ESP?WROOM?02*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP-WROOM-02_0_1"
      (rectangle (start 10.16 12.7) (end -10.16 -12.7)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "ESP-WROOM-02_1_1"
      (pin power_in line (at 0 15.24 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 5.08 180) (length 2.54)
        (name "IO4" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -2.54 0) (length 2.54)
        (name "RXD" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -5.08 0) (length 2.54)
        (name "TXD" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 2.54 180) (length 2.54)
        (name "IO5" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 2.54)
        (name "RST" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 2.54)
        (name "TOUT" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -10.16 180) (length 2.54)
        (name "IO16" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -5.08 180) (length 2.54)
        (name "IO14" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 0 180) (length 2.54)
        (name "IO12" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
        (name "IO13" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -7.62 180) (length 2.54)
        (name "IO15" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 7.62 180) (length 2.54)
        (name "IO2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 10.16 180) (length 2.54)
        (name "IO0" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -15.24 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-PICO-D4" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -17.78 39.37 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "ESP32-PICO-D4" (at 3.81 39.37 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm" (at 0 -43.18 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-pico-d4_datasheet_en.pdf" (at 6.35 -25.4 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "RF Radio BT ESP ESP32 Espressif external antenna" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "RF Module, ESP32 SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, external antenna, QFN-48" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-PICO-D4_0_0"
      (pin power_in line (at -5.08 40.64 270) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 -25.4 180) (length 2.54)
        (name "IO34" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 -27.94 180) (length 2.54)
        (name "IO35" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -20.32 180) (length 2.54)
        (name "IO32" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -22.86 180) (length 2.54)
        (name "IO33" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -12.7 180) (length 2.54)
        (name "IO25" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -15.24 180) (length 2.54)
        (name "IO26" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -17.78 180) (length 2.54)
        (name "IO27" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 5.08 180) (length 2.54)
        (name "IO14" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 10.16 180) (length 2.54)
        (name "IO12" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 40.64 270) (length 2.54)
        (name "VDD3P3_RTC" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 35.56 180) (length 2.54)
        (name "LNA_IN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 7.62 180) (length 2.54)
        (name "IO13" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 2.54 180) (length 2.54)
        (name "IO15" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 25.4 180) (length 2.54)
        (name "IO2" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 30.48 180) (length 2.54)
        (name "IO0" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 20.32 180) (length 2.54)
        (name "IO4" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 0 0) (length 2.54)
        (name "IO16" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 20.32 -33.02 180) (length 2.54)
        (name "VDD_SDIO" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -2.54 0) (length 2.54)
        (name "IO17" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 15.24 180) (length 2.54)
        (name "SD2/IO9" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 12.7 180) (length 2.54)
        (name "SD3/IO10" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 40.64 270) (length 2.54)
        (name "VDDA3P3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -12.7 0) (length 2.54)
        (name "CMD" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -10.16 0) (length 2.54)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -5.08 0) (length 2.54)
        (name "SD0" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -7.62 0) (length 2.54)
        (name "SD1" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 17.78 180) (length 2.54)
        (name "IO5" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 0 180) (length 2.54)
        (name "IO18" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -10.16 180) (length 2.54)
        (name "IO23" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 40.64 270) (length 2.54)
        (name "VDD3P3_CPU" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -2.54 180) (length 2.54)
        (name "IO19" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -7.62 180) (length 2.54)
        (name "IO22" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -2.54 40.64 270) (length 2.54) hide
        (name "VDDA3P3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 22.86 180) (length 2.54)
        (name "U0RXD/IO3" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 27.94 180) (length 2.54)
        (name "U0TXD/IO1" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -5.08 180) (length 2.54)
        (name "IO21" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 40.64 270) (length 2.54) hide
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -17.78 -25.4 0) (length 2.54) hide
        (name "XTAL_N_NC" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -17.78 -27.94 0) (length 2.54) hide
        (name "XTAL_P_NC" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 40.64 270) (length 2.54) hide
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -17.78 -30.48 0) (length 2.54) hide
        (name "CAP2_NC" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -17.78 -33.02 0) (length 2.54) hide
        (name "CAP1_NC" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -40.64 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 30.48 0) (length 2.54)
        (name "SENSOR_VP" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 27.94 0) (length 2.54)
        (name "SENSOR_CAPP" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 25.4 0) (length 2.54)
        (name "SENSOR_CAPN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 22.86 0) (length 2.54)
        (name "SENSOR_VN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 35.56 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ESP32-PICO-D4_0_1"
      (rectangle (start -17.78 38.1) (end 17.78 -38.1)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "ESP32-S2-WROVER" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -12.7 29.21 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "ESP32-S2-WROVER" (at 2.54 29.21 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "RF_Module:ESP32-S2-WROVER" (at 19.05 -29.21 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s2-wroom_esp32-s2-wroom-i_datasheet_en.pdf" (at -7.62 -20.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "RF Radio ESP ESP32 Espressif onboard PCB antenna" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "RF Module, ESP32-D0WDQ6 SoC, Wi-Fi 802.11b/g/n, 32-bit, 2.7-3.6V, onboard antenna, SMD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "ESP32?S2?WROVER*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-S2-WROVER_0_1"
      (rectangle (start -12.7 27.94) (end 12.7 -25.4)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "ESP32-S2-WROVER_1_1"
      (pin power_in line (at 0 -27.94 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 5.08 0) (length 2.54)
        (name "IO07" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 2.54 0) (length 2.54)
        (name "IO08" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 0 0) (length 2.54)
        (name "IO09" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -2.54 0) (length 2.54)
        (name "IO10" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -5.08 0) (length 2.54)
        (name "IO11" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -7.62 0) (length 2.54)
        (name "IO12" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -10.16 0) (length 2.54)
        (name "IO13" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -12.7 0) (length 2.54)
        (name "IO14" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -15.24 0) (length 2.54)
        (name "IO15" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -17.78 0) (length 2.54)
        (name "IO16" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 30.48 270) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -20.32 0) (length 2.54)
        (name "IO17" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -22.86 0) (length 2.54)
        (name "IO18" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -17.78 180) (length 2.54)
        (name "USB_D-" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
        (name "USB_D+" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
        (name "IO21" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
        (name "IO26" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -27.94 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
        (name "IO33" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
        (name "IO34" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
        (name "IO35" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 22.86 0) (length 2.54)
        (name "IO00" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 0 180) (length 2.54)
        (name "IO36" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
        (name "IO37" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
        (name "IO38" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
        (name "IO39" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
        (name "IO40" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
        (name "IO41" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
        (name "IO42" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
        (name "TXD0" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 20.32 180) (length 2.54)
        (name "RXD0" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 22.86 180) (length 2.54)
        (name "IO45" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 20.32 0) (length 2.54)
        (name "IO01" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 25.4 180) (length 2.54)
        (name "IO46" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 25.4 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -27.94 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -27.94 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 17.78 0) (length 2.54)
        (name "IO02" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 15.24 0) (length 2.54)
        (name "IO03" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 12.7 0) (length 2.54)
        (name "IO04" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 10.16 0) (length 2.54)
        (name "IO05" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 7.62 0) (length 2.54)
        (name "IO06" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-S2-WROVER-I" (extends "ESP32-S2-WROVER")
    (property "Reference" "U" (at -12.7 29.21 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "ESP32-S2-WROVER-I" (at 2.54 29.21 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "RF_Module:ESP32-S2-WROVER" (at 19.05 -29.21 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s2-wroom_esp32-s2-wroom-i_datasheet_en.pdf" (at -7.62 -20.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "RF Radio ESP ESP32 Espressif onboard PCB antenna" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "RF Module, ESP32-D0WDQ6 SoC, Wi-Fi 802.11b/g/n, 32-bit, 2.7-3.6V, onboard antenna, SMD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "ESP32?S2?WROVER*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "ESP32-WROOM-32" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -12.7 34.29 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "ESP32-WROOM-32" (at 1.27 34.29 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "RF_Module:ESP32-WROOM-32" (at 0 -38.1 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32_datasheet_en.pdf" (at -7.62 1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "RF Radio BT ESP ESP32 Espressif onboard PCB antenna" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "RF Module, ESP32-D0WDQ6 SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, onboard antenna, SMD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "ESP32?WROOM?32*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-WROOM-32_0_1"
      (rectangle (start -12.7 33.02) (end 12.7 -33.02)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "ESP32-WROOM-32_1_1"
      (pin power_in line (at 0 -35.56 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
        (name "IO25" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
        (name "IO26" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -17.78 180) (length 2.54)
        (name "IO27" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
        (name "IO14" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
        (name "IO12" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -35.56 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
        (name "IO13" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -5.08 0) (length 2.54)
        (name "SHD/SD2" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -7.62 0) (length 2.54)
        (name "SWP/SD3" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -12.7 0) (length 2.54)
        (name "SCS/CMD" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 35.56 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -10.16 0) (length 2.54)
        (name "SCK/CLK" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 0 0) (length 2.54)
        (name "SDO/SD0" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -2.54 0) (length 2.54)
        (name "SDI/SD1" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
        (name "IO15" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 25.4 180) (length 2.54)
        (name "IO2" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 30.48 180) (length 2.54)
        (name "IO0" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 20.32 180) (length 2.54)
        (name "IO4" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
        (name "IO16" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
        (name "IO17" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
        (name "IO5" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 30.48 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 0 180) (length 2.54)
        (name "IO18" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
        (name "IO19" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -12.7 -27.94 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
        (name "SCA" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 22.86 180) (length 2.54)
        (name "RXD0/IO3" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 27.94 180) (length 2.54)
        (name "TXD0/IO1" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
        (name "IO23" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -35.56 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -35.56 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 25.4 0) (length 2.54)
        (name "SENSOR_VP" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 22.86 0) (length 2.54)
        (name "SENSOR_VN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 -25.4 180) (length 2.54)
        (name "IO34" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 -27.94 180) (length 2.54)
        (name "IO35" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -20.32 180) (length 2.54)
        (name "IO32" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -22.86 180) (length 2.54)
        (name "IO33" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-WROOM-32D" (extends "ESP32-WROOM-32")
    (property "Reference" "U" (at -12.7 34.29 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "ESP32-WROOM-32D" (at 1.27 34.29 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "RF_Module:ESP32-WROOM-32D" (at 16.51 -34.29 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32d_esp32-wroom-32u_datasheet_en.pdf" (at -7.62 1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "RF Radio BT ESP ESP32 Espressif onboard PCB antenna" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "RF Module, ESP32-D0WD SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, onboard antenna, SMD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "ESP32?WROOM?32D*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "ESP32-WROOM-32U" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -12.7 34.29 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "ESP32-WROOM-32U" (at 1.27 34.29 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "RF_Module:ESP32-WROOM-32U" (at 0 -38.1 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32d_esp32-wroom-32u_datasheet_en.pdf" (at -7.62 1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "RF Radio BT ESP ESP32 Espressif external U.FL antenna" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "RF Module, ESP32-D0WD SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, external antenna, SMD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "ESP32?WROOM?32U*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-WROOM-32U_0_1"
      (rectangle (start -12.7 33.02) (end 12.7 -33.02)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "ESP32-WROOM-32U_1_1"
      (pin power_in line (at 0 -35.56 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
        (name "IO25" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
        (name "IO26" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -17.78 180) (length 2.54)
        (name "IO27" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
        (name "IO14" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
        (name "IO12" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -35.56 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
        (name "IO13" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -5.08 0) (length 2.54)
        (name "SHD/SD2" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -7.62 0) (length 2.54)
        (name "SWP/SD3" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -12.7 0) (length 2.54)
        (name "SCS/CMD" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 35.56 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -10.16 0) (length 2.54)
        (name "SCK/CLK" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 0 0) (length 2.54)
        (name "SDO/SD0" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -2.54 0) (length 2.54)
        (name "SDI/SD1" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
        (name "IO15" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 25.4 180) (length 2.54)
        (name "IO2" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 30.48 180) (length 2.54)
        (name "IO0" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 20.32 180) (length 2.54)
        (name "IO4" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
        (name "IO16" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
        (name "IO17" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
        (name "IO5" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 30.48 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 0 180) (length 2.54)
        (name "IO18" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
        (name "IO19" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -12.7 -27.94 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
        (name "IO21" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 22.86 180) (length 2.54)
        (name "RXD0/IO3" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 27.94 180) (length 2.54)
        (name "TXD0/IO1" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
        (name "IO22" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
        (name "IO23" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -35.56 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -35.56 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 25.4 0) (length 2.54)
        (name "SENSOR_VP" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 22.86 0) (length 2.54)
        (name "SENSOR_VN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 -25.4 180) (length 2.54)
        (name "IO34" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 -27.94 180) (length 2.54)
        (name "IO35" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -20.32 180) (length 2.54)
        (name "IO32" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -22.86 180) (length 2.54)
        (name "IO33" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MDBT50Q-1MV2" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MDBT50Q-1MV2" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:Raytac_MDBT50Q" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.raytac.com/download/index.php?index_id=43" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "BLE ANT ZigBee Thread 802.15.4 nRF52840 nordic MDBT50Q" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52840 module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Raytac?MDBT50Q*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MDBT50Q-1MV2_0_1"
      (rectangle (start -17.78 43.18) (end 17.78 -43.18)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "MDBT50Q-1MV2_1_1"
      (pin power_in line (at 0 -45.72 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 20.32 0) (length 2.54)
        (name "P0.29" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
        (alternate "AIN5" input line)
      )
      (pin bidirectional line (at -20.32 33.02 0) (length 2.54)
        (name "P0.02" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
        (alternate "AIN0" input line)
      )
      (pin bidirectional line (at -20.32 15.24 0) (length 2.54)
        (name "P0.31" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
        (alternate "AIN7" input line)
      )
      (pin bidirectional line (at -20.32 22.86 0) (length 2.54)
        (name "P0.28" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
        (alternate "AIN4" input line)
      )
      (pin bidirectional line (at -20.32 17.78 0) (length 2.54)
        (name "P0.30" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
        (alternate "AIN6" input line)
      )
      (pin passive line (at 0 -45.72 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -20.32 180) (length 2.54)
        (name "P0.27" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 35.56 180) (length 2.54)
        (name "P0.00" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
        (alternate "XL1" input line)
      )
      (pin bidirectional line (at 20.32 33.02 180) (length 2.54)
        (name "P0.01" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
        (alternate "XL2" input line)
      )
      (pin bidirectional line (at 20.32 -17.78 180) (length 2.54)
        (name "P0.26" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -45.72 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 27.94 0) (length 2.54)
        (name "P0.04" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
        (alternate "AIN2" input line)
      )
      (pin bidirectional line (at -20.32 25.4 0) (length 2.54)
        (name "P0.05" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
        (alternate "AIN3" input line)
      )
      (pin bidirectional line (at 20.32 27.94 180) (length 2.54)
        (name "P0.06" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -35.56 180) (length 2.54)
        (name "P0.07" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
        (alternate "TRACECLK" output line)
      )
      (pin bidirectional line (at 20.32 25.4 180) (length 2.54)
        (name "P0.08" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -25.4 0) (length 2.54)
        (name "P1.08" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -33.02 180) (length 2.54)
        (name "P1.09" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
        (alternate "TRACEDATA3" output line)
      )
      (pin bidirectional line (at 20.32 -30.48 180) (length 2.54)
        (name "P0.11" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
        (alternate "TRACEDATA2" output line)
      )
      (pin power_in line (at -2.54 45.72 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -27.94 180) (length 2.54)
        (name "P0.12" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
        (alternate "TRACEDATA1" output line)
      )
      (pin bidirectional line (at -20.32 -27.94 0) (length 2.54)
        (name "P1.10" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 45.72 270) (length 2.54)
        (name "VDDH" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 5.08 45.72 270) (length 2.54)
        (name "DCCH" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 45.72 270) (length 2.54)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -45.72 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 0 0) (length 2.54)
        (name "D-" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -2.54 0) (length 2.54)
        (name "D+" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 17.78 180) (length 2.54)
        (name "P0.14" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 20.32 180) (length 2.54)
        (name "P0.13" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 12.7 180) (length 2.54)
        (name "P0.16" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 15.24 180) (length 2.54)
        (name "P0.15" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -30.48 0) (length 2.54)
        (name "P1.11" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 5.08 180) (length 2.54)
        (name "P0.18" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
        (alternate "~{RESET}" input line)
      )
      (pin bidirectional line (at 20.32 10.16 180) (length 2.54)
        (name "P0.17" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 0 180) (length 2.54)
        (name "P0.19" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -5.08 180) (length 2.54)
        (name "P0.21" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -2.54 180) (length 2.54)
        (name "P0.20" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -10.16 180) (length 2.54)
        (name "P0.23" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -7.62 180) (length 2.54)
        (name "P0.22" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -25.4 180) (length 2.54)
        (name "P1.00" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
        (alternate "TRACEDATA0" output line)
      )
      (pin bidirectional line (at 20.32 -12.7 180) (length 2.54)
        (name "P0.24" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -15.24 180) (length 2.54)
        (name "P0.25" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -33.02 0) (length 2.54)
        (name "P1.12" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -10.16 0) (length 2.54)
        (name "P1.02" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 40.64 0) (length 2.54)
        (name "SWDIO" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 10.16 0) (length 2.54)
        (name "P0.09" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
        (alternate "NFC1" input line)
      )
      (pin input line (at -20.32 38.1 0) (length 2.54)
        (name "SWDCLK" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 7.62 0) (length 2.54)
        (name "P0.10" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
        (alternate "NFC2" input line)
      )
      (pin passive line (at 0 -45.72 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -15.24 0) (length 2.54)
        (name "P1.04" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -20.32 0) (length 2.54)
        (name "P1.06" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -22.86 0) (length 2.54)
        (name "P1.07" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -17.78 0) (length 2.54)
        (name "P1.05" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -35.56 0) (length 2.54)
        (name "P1.13" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -12.7 0) (length 2.54)
        (name "P1.03" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -7.62 0) (length 2.54)
        (name "P1.01" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -38.1 0) (length 2.54)
        (name "P1.14" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -40.64 0) (length 2.54)
        (name "P1.15" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 30.48 0) (length 2.54)
        (name "P0.03" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
        (alternate "AIN1" input line)
      )
    )
  )
  (symbol "MDBT50Q-P1MV2" (extends "MDBT50Q-1MV2")
    (property "Reference" "U" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MDBT50Q-P1MV2" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:Raytac_MDBT50Q" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.raytac.com/download/index.php?index_id=43" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "BLE ANT ZigBee Thread 802.15.4 nRF52840 nordic MDBT50Q" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52840 module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Raytac?MDBT50Q*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MDBT50Q-U1MV2" (extends "MDBT50Q-1MV2")
    (property "Reference" "U" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MDBT50Q-U1MV2" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:Raytac_MDBT50Q" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.raytac.com/download/index.php?index_id=43" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "BLE ANT ZigBee Thread 802.15.4 nRF52840 nordic MDBT50Q" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52840 module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Raytac?MDBT50Q*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MDBT50Q-512K" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MDBT50Q-512K" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:Raytac_MDBT50Q" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.raytac.com/download/index.php?index_id=46" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "MCU, ARM, BLE, ANT, 2.4GHz, 802.15.4 MDBT50Q" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52833 module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Raytac?MDBT50Q*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MDBT50Q-512K_0_1"
      (rectangle (start -17.78 43.18) (end 17.78 -43.18)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "MDBT50Q-512K_1_1"
      (pin power_in line (at 0 -45.72 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 20.32 0) (length 2.54)
        (name "P0.29" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
        (alternate "AIN5" input line)
      )
      (pin bidirectional line (at -20.32 33.02 0) (length 2.54)
        (name "P0.02" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
        (alternate "AIN0" input line)
      )
      (pin bidirectional line (at -20.32 15.24 0) (length 2.54)
        (name "P0.31" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
        (alternate "AIN7" input line)
      )
      (pin bidirectional line (at -20.32 22.86 0) (length 2.54)
        (name "P0.28" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
        (alternate "AIN4" input line)
      )
      (pin bidirectional line (at -20.32 17.78 0) (length 2.54)
        (name "P0.30" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
        (alternate "AIN6" input line)
      )
      (pin passive line (at 0 -45.72 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -20.32 180) (length 2.54)
        (name "P0.27" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 35.56 180) (length 2.54)
        (name "P0.00" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
        (alternate "XL1" input line)
      )
      (pin bidirectional line (at 20.32 33.02 180) (length 2.54)
        (name "P0.01" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
        (alternate "XL2" input line)
      )
      (pin bidirectional line (at 20.32 -17.78 180) (length 2.54)
        (name "P0.26" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -45.72 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 27.94 0) (length 2.54)
        (name "P0.04" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
        (alternate "AIN2" input line)
      )
      (pin bidirectional line (at -20.32 25.4 0) (length 2.54)
        (name "P0.05" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
        (alternate "AIN3" input line)
      )
      (pin bidirectional line (at 20.32 27.94 180) (length 2.54)
        (name "P0.06" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -35.56 180) (length 2.54)
        (name "P0.07" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
        (alternate "TRACECLK" output line)
      )
      (pin bidirectional line (at 20.32 25.4 180) (length 2.54)
        (name "P0.08" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -40.64 0) (length 2.54)
        (name "P1.08" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -33.02 180) (length 2.54)
        (name "P1.09" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
        (alternate "TRACEDATA3" output line)
      )
      (pin bidirectional line (at 20.32 -30.48 180) (length 2.54)
        (name "P0.11" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
        (alternate "TRACEDATA2" output line)
      )
      (pin power_in line (at -2.54 45.72 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -27.94 180) (length 2.54)
        (name "P0.12" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
        (alternate "TRACEDATA1" output line)
      )
      (pin bidirectional line (at -20.32 -15.24 0) (length 2.54)
        (name "P0.25" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 45.72 270) (length 2.54)
        (name "VDDH" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 5.08 43.18 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 45.72 270) (length 2.54)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -45.72 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 0 0) (length 2.54)
        (name "D-" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -2.54 0) (length 2.54)
        (name "D+" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 17.78 180) (length 2.54)
        (name "P0.14" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 20.32 180) (length 2.54)
        (name "P0.13" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 12.7 180) (length 2.54)
        (name "P0.16" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 15.24 180) (length 2.54)
        (name "P0.15" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -17.78 -17.78 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 5.08 180) (length 2.54)
        (name "P0.18" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
        (alternate "~{RESET}" input line)
      )
      (pin bidirectional line (at 20.32 10.16 180) (length 2.54)
        (name "P0.17" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 17.78 0 180) (length 2.54) hide
        (name "P0.19" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -5.08 180) (length 2.54)
        (name "P0.21" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -2.54 180) (length 2.54)
        (name "P0.20" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 17.78 -10.16 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -7.62 180) (length 2.54)
        (name "P0.22" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -25.4 180) (length 2.54)
        (name "P1.00" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
        (alternate "TRACEDATA0" output line)
      )
      (pin bidirectional line (at 20.32 -12.7 180) (length 2.54)
        (name "P0.24" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 17.78 -15.24 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -12.7 0) (length 2.54)
        (name "P0.23" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -25.4 0) (length 2.54)
        (name "P1.02" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 40.64 0) (length 2.54)
        (name "SWDIO" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 10.16 0) (length 2.54)
        (name "P0.09" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
        (alternate "NFC1" input line)
      )
      (pin input line (at -20.32 38.1 0) (length 2.54)
        (name "SWDCLK" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 7.62 0) (length 2.54)
        (name "P0.10" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
        (alternate "NFC2" input line)
      )
      (pin passive line (at 0 -45.72 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -30.48 0) (length 2.54)
        (name "P1.04" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -35.56 0) (length 2.54)
        (name "P1.06" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -38.1 0) (length 2.54)
        (name "P1.07" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 17.78 38.1 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -33.02 0) (length 2.54)
        (name "P1.05" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 17.78 40.64 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -22.86 0) (length 2.54)
        (name "P1.01" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -27.94 0) (length 2.54)
        (name "P1.03" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -10.16 0) (length 2.54)
        (name "P0.19" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 30.48 0) (length 2.54)
        (name "P0.03" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
        (alternate "AIN1" input line)
      )
    )
  )
  (symbol "MDBT50Q-P512K" (extends "MDBT50Q-512K")
    (property "Reference" "U" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MDBT50Q-P512K" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:Raytac_MDBT50Q" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.raytac.com/download/index.php?index_id=46" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "MCU, ARM, BLE, ANT, 2.4GHz, 802.15.4 MDBT50Q" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52833 module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Raytac?MDBT50Q*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MDBT50Q-U512K" (extends "MDBT50Q-512K")
    (property "Reference" "U" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MDBT50Q-U512K" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:Raytac_MDBT50Q" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.raytac.com/download/index.php?index_id=46" (at 0 -5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "MCU, ARM, BLE, ANT, 2.4GHz, 802.15.4 MDBT50Q" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52833 module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Raytac?MDBT50Q*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "MM002" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -26.67 21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MM002" (at 24.13 21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at -13.97 -27.94 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.nemeus.fr/resources/uploads/2015/04/MM002-xx-EU_datasheet_v0.11.pdf" (at -13.97 -27.94 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IOT LoRa SIGFOX" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "NEMEUS Modem dual-mode LoRa/SIGFOX" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MM002_0_1"
      (rectangle (start -27.94 20.32) (end 27.94 -17.78)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "MM002_1_1"
      (pin power_in line (at -5.08 -20.32 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -30.48 2.54 0) (length 2.54)
        (name "PA15-IO/JTDI" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -30.48 10.16 0) (length 2.54)
        (name "PA14-IO/JTCK/SWCLK" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -30.48 7.62 0) (length 2.54)
        (name "PA13-IO/JTMS/SWDAT" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -30.48 -7.62 0) (length 2.54)
        (name "PA12-IO/UART1-RTS/USB-DP" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -30.48 -5.08 0) (length 2.54)
        (name "PA11-IO/UART1-CTS/USB-DM" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -20.32 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -20.32 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -15.24 180) (length 2.54)
        (name "ANT" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -20.32 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -10.16 180) (length 2.54)
        (name "PA7-IO/SPI-MOSI" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -30.48 15.24 0) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -5.08 180) (length 2.54)
        (name "PA5-IO/SPI-SCK" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -7.62 180) (length 2.54)
        (name "PA6-IO/SPI-MISO" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -2.54 180) (length 2.54)
        (name "PA4-IO/SPI-NSS" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 10.16 180) (length 2.54)
        (name "PA3-IO/ADC/UART2-RX" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 12.7 180) (length 2.54)
        (name "PA2-IO/ADC/UART2-TX" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 17.78 180) (length 2.54)
        (name "PA0-IO/ADC/UART2-CTS/WKUP" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 15.24 180) (length 2.54)
        (name "PA1-IO/ADC/UART2-RTS" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -15.24 22.86 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -20.32 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 2.54 180) (length 2.54)
        (name "PB9-IO/I2C-SDA" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 5.08 180) (length 2.54)
        (name "PB8-IO/I2C-SCL" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -30.48 17.78 0) (length 2.54)
        (name "BOOT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -30.48 -12.7 0) (length 2.54)
        (name "PB7-IO/UART1-RX" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -30.48 -10.16 0) (length 2.54)
        (name "PB6-IO/UART1-TX" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -30.48 0 0) (length 2.54)
        (name "PB4-IO/NJTRST" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -30.48 5.08 0) (length 2.54)
        (name "PB3-IO/JTDO" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Particle_P1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -24.13 46.99 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Particle_P1" (at -24.13 49.53 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:Particle_P1" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://docs.particle.io/datasheets/p1-datasheet/" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Wi-Fi module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Wi-Fi module, 1MB flash, 128KB RAM" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Particle*P1*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Particle_P1_1_1"
      (rectangle (start -25.4 45.72) (end 25.4 -45.72)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin power_in line (at -22.86 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -25.4 35.56 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 25.4 35.56 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 25.4 38.1 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -15.24 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 25.4 40.64 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 2.54 180) (length 2.54)
        (name "WL_JTAG_TDI" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 0 180) (length 2.54)
        (name "WL_JTAG_TCK" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -2.54 180) (length 2.54)
        (name "WL_JTAG_~{TRST}" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -5.08 180) (length 2.54)
        (name "WL_JTAG_TMS" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 48.26 270) (length 2.54)
        (name "VBAT_WL" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -7.62 180) (length 2.54)
        (name "WL_JTAG_TDO" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 0 0) (length 2.54)
        (name "MICRO_SPI1_MISO/PA6" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 -2.54 0) (length 2.54)
        (name "MICRO_SPI1_SCK/PA5" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 -5.08 0) (length 2.54)
        (name "MICRO_SPI1_MOSI/PA7" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 -7.62 0) (length 2.54)
        (name "MICRO_SPI1_SS/PA4" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 48.26 270) (length 2.54)
        (name "VDD_3V3" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 48.26 270) (length 2.54)
        (name "VDD_3V3" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 -20.32 0) (length 2.54)
        (name "MICRO_UART2_RTS/PA1" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 48.26 270) (length 2.54)
        (name "VBAT_WL" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 -22.86 0) (length 2.54)
        (name "MICRO_UART2_CTS/PA0" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 -25.4 0) (length 2.54)
        (name "MICRO_UART2_RXD/PA3" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 -27.94 0) (length 2.54)
        (name "MICRO_UART2_TXD/PA2" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -27.94 180) (length 2.54)
        (name "TESTMODE" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -33.02 180) (length 2.54)
        (name "MICRO_~{RST}" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 -12.7 0) (length 2.54)
        (name "MICRO_I2C1_SCL/PB6" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 -15.24 0) (length 2.54)
        (name "MICRO_I2C1_SDA/PB7" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.7 48.26 270) (length 2.54)
        (name "VBAT_MICRO" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -20.32 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 30.48 0) (length 2.54)
        (name "MICRO_GPIO_1/PB0" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 27.94 0) (length 2.54)
        (name "MICRO_GPIO_2/PB1" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 25.4 0) (length 2.54)
        (name "MICRO_GPIO_3/PC0" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 22.86 0) (length 2.54)
        (name "MICRO_GPIO_5/PC3" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 20.32 0) (length 2.54)
        (name "MICRO_GPIO_6/PC4" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 17.78 0) (length 2.54)
        (name "MICRO_GPIO_7/PB5" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 15.24 0) (length 2.54)
        (name "MICRO_GPIO_8/PC7" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 12.7 0) (length 2.54)
        (name "MICRO_GPIO_9/PC13" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 10.16 0) (length 2.54)
        (name "MICRO_GPIO_12/PC1" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 7.62 0) (length 2.54)
        (name "MICRO_GPIO_13/PC2" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 48.26 270) (length 2.54)
        (name "VDDIO_3V3_WL" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 5.08 0) (length 2.54)
        (name "MICRO_GPIO_14/PC5" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 17.78 180) (length 2.54)
        (name "MICRO_JTAG_~{TRST}/PB4" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 15.24 180) (length 2.54)
        (name "MICRO_JTAG_TDO/PB3" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 12.7 180) (length 2.54)
        (name "MICRO_JTAG_TDI/PA15" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 10.16 180) (length 2.54)
        (name "MICRO_JTAG_TMS/PA13" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 7.62 180) (length 2.54)
        (name "MICRO_JTAG_TCK/PA14" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -12.7 180) (length 2.54)
        (name "BTCX_STATUS" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -15.24 180) (length 2.54)
        (name "BTCX_RF_ACTIVE" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -17.78 180) (length 2.54)
        (name "BTCX_TXCONF" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -17.78 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -22.86 180) (length 2.54)
        (name "WL_SLEEP_CLK" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 30.48 180) (length 2.54)
        (name "MICRO_UART1_RTS/PA12" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 27.94 180) (length 2.54)
        (name "MICRO_UART1_CTS/PA11" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 25.4 180) (length 2.54)
        (name "MICRO_UART1_RXD/PA10" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 22.86 180) (length 2.54)
        (name "MICRO_UART1_TXD/PA9" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "65" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "66" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "67" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "68" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.7 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "69" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 48.26 270) (length 2.54)
        (name "WL_REG_ON" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 15.24 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "70" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "71" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "72" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -48.26 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "73" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -25.4 -33.02 0) (length 2.54) hide
        (name "PAD1" (effects (font (size 1.27 1.27))))
        (number "74" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -25.4 -35.56 0) (length 2.54) hide
        (name "PAD2" (effects (font (size 1.27 1.27))))
        (number "75" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -25.4 40.64 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -25.4 38.1 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "RAK4200" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "RAK4200" (at 0 25.4 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:RAK4200" (at 5.08 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK4200/Hardware-Specification/RAK4200_Module_Specifications_V1.4.pdf" (at 5.08 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IoT, LoRa, LoRaWAN, RF" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LoRa Module, STM32L071,  RAKwireless" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "RAK4200*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RAK4200_0_1"
      (rectangle (start -17.78 20.32) (end 17.78 -20.32)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "RAK4200_1_1"
      (pin bidirectional line (at -20.32 10.16 0) (length 2.54)
        (name "PA3/UART2_RX" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 12.7 180) (length 2.54)
        (name "I2C_SDA/PB7" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -15.24 180) (length 2.54)
        (name "RF" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 7.62 0) (length 2.54)
        (name "PA5/SPI_CLK" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 5.08 0) (length 2.54)
        (name "PA6/SPI_MISO" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 2.54 0) (length 2.54)
        (name "PA7/SPI_MOSI" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -15.24 0) (length 2.54)
        (name "~{MCU_NRESET}" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 12.7 0) (length 2.54)
        (name "PA2/UART2_TX" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 22.86 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 15.24 0) (length 2.54)
        (name "PA1/UART2_DE" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 0 0) (length 2.54)
        (name "PA9/UART1_TX" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -2.54 0) (length 2.54)
        (name "PA10/UART1_RX" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -5.08 0) (length 2.54)
        (name "PA12/UART1_DE" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -7.62 0) (length 2.54)
        (name "PA13/SWDIO" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -10.16 0) (length 2.54)
        (name "PA14/SWCLK" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 15.24 180) (length 2.54)
        (name "I2C_SCL/PB6" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "RAK811-HF-EU868" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "RAK811-HF-EU868" (at 0 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:RAK811" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IoT LoRa LoRaWAN RF" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LoRa Module, STM32L151, EU868, RAKwireless" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "RAK811*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RAK811-HF-EU868_0_0"
      (pin power_in line (at 0 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 0 0) (length 2.54)
        (name "PA13" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 22.86 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -2.54 0) (length 2.54)
        (name "PA14" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -5.08 0) (length 2.54)
        (name "PA15" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
        (name "PB3" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
        (name "PB5" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -17.78 0) (length 2.54)
        (name "BOOT0" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
        (name "PB8" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
        (name "PB9" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
        (name "PB12" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 12.7 0) (length 2.54)
        (name "PA2" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 15.24 0) (length 2.54)
        (name "PA1" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 17.78 0) (length 2.54)
        (name "PA0" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -12.7 0) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
        (name "PB10" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 0 180) (length 2.54)
        (name "PB11" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
        (name "PB2" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
        (name "PB14" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 -12.7 180) (length 2.54)
        (name "RF_OUT" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
        (name "PB15" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 10.16 0) (length 2.54)
        (name "PA8" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 7.62 0) (length 2.54)
        (name "PA9/USART1_TX" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 5.08 0) (length 2.54)
        (name "PA10/USART1_RX" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 2.54 0) (length 2.54)
        (name "PA12" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
        (name "PB4" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "RAK811-HF-EU868_0_1"
      (rectangle (start 12.7 -20.32) (end -12.7 20.32)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "RAK811-HF-AS923" (extends "RAK811-HF-EU868")
    (property "Reference" "U" (at 0 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "RAK811-HF-AS923" (at 0 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:RAK811" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IoT LoRa LoRaWAN RF" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LoRa Module, STM32L151, AS923, RAKwireless" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "RAK811*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RAK811-HF-AU915" (extends "RAK811-HF-EU868")
    (property "Reference" "U" (at 0 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "RAK811-HF-AU915" (at 0 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:RAK811" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IoT LoRa LoRaWAN RF" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LoRa Module, STM32L151, AU915, RAKwireless" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "RAK811*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RAK811-HF-IN865" (extends "RAK811-HF-EU868")
    (property "Reference" "U" (at 0 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "RAK811-HF-IN865" (at 0 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:RAK811" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IoT LoRa LoRaWAN RF" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LoRa Module, STM32L151, IN865, RAKwireless" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "RAK811*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RAK811-HF-KR920" (extends "RAK811-HF-EU868")
    (property "Reference" "U" (at 0 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "RAK811-HF-KR920" (at 0 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:RAK811" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IoT LoRa LoRaWAN RF" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LoRa Module, STM32L151, KR920, RAKwireless" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "RAK811*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RAK811-HF-US915" (extends "RAK811-HF-EU868")
    (property "Reference" "U" (at 0 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "RAK811-HF-US915" (at 0 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:RAK811" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IoT LoRa LoRaWAN RF" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LoRa Module, STM32L151, US915, RAKwireless" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "RAK811*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RAK811-LF-EU433" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "RAK811-LF-EU433" (at 0 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:RAK811" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IoT LoRa LoRaWAN RF" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LoRa Module, STM32L151, EU433, RAKwireless" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "RAK811*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RAK811-LF-EU433_0_0"
      (pin power_in line (at 0 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -2.54 0) (length 2.54)
        (name "PA13" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 22.86 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -5.08 0) (length 2.54)
        (name "PA14" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -7.62 0) (length 2.54)
        (name "PA15" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 10.16 0) (length 2.54)
        (name "PA3" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
        (name "PB5" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -17.78 0) (length 2.54)
        (name "BOOT0" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
        (name "PB6" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
        (name "PB7" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
        (name "PB12" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 12.7 0) (length 2.54)
        (name "PA2" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 15.24 0) (length 2.54)
        (name "PA1" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 17.78 0) (length 2.54)
        (name "PA0" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -12.7 0) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
        (name "PB10" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
        (name "PB11" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
        (name "PB2" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
        (name "PB14" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 -12.7 180) (length 2.54)
        (name "RF_OUT" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -22.86 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
        (name "PB15" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 0 180) (length 2.54)
        (name "PB13" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 7.62 0) (length 2.54)
        (name "PA9/USART1_TX" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 5.08 0) (length 2.54)
        (name "PA10/USART1_RX" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 0 0) (length 2.54)
        (name "PA12" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 2.54 0) (length 2.54)
        (name "PA11" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "RAK811-LF-EU433_0_1"
      (rectangle (start 12.7 -20.32) (end -12.7 20.32)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "RAK811-LF-CN470" (extends "RAK811-LF-EU433")
    (property "Reference" "U" (at 0 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "RAK811-LF-CN470" (at 0 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:RAK811" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://downloads.rakwireless.com/LoRa/RAK811/Hardware_Specification/RAK811_LoRa_Module_Datasheet_V1.4.pdf" (at -11.43 31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IoT LoRa LoRaWAN RF" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "LoRa Module, STM32L151, CN470, RAKwireless" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "RAK811*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RFM69HW" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -3.81 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "RFM69HW" (at -7.62 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:HOPERF_RFM69HW" (at 0 -15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbb56f1fd7.pdf" (at 0 -7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Radio ISM Transceiver Module AES" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ISM Radio Transceiver Module, SPI interface" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HOPERF*RFM69HW*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RFM69HW_0_1"
      (rectangle (start -10.16 10.16) (end 10.16 -10.16)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "RFM69HW_1_1"
      (pin input line (at -12.7 -5.08 0) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 7.62 180) (length 2.54)
        (name "ANA" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 -12.7 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 2.54)
        (name "SCK" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 5.08 0) (length 2.54)
        (name "MISO" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 2.54)
        (name "MOSI" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 2.54)
        (name "NSS" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -2.54 -10.16 90) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 5.08 180) (length 2.54)
        (name "DIO0" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 2.54 180) (length 2.54)
        (name "DIO1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 0 180) (length 2.54)
        (name "DIO2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
        (name "DIO3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -5.08 180) (length 2.54)
        (name "DIO4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -7.62 180) (length 2.54)
        (name "DIO5" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "3.3V" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "RFM69W" (extends "RFM69HW")
    (property "Reference" "U" (at -3.81 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "RFM69W" (at -7.62 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:HOPERF_RFM69HW" (at 0 -15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbe34756e1.pdf" (at 0 -7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Radio, ISM, Transceiver, Module, AES" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ISM Radio Transceiver Module, SPI interface" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HOPERF*RFM69HW*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RFM95W-868S2" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -10.414 11.684 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "RFM95W-868S2" (at 1.524 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Low power long range transceiver module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low power long range transceiver module, SPI and parallel interface, 868 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HOPERF*RFM9XW*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RFM95W-868S2_0_1"
      (rectangle (start -10.16 10.16) (end 10.16 -12.7)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "RFM95W-868S2_1_1"
      (pin power_in line (at -2.54 -15.24 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -15.24 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
        (name "DIO3" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 0 180) (length 2.54)
        (name "DIO4" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "3.3V" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -10.16 180) (length 2.54)
        (name "DIO0" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -7.62 180) (length 2.54)
        (name "DIO1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -5.08 180) (length 2.54)
        (name "DIO2" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 2.54 0) (length 2.54)
        (name "MISO" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 2.54)
        (name "MOSI" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 2.54)
        (name "SCK" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 2.54)
        (name "NSS" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -5.08 0) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 2.54 180) (length 2.54)
        (name "DIO5" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -15.24 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 7.62 180) (length 2.54)
        (name "ANT" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "RFM69HCW" (extends "RFM95W-868S2")
    (property "Reference" "U" (at -10.414 11.684 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "RFM69HCW" (at 1.524 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcb8284d838.pdf" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "low power Radio ISM Transceiver Module AES encryption SPI HopeRF" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low power ISM Radio Transceiver Module, SPI interface, AES encryption, 434 or 915 MHz, up to 100mW, up to 300 kb/s, SMD-16, DIP-16" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HOPERF*RFM9XW*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RFM95W-915S2" (extends "RFM95W-868S2")
    (property "Reference" "U" (at -10.414 11.684 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "RFM95W-915S2" (at 1.524 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Low power long range transceiver module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low power long range transceiver module, SPI and parallel interface, 915 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HOPERF*RFM9XW*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RFM96W-315S2" (extends "RFM95W-868S2")
    (property "Reference" "U" (at -10.414 11.684 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "RFM96W-315S2" (at 1.524 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcc0ac60235.pdf" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Low power long range transceiver module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low power long range transceiver module, SPI and parallel interface, 315 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HOPERF*RFM9XW*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RFM96W-433S2" (extends "RFM95W-868S2")
    (property "Reference" "U" (at -10.414 11.684 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "RFM96W-433S2" (at 1.524 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcc0ac60235.pdf" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Low power long range transceiver module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low power long range transceiver module, SPI and parallel interface, 433 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HOPERF*RFM9XW*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RFM97W-868S2" (extends "RFM95W-868S2")
    (property "Reference" "U" (at -10.414 11.684 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "RFM97W-868S2" (at 1.524 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Low power long range transceiver module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low power long range transceiver module, SPI and parallel interface, 868 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -139 dBm, SMD-16, DIP-16" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HOPERF*RFM9XW*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RFM97W-915S2" (extends "RFM95W-868S2")
    (property "Reference" "U" (at -10.414 11.684 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "RFM97W-915S2" (at 1.524 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Low power long range transceiver module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low power long range transceiver module, SPI and parallel interface, 915 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -139 dBm, SMD-16, DIP-16" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HOPERF*RFM9XW*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RFM98W-315S2" (extends "RFM95W-868S2")
    (property "Reference" "U" (at -10.414 11.684 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "RFM98W-315S2" (at 1.524 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcdb5e17543.pdf" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Low power long range transceiver module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low power long range transceiver module, SPI and parallel interface, 315 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HOPERF*RFM9XW*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "RFM98W-433S2" (extends "RFM95W-868S2")
    (property "Reference" "U" (at -10.414 11.684 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "RFM98W-433S2" (at 1.524 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.hoperf.com/data/upload/portal/20181127/5bfcdb5e17543.pdf" (at -83.82 41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Low power long range transceiver module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low power long range transceiver module, SPI and parallel interface, 433 MHz, spreading factor 6 to12, bandwidth 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "HOPERF*RFM9XW*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "STM32WB5MMG" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 7.62 59.69 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "STM32WB5MMG" (at 10.16 -59.69 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:ST-SiP-LGA-86-11x7.3mm" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32wb5mmg.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "bluetooth bluetooth5 bluetooth5.0 802.15.4 zigbee module stm32 rf ARM Cortex-M3 Cortex-M0+" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ST Microelectronics STM32WB55VG ARM Cortex Bluetooth Low Energy 5.0, Zigbee and 802.15.4 module, 1 MB Flash, 256kb RAM, Fully integrated BOM" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "RF?Module:ST?SiP?LGA?86?11x7.3mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "STM32WB5MMG_1_1"
      (rectangle (start -10.16 58.42) (end 10.16 -58.42)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (pin bidirectional line (at 12.7 40.64 180) (length 2.54)
        (name "PA2" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -50.8 180) (length 2.54)
        (name "NRST" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -20.32 180) (length 2.54)
        (name "PB9" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -22.86 0) (length 2.54)
        (name "PC0" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 45.72 0) (length 2.54)
        (name "PH3-BOOT0" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -17.78 180) (length 2.54)
        (name "PB8" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 60.96 270) (length 2.54)
        (name "VBAT" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -60.96 90) (length 2.54)
        (name "VSSSMPS" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 60.96 270) (length 2.54)
        (name "VDDSMPS" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -15.24 180) (length 2.54)
        (name "PB7" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -10.16 180) (length 2.54)
        (name "PB5" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 43.18 180) (length 2.54)
        (name "PA1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -7.62 180) (length 2.54)
        (name "PB4" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -5.08 180) (length 2.54)
        (name "PB3" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -48.26 0) (length 2.54)
        (name "PC10" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -50.8 0) (length 2.54)
        (name "PC11" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -53.34 0) (length 2.54)
        (name "PC12" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 12.7 180) (length 2.54)
        (name "PA13" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 10.16 180) (length 2.54)
        (name "PA14" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 7.62 180) (length 2.54)
        (name "PA15" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 20.32 180) (length 2.54)
        (name "PA10" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 15.24 180) (length 2.54)
        (name "PA12" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 45.72 180) (length 2.54)
        (name "PA0" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 17.78 180) (length 2.54)
        (name "PA11" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -60.96 90) (length 2.54) hide
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 60.96 270) (length 2.54)
        (name "VDDUSB" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 20.32 0) (length 2.54)
        (name "PD0" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 17.78 0) (length 2.54)
        (name "PD1" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -30.48 180) (length 2.54)
        (name "PB13" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -38.1 0) (length 2.54)
        (name "PC6" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -33.02 180) (length 2.54)
        (name "PB14" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -35.56 180) (length 2.54)
        (name "PB15" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -12.7 180) (length 2.54)
        (name "PB6" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 60.96 270) (length 2.54)
        (name "VREF" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -55.88 0) (length 2.54)
        (name "PC13" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -27.94 180) (length 2.54)
        (name "PB12" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 35.56 0) (length 2.54)
        (name "PE4" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 0 180) (length 2.54)
        (name "PB1" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 2.54 180) (length 2.54)
        (name "PB0" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -35.56 0) (length 2.54)
        (name "PC5" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -25.4 180) (length 2.54)
        (name "PB11" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -22.86 180) (length 2.54)
        (name "PB10" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
        (name "PB2" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -33.02 0) (length 2.54)
        (name "PC4" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -60.96 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 25.4 180) (length 2.54)
        (name "PA8" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 22.86 180) (length 2.54)
        (name "PA9" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 27.94 180) (length 2.54)
        (name "PA7" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 30.48 180) (length 2.54)
        (name "PA6" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 33.02 180) (length 2.54)
        (name "PA5" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 35.56 180) (length 2.54)
        (name "PA4" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 38.1 180) (length 2.54)
        (name "PA3" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -60.96 90) (length 2.54) hide
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -40.64 180) (length 2.54)
        (name "ANT_IN" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.7 -43.18 180) (length 2.54)
        (name "RF_OUT" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 60.96 270) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -60.96 90) (length 2.54) hide
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 40.64 0) (length 2.54)
        (name "PH0" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 43.18 0) (length 2.54)
        (name "PH1" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -15.24 0) (length 2.54)
        (name "PD14" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 27.94 0) (length 2.54)
        (name "PE1" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -12.7 0) (length 2.54)
        (name "PD13" (effects (font (size 1.27 1.27))))
        (number "65" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -10.16 0) (length 2.54)
        (name "PD12" (effects (font (size 1.27 1.27))))
        (number "66" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 2.54 0) (length 2.54)
        (name "PD7" (effects (font (size 1.27 1.27))))
        (number "67" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 15.24 0) (length 2.54)
        (name "PD2" (effects (font (size 1.27 1.27))))
        (number "68" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -45.72 0) (length 2.54)
        (name "PC9" (effects (font (size 1.27 1.27))))
        (number "69" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -30.48 0) (length 2.54)
        (name "PC3" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 12.7 0) (length 2.54)
        (name "PD3" (effects (font (size 1.27 1.27))))
        (number "70" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -40.64 0) (length 2.54)
        (name "PC7" (effects (font (size 1.27 1.27))))
        (number "71" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 33.02 0) (length 2.54)
        (name "PE3" (effects (font (size 1.27 1.27))))
        (number "72" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 10.16 0) (length 2.54)
        (name "PD4" (effects (font (size 1.27 1.27))))
        (number "73" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -2.54 0) (length 2.54)
        (name "PD9" (effects (font (size 1.27 1.27))))
        (number "74" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 0 0) (length 2.54)
        (name "PD8" (effects (font (size 1.27 1.27))))
        (number "75" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -17.78 0) (length 2.54)
        (name "PD15" (effects (font (size 1.27 1.27))))
        (number "76" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -5.08 0) (length 2.54)
        (name "PD10" (effects (font (size 1.27 1.27))))
        (number "77" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 30.48 0) (length 2.54)
        (name "PE2" (effects (font (size 1.27 1.27))))
        (number "78" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 25.4 0) (length 2.54)
        (name "PE0" (effects (font (size 1.27 1.27))))
        (number "79" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -27.94 0) (length 2.54)
        (name "PC2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 7.62 0) (length 2.54)
        (name "PD5" (effects (font (size 1.27 1.27))))
        (number "80" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 5.08 0) (length 2.54)
        (name "PD6" (effects (font (size 1.27 1.27))))
        (number "81" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -7.62 0) (length 2.54)
        (name "PD11" (effects (font (size 1.27 1.27))))
        (number "82" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -43.18 0) (length 2.54)
        (name "PC8" (effects (font (size 1.27 1.27))))
        (number "83" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -60.96 90) (length 2.54) hide
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "84" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 -45.72 180) (length 2.54) hide
        (name "ANT_NC" (effects (font (size 1.27 1.27))))
        (number "85" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -60.96 90) (length 2.54) hide
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "86" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -25.4 0) (length 2.54)
        (name "PC1" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TD1205" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -11.43 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TD1205" (at 8.89 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:TD1205" (at 11.43 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://github.com/Telecom-Design/Documentation_TD_RF_Module/blob/master/TD1205%20Datasheet.pdf" (at -6.35 -35.56 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IOT SIGFOX GPS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "High-Performance, Low-Current SIGFOX™ Gateway And GPS Receiver With Integrated Antennas" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TD1205*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TD1205_0_1"
      (rectangle (start -12.7 10.16) (end 12.7 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "TD1205_1_1"
      (pin power_in line (at -5.08 -10.16 90) (length 2.54)
        (name "BAT-" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 12.7 270) (length 2.54)
        (name "BAT+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 12.7 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 2.54 180) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
        (name "UART-TX" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
        (name "UART-RX" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
        (name "DB2-SWDIO" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
        (name "DB3-SWCLK" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TD1208" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -11.43 19.05 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TD1208" (at 8.89 19.05 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RF_Module:TD1208" (at 17.78 -21.59 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://github.com/Telecom-Design/Documentation_TD_RF_Module/blob/master/TD1208%20Datasheet.pdf" (at -6.35 -27.94 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IOT SIGFOX" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "High-Performance, Low-Current SIGFOX™ Gateway" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TD1208*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TD1208_0_1"
      (rectangle (start -12.7 17.78) (end 12.7 -20.32)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "TD1208_1_1"
      (pin power_in line (at -7.62 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
        (name "USR2" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
        (name "USR3" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 2.54 0) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
        (name "DAC0" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
        (name "USR0" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
        (name "USR1" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -2.54 0) (length 2.54)
        (name "UART-TX" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -5.08 0) (length 2.54)
        (name "UART-RX" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 0 180) (length 2.54)
        (name "ADC0" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
        (name "TIM2" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -22.86 90) (length 2.54)
        (name "RF_GND" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
        (name "RF" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 -22.86 90) (length 2.54)
        (name "RF_GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at -15.24 12.7 0) (length 2.54)
        (name "Reserved" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
        (name "USR4" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 5.08 0) (length 2.54)
        (name "DB3-SWCLK" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 7.62 0) (length 2.54)
        (name "DB2-SWDIO" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -10.16 0) (length 2.54)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -12.7 0) (length 2.54)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 20.32 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TR-52DA" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -25.4 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TR-52DA" (at 25.4 11.43 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "RF_Module:IQRF_TRx2DA_KON-SIM-01" (at -25.4 -11.43 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "https://iqrf.org/weben/downloads.php?id=213" (at 25.4 -13.97 0)
      (effects (font (size 1.27 1.27)) (justify right) hide)
    )
    (property "ki_keywords" "IQRF common transceiver, PCB antenna, FSK modulation" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "IQRF common transceiver with PCB antenna, FSK modulation" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "IQRF?TRx2DA?KON?SIM?01*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TR-52DA_0_1"
      (rectangle (start -25.4 10.16) (end 25.4 -10.16)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "TR-52DA_1_1"
      (pin bidirectional line (at -27.94 2.54 0) (length 2.54)
        (name "RA0/AN0/C12IN0" (effects (font (size 1.27 1.27))))
        (number "C1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 0 0) (length 2.54)
        (name "RC2/VOUT" (effects (font (size 1.27 1.27))))
        (number "C2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "C3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "C4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -2.54 180) (length 2.54)
        (name "RA5/RB4/RC6/AN4/AN11/TX/~{SS}/C2OUT/CCP3" (effects (font (size 1.27 1.27))))
        (number "C5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 0 180) (length 2.54)
        (name "RC3/SCK/SCL" (effects (font (size 1.27 1.27))))
        (number "C6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 2.54 180) (length 2.54)
        (name "RC4/SDI/SDA" (effects (font (size 1.27 1.27))))
        (number "C7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 5.08 180) (length 2.54)
        (name "RC5/RC7/RX/SDO" (effects (font (size 1.27 1.27))))
        (number "C8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "DCTR-52DA" (extends "TR-52DA")
    (property "Reference" "U" (at -25.4 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "DCTR-52DA" (at 25.4 11.43 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "RF_Module:IQRF_TRx2DA_KON-SIM-01" (at -25.4 -11.43 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "https://iqrf.org/weben/downloads.php?id=213" (at 25.4 -13.97 0)
      (effects (font (size 1.27 1.27)) (justify right) hide)
    )
    (property "ki_keywords" "IQRF data controlled transceiver, PCB antenna, FSK modulation" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "IQRF data controlled transceiver with PCB antenna, FSK modulation" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "IQRF?TRx2DA?KON?SIM?01*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "DCTR-52DAT" (extends "TR-52DA")
    (property "Reference" "U" (at -25.4 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "DCTR-52DAT" (at 25.4 11.43 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "RF_Module:IQRF_TRx2DA_KON-SIM-01" (at -25.4 -11.43 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "https://iqrf.org/weben/downloads.php?id=213" (at 25.4 -13.97 0)
      (effects (font (size 1.27 1.27)) (justify right) hide)
    )
    (property "ki_keywords" "IQRF data controlled transceiver, PCB antenna, thermometer, FSK modulation" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "IQRF data controlled transceiver with PCB antenna and thermometer, FSK modulation" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "IQRF?TRx2DA?KON?SIM?01*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "TR-52DAT" (extends "TR-52DA")
    (property "Reference" "U" (at -25.4 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TR-52DAT" (at 25.4 11.43 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "RF_Module:IQRF_TRx2DA_KON-SIM-01" (at -25.4 -11.43 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "https://iqrf.org/weben/downloads.php?id=213" (at 25.4 -13.97 0)
      (effects (font (size 1.27 1.27)) (justify right) hide)
    )
    (property "ki_keywords" "IQRF common transceiver, PCB antenna, thermometer, FSK modulation" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "IQRF common transceiver with PCB antenna and thermometer, FSK modulation" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "IQRF?TRx2DA?KON?SIM?01*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "TR-72DA" (extends "TR-52DA")
    (property "Reference" "U" (at -25.4 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TR-72DA" (at 25.4 11.43 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "RF_Module:IQRF_TRx2DA_KON-SIM-01" (at -25.4 -11.43 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "https://iqrf.org/weben/downloads.php?id=337" (at 25.4 -13.97 0)
      (effects (font (size 1.27 1.27)) (justify right) hide)
    )
    (property "ki_keywords" "IQRF transceiver, PCB antenna, GMSK modulation" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "IQRF transceiver with PCB antenna, GMSK modulation" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "IQRF?TRx2DA?KON?SIM?01*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "TR-72DAT" (extends "TR-52DA")
    (property "Reference" "U" (at -25.4 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TR-72DAT" (at 25.4 11.43 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "RF_Module:IQRF_TRx2DA_KON-SIM-01" (at -25.4 -11.43 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "https://iqrf.org/weben/downloads.php?id=337" (at 25.4 -13.97 0)
      (effects (font (size 1.27 1.27)) (justify right) hide)
    )
    (property "ki_keywords" "IQRF transceiver, PCB antenna, thermometer, GMSK modulation" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "IQRF transceiver with PCB antenna and thermometer, GMSK modulation" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "IQRF?TRx2DA?KON?SIM?01*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "iM880A" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -19.05 21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "iM880A" (at 19.05 21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at -5.08 -27.94 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.wireless-solutions.de/images/stories/downloads/Radio%20Modules/iM880A/General_Information/iM880A_Datasheet_V1_1.pdf" (at -5.08 -27.94 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IOT LoRa" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "IMST Long Range Radio Module" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "iM880A_0_1"
      (rectangle (start -20.32 20.32) (end 22.86 -20.32)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "iM880A_1_1"
      (pin power_in line (at -7.62 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 5.08 20.32 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 12.7 180) (length 2.54)
        (name "P7-IO/SPI-MISO" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 10.16 180) (length 2.54)
        (name "P8-IO/SPI-MOSI" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 7.62 180) (length 2.54)
        (name "P9-IO/SPI-CLK" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 5.08 180) (length 2.54)
        (name "P10-IO/SPI-NSS" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 22.86 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -10.16 0) (length 2.54)
        (name "RxD-IO/UART-RX" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -12.7 0) (length 2.54)
        (name "TxD-IO/UART-TX" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 10.16 0) (length 2.54)
        (name "P1-IO/JTCK/SWCLK" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 2.54 180) (length 2.54)
        (name "P11-IO" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 0 180) (length 2.54)
        (name "P12-IO/I2C-SCL" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -2.54 180) (length 2.54)
        (name "P13-IO/I2C-SDA" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -5.08 180) (length 2.54)
        (name "P14-IO/ADC" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -7.62 180) (length 2.54)
        (name "P15-IO/WKUP" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 15.24 0) (length 2.54)
        (name "BOOT" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 20.32 270) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -10.16 180) (length 2.54)
        (name "P17-IO/ADC" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 7.62 0) (length 2.54)
        (name "P2-IO/JTMS/SWDIO" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -15.24 180) (length 2.54)
        (name "RF" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 5.08 0) (length 2.54)
        (name "P3-IO/JTDO" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 2.54 0) (length 2.54)
        (name "P4-IO/JTDI" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 0 0) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -5.08 0) (length 2.54)
        (name "P5-IO/UART-CTS" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -7.62 0) (length 2.54)
        (name "P6-IO/UART-RTS" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "iM880B" (extends "iM880A")
    (property "Reference" "U" (at -19.05 21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "iM880B" (at 19.05 21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at -5.08 -27.94 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.wireless-solutions.de/images/stories/downloads/Radio%20Modules/iM880B/General_Information/iM880B_Datasheet_V1_0.pdf" (at -5.08 -27.94 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IOT LoRa" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "IMST Long Range Radio Module - LoRa Alliance Certified" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
)
