(footprint "TestPoint_D2.5mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "SMD pad as test Point, diameter 2.5mm")
  (tags "test point SMD pad")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -2.148) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0fecc0bc-9640-4f76-b6ab-04e23f80de41)
  )
  (fp_text value "TestPoint_D2.5mm" (at 0 2.25) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 138e56ca-7edb-48aa-9dba-af65820d711f)
  )
  (fp_text user "${REFERENCE}" (at 0 -2.15) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 813fbb69-c107-4125-bc8e-882f78863ff8)
  )
  (fp_circle (center 0 0) (end 0 1.45)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 688e12e1-e110-4abc-a9a5-a7de881eb903))
  (fp_circle (center 0 0) (end 1.75 0)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 9a309fad-1502-4f82-86b3-5ad73f81edf1))
  (pad "1" smd circle (at 0 0) (size 2.5 2.5) (layers "F.Cu" "F.Mask") (tstamp 197dbe30-be8e-4a1d-bec3-2484ff4b9b67))
)
