(footprint "ESP32-C3_SuperMini_wide"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "ESP32 C3 Super Mini")
	(tags "ESP32 C3")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "cee1dcb7-49d6-47bf-afb1-c5247cf191bf")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "ESP32-C3_SuperMini_wide"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b699cd6c-c89b-47f3-ace3-24c02047a611")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Alexander Footprint Library:ESP32-C3_SuperMini"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6f412b33-4d27-4658-9f7e-6d4eb7572bd6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0c4ada2c-e3c2-48fb-841a-1685ffc1aa17")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "ESP32 C3 Super Mini"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6521eb37-600e-4181-a5c2-ca9bf5df9738")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a6afda93-6dfa-4e1c-8d97-7ebeb08412d1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at 0 -20.32)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0)
		(chamfer_ratio 0.25)
		(chamfer top_left bottom_left)
		(uuid "252cede5-90f2-40ba-bca6-80df6d8b32ea")
	)
	(pad "2" thru_hole roundrect
		(at 0 -17.78)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "7e7e3350-9da2-4ff2-b54a-ddfd36440959")
	)
	(pad "3" thru_hole roundrect
		(at 0 -15.24)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "38e17834-b199-4941-8e83-2e1c25a0415d")
	)
	(pad "4" thru_hole roundrect
		(at 0 -12.7)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "65aea9e7-5fa2-450b-b7da-93f23cbf35c4")
	)
	(pad "5" thru_hole roundrect
		(at 0 -10.16)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "5339b229-d3c9-4db8-946d-cb39d6052073")
	)
	(pad "6" thru_hole roundrect
		(at 0 -7.62)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "003ca421-48da-495a-8228-c662e837bbe6")
	)
	(pad "7" thru_hole roundrect
		(at 0 -5.08)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "18e0aa4f-ae48-4891-8813-df4b1f29afec")
	)
	(pad "8" thru_hole roundrect
		(at 0 -2.54)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "747ebc4b-c6b6-43b1-b72c-b9b076ed7fe8")
	)
	(pad "9" thru_hole roundrect
		(at 15.24 -2.54 180)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "28529b75-5904-4f56-ac4c-87987c46f0b4")
	)
	(pad "10" thru_hole roundrect
		(at 15.24 -5.08 180)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "3e94f39b-ca4a-4580-bcac-908e237e435b")
	)
	(pad "11" thru_hole roundrect
		(at 15.24 -7.62 180)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "26133158-e0fe-4a23-8cde-a1b104c76ccf")
	)
	(pad "12" thru_hole roundrect
		(at 15.24 -10.16 180)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "ced87b75-2068-4b4a-b15d-bc76927e13ea")
	)
	(pad "13" thru_hole roundrect
		(at 15.24 -12.7 180)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "15f23942-e2ef-4aba-8a3e-0a6ef14a58c8")
	)
	(pad "14" thru_hole roundrect
		(at 15.24 -15.24 180)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "df2ac79d-56ce-4de3-91fd-b4a3c86b8073")
	)
	(pad "15" thru_hole rect
		(at 15.24 -17.78 180)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8f245a9e-e90d-46da-a660-280713b711e8")
	)
	(pad "16" thru_hole roundrect
		(at 15.24 -20.32 180)
		(size 4.25 1.7)
		(drill 1
			(offset -1.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
		(uuid "e507832b-4ac6-4b32-bf73-e0e41fa95fc2")
	)
)
