(footprint "Conn_Probe"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
	(tags "Through hole pin header THT 1x01 2.54mm single row")
	(property "Reference" "DBG**"
		(at 0 -4 0)
		(layer "F.SilkS")
		(uuid "6c50d304-4606-47dc-966e-5ce9cce54912")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Conn_Probe"
		(at 0 2.33 0)
		(layer "F.Fab")
		(uuid "86a9f2cd-c84c-4f67-881e-c331171fcf5a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f533db6b-d87a-483d-8669-171e932359e2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "79edd7bb-ff18-468b-a74c-de472aa41331")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a34fbf3c-c5d6-441f-ab34-787ec4073ba2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "6976de06-a21f-4558-b5c2-96b2fac0f546")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd oval
		(at 0 0)
		(size 5 3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "bf29d5b2-1ed9-48cf-a932-2258e5e431d0")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
