(footprint "XCVR_ESP32-S3-WROOM-2-N32R8V"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -6.575 -14.135 0)
		(layer "F.SilkS")
		(uuid "70dccb18-c93a-4151-985f-c8db3ebcdb43")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "XCVR_ESP32-S3-WROOM-2-N32R8V"
		(at 8.03 14.365 0)
		(layer "F.Fab")
		(uuid "be19edfa-a5d3-4edc-80b2-e5781e27506d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8ee5fc58-d3f9-439b-9750-9836e9fdb28f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b1e991f7-0ea4-49ea-8c90-0e56f3eee24e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "4cefa354-3033-4b8f-974b-36bd65264a5c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -9 -12.75)
		(end 9 -12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f4b8ac41-d4a1-4730-b87e-67abfce3d2dd")
	)
	(fp_line
		(start -9 -6.03)
		(end -9 -12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c61c1cf7-7b5f-4e5b-aa8a-9f38af8252b5")
	)
	(fp_line
		(start -9 12.02)
		(end -9 12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b71fa52e-faae-4da7-9d31-065d910ff454")
	)
	(fp_line
		(start -9 12.75)
		(end -7.755 12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "aaabc694-a9d4-4447-9f0f-5f74f934350e")
	)
	(fp_line
		(start 9 -12.75)
		(end 9 -6.03)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0ecbcbd9-6bf7-428f-8fcd-eb387ff3efcd")
	)
	(fp_line
		(start 9 12.02)
		(end 9 12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ecdd80f2-627f-44c4-9366-03838bcbed98")
	)
	(fp_line
		(start 9 12.75)
		(end 7.755 12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1187b47a-51b6-40da-becd-d576402a7e12")
	)
	(fp_circle
		(center -10.2 -5.26)
		(end -10.1 -5.26)
		(stroke
			(width 0.2)
			(type solid)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "72d1eab7-cf92-4a2e-8568-294027a868f6")
	)
	(fp_line
		(start -9.75 -13)
		(end 9.75 -13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "35bf6783-0ba2-4242-9bba-89db8a923a26")
	)
	(fp_line
		(start -9.75 13.5)
		(end -9.75 -13)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8d6a6467-a6ab-4627-8dd7-37af86fc102b")
	)
	(fp_line
		(start -9.75 13.5)
		(end 9.75 13.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "da3bf799-45fe-4a1b-ae03-d1516a17bc81")
	)
	(fp_line
		(start 9.75 -13)
		(end 9.75 13.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "679a9ac4-f584-4258-bd71-4fbf0d2cc2b5")
	)
	(fp_line
		(start -9 -12.75)
		(end 9 -12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b087dd86-c9cc-4fcb-b503-e7b3b4af7d44")
	)
	(fp_line
		(start -9 -6.75)
		(end -9 -12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f80a9c93-c17b-4613-ad01-233521823940")
	)
	(fp_line
		(start -9 -6.75)
		(end 9 -6.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e5ae43b2-b0bd-462e-a3eb-7deb03f7c3fd")
	)
	(fp_line
		(start -9 12.75)
		(end -9 -6.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "17995ced-24a0-429a-bb5e-b503df5b0abb")
	)
	(fp_line
		(start 9 -12.75)
		(end 9 -6.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "32cc6206-91ad-4518-8bd6-896d65b457d5")
	)
	(fp_line
		(start 9 -6.75)
		(end 9 12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "af4049b5-e857-4301-b21e-4623082b5fe4")
	)
	(fp_line
		(start 9 12.75)
		(end -9 12.75)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b48f997c-d6c5-477e-99f3-19b5f671ef6d")
	)
	(fp_circle
		(center -10.2 -5.26)
		(end -10.1 -5.26)
		(stroke
			(width 0.2)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "599b1cf8-2aca-49aa-9f05-874e8c3714cf")
	)
	(fp_text user "ANTENNA"
		(at -4.5 -9.5 0)
		(layer "F.Fab")
		(uuid "0cfa8efe-d21a-4dd6-9bad-70bf807683c0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -8.75 -5.26)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "23cc5470-2af6-4653-b81e-832a96b4d738")
	)
	(pad "2" smd rect
		(at -8.75 -3.99)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "054ee04f-d1f5-4f48-99e5-3dfa431004b2")
	)
	(pad "3" smd rect
		(at -8.75 -2.72)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "646bd8fe-76f0-4bf9-914b-8ede2af18e34")
	)
	(pad "4" smd rect
		(at -8.75 -1.45)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "59609f5b-2a6c-45c6-8fb3-e04494c5ea67")
	)
	(pad "5" smd rect
		(at -8.75 -0.18)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "e728c4e4-7977-4326-8775-2f34d158d462")
	)
	(pad "6" smd rect
		(at -8.75 1.09)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "2df3f2d8-9e91-458b-9428-6d256a741ee2")
	)
	(pad "7" smd rect
		(at -8.75 2.36)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "e88c83aa-44f3-4f8d-9dc6-f195d6355d0f")
	)
	(pad "8" smd rect
		(at -8.75 3.63)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "573990ca-8bdc-4d2f-9f67-d95afbcaa3bb")
	)
	(pad "9" smd rect
		(at -8.75 4.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "1282bcb5-e5cf-4981-abe2-04e84c1b93c9")
	)
	(pad "10" smd rect
		(at -8.75 6.17)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "56c0245d-0622-4faf-a24a-f667607bf151")
	)
	(pad "11" smd rect
		(at -8.75 7.44)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "ee168327-369a-49bf-9398-717764dcff68")
	)
	(pad "12" smd rect
		(at -8.75 8.71)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "c5c54b92-bf37-45af-8641-d850041028f8")
	)
	(pad "13" smd rect
		(at -8.75 9.98)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "186b262d-2281-42e2-8aa1-25d5ff6df839")
	)
	(pad "14" smd rect
		(at -8.75 11.25)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "d692aafc-7227-4968-a69f-e95c9d494167")
	)
	(pad "15" smd rect
		(at -6.985 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "6785f087-92b0-4060-860d-700e3975e4e3")
	)
	(pad "16" smd rect
		(at -5.715 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "ff3f1e17-fe38-476d-8093-c02c75993531")
	)
	(pad "17" smd rect
		(at -4.445 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "df07325d-06de-418c-a2ed-46b6c26e5213")
	)
	(pad "18" smd rect
		(at -3.175 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "7b378ad0-abf2-45e2-a134-f224d6af372f")
	)
	(pad "19" smd rect
		(at -1.905 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "50bb043c-147d-450b-82df-75126171b58e")
	)
	(pad "20" smd rect
		(at -0.635 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "dd3446ee-d78f-4394-a9bd-91edd337f9a2")
	)
	(pad "21" smd rect
		(at 0.635 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "1130649d-9901-4933-a79b-26e6a902cfa8")
	)
	(pad "22" smd rect
		(at 1.905 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "120f1ccd-7cf3-4ae8-9a57-2f1fcea20b6c")
	)
	(pad "23" smd rect
		(at 3.175 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "05281858-5027-42aa-91f0-0b8253c3f3b1")
	)
	(pad "24" smd rect
		(at 4.445 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "d6b96b8e-e2c5-4f2a-a716-705b44f12e8e")
	)
	(pad "25" smd rect
		(at 5.715 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "59d0888a-4a9a-40dd-bfc4-c52bce40e5a6")
	)
	(pad "26" smd rect
		(at 6.985 12.5)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "3104514e-8709-4d3e-95a5-ad88a9606788")
	)
	(pad "27" smd rect
		(at 8.75 11.25)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "3bd6191c-aea9-40c5-ba01-ebf9270f390f")
	)
	(pad "28" smd rect
		(at 8.75 9.98)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "50ba01d1-bd83-4b19-b2b3-d43340050bbd")
	)
	(pad "29" smd rect
		(at 8.75 8.71)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "1cb39055-5805-4396-bf18-29b4a05ac03a")
	)
	(pad "30" smd rect
		(at 8.75 7.44)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "61d4f689-c59d-4937-9754-aa9933c9169c")
	)
	(pad "31" smd rect
		(at 8.75 6.17)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "6706bce8-fa64-4911-9893-b35f7e6359cd")
	)
	(pad "32" smd rect
		(at 8.75 4.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "9dded6fa-39d7-4c98-933d-2fd4361388ea")
	)
	(pad "33" smd rect
		(at 8.75 3.63)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "ea077fec-fc30-431a-b0e4-d895c5212617")
	)
	(pad "34" smd rect
		(at 8.75 2.36)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "0047d992-264e-4fc1-ae6d-6d8b7a1c4cae")
	)
	(pad "35" smd rect
		(at 8.75 1.09)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "ea642b7b-eeb3-4930-934a-0c2eeaff46b6")
	)
	(pad "36" smd rect
		(at 8.75 -0.18)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "ecfa3eb1-33a8-4a8c-9ec1-7d5cfc216ed8")
	)
	(pad "37" smd rect
		(at 8.75 -1.45)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "dd4a57bf-75df-4ae3-bd23-61a45f999e9c")
	)
	(pad "38" smd rect
		(at 8.75 -2.72)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "ce26a329-58b4-48f2-9072-e7688f1bb54d")
	)
	(pad "39" smd rect
		(at 8.75 -3.99)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "e290ea5f-be10-45d1-9626-2dc9d19967cf")
	)
	(pad "40" smd rect
		(at 8.75 -5.26)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "badcea0d-1c0a-4581-88b7-57007b230c53")
	)
	(pad "41_1" smd rect
		(at -1.36 0.09)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "6958e0f2-3750-4818-aa3d-a3996e495a2b")
	)
	(pad "41_2" smd rect
		(at -2.86 0.09)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "5fad87f9-6d3d-4569-868e-d156be6d47f3")
	)
	(pad "41_3" smd rect
		(at 0.14 0.09)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "4681ec89-d623-4045-a95a-47ed30145bae")
	)
	(pad "41_4" smd rect
		(at -2.86 1.59)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "39ea0cc1-d59d-4912-9aed-0d4f34b62c8f")
	)
	(pad "41_5" smd rect
		(at -1.36 1.59)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "e7b3eafd-8ca9-44c2-b8f7-44cb1af0fdb3")
	)
	(pad "41_6" smd rect
		(at 0.14 1.59)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "0e0ceb86-fd45-4ef4-81c1-e46adf7481b6")
	)
	(pad "41_7" smd rect
		(at -2.86 -1.41)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "ede06980-cec2-4314-9374-14d014187f01")
	)
	(pad "41_8" smd rect
		(at -1.36 -1.41)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "e9e411ee-6514-46c9-a484-d10fa35c1f4e")
	)
	(pad "41_9" smd rect
		(at 0.14 -1.41)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "10b3a84f-3871-452c-8b33-eae77ff269dd")
	)
	(pad "41_10" thru_hole circle
		(at -1.36 -0.66)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "c73a4e38-a010-4539-9282-051ec51e549d")
	)
	(pad "41_11" thru_hole circle
		(at -2.86 -0.66)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "72f31940-6339-4880-af42-62234474dc05")
	)
	(pad "41_12" thru_hole circle
		(at 0.14 -0.66)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "b6a67b1b-fd1d-42ac-99c3-c024e95dbb86")
	)
	(pad "41_13" thru_hole circle
		(at -2.86 0.84)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "650e8074-3a1b-42c1-932a-aa83e5d33ab0")
	)
	(pad "41_14" thru_hole circle
		(at -1.36 0.84)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "e8c850b7-a6f9-4447-9c1c-f565817b1dcb")
	)
	(pad "41_15" thru_hole circle
		(at 0.14 0.84)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "3ea0b839-1790-4466-b0a4-1f001b37874e")
	)
	(pad "41_16" thru_hole circle
		(at -2.11 -1.41)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "78921b6f-8120-47b9-b355-714f413076e5")
	)
	(pad "41_17" thru_hole circle
		(at -0.61 -1.41)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "2151de9b-58d7-4090-b308-1255cf64dd45")
	)
	(pad "41_18" thru_hole circle
		(at -2.11 0.09)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "2404b10e-cfb2-4a1d-875d-0c52c1e20813")
	)
	(pad "41_19" thru_hole circle
		(at -0.61 0.09)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "3d1faa00-df4c-4e4f-b6db-4ddd171f2583")
	)
	(pad "41_20" thru_hole circle
		(at -2.11 1.59)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "c8ddaa47-c3ab-4ab0-9261-166c6b3b1bbc")
	)
	(pad "41_21" thru_hole circle
		(at -0.61 1.59)
		(size 0.3 0.3)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "5433d672-90db-4e30-a3bf-4765f380122b")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "1d6f16d9-4e74-4bb2-b892-44c43d7f8cd4")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9 -12.75) (xy 9 -12.75) (xy 9 -6.75) (xy -9 -6.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu")
		(uuid "4a07c2f7-0bc9-4265-a707-4b3bd7883fd0")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9 -12.75) (xy 9 -12.75) (xy 9 -6.75) (xy -9 -6.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(uuid "effff455-e044-4949-80a4-b7aa3fec5ce2")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9 -12.75) (xy 9 -12.75) (xy 9 -6.75) (xy -9 -6.75)
			)
		)
	)
)
