(module "ESP32C3WROOM02H4" (layer F.Cu)
  (descr "ESP32-C3-WROOM-02-H4-3")
  (tags "Integrated Circuit")
  (attr smd)
  (fp_text reference IC** (at 9.500 -10) (layer F.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text user %R (at 9.500 -10) (layer F.Fab)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text value "ESP32C3WROOM02H4" (at 9.500 -10) (layer F.SilkS) hide
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_line (start 0.5 -0) (end 18.5 -0) (layer F.Fab) (width 0.1))
  (fp_line (start 18.5 -0) (end 18.5 -20) (layer F.Fab) (width 0.1))
  (fp_line (start 18.5 -20) (end 0.5 -20) (layer F.Fab) (width 0.1))
  (fp_line (start 0.5 -20) (end 0.5 -0) (layer F.Fab) (width 0.1))
  (fp_line (start -1 -21) (end 20 -21) (layer F.CrtYd) (width 0.1))
  (fp_line (start 20 -21) (end 20 1) (layer F.CrtYd) (width 0.1))
  (fp_line (start 20 1) (end -1 1) (layer F.CrtYd) (width 0.1))
  (fp_line (start -1 1) (end -1 -21) (layer F.CrtYd) (width 0.1))
  (fp_line (start 0.5 -14) (end 0.5 -20) (layer F.SilkS) (width 0.2))
  (fp_line (start 0.5 -20) (end 18.5 -20) (layer F.SilkS) (width 0.2))
  (fp_line (start 18.5 -20) (end 18.5 -14) (layer F.SilkS) (width 0.2))
  (fp_line (start 2.5 -0) (end 16.5 -0) (layer F.SilkS) (width 0.2))
  (fp_line (start -0.5 -12.8) (end -0.5 -12.8) (layer F.SilkS) (width 0.1))
  (fp_line (start -0.5 -12.9) (end -0.5 -12.9) (layer F.SilkS) (width 0.1))
  (fp_arc (start -0.5 -12.85) (end -0.500 -12.8) (angle -180) (layer F.SilkS) (width 0.1))
  (fp_arc (start -0.5 -12.85) (end -0.500 -12.9) (angle -180) (layer F.SilkS) (width 0.1))
  (pad 1 smd rect (at 0.750 -12.9 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.750 -11.4 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.750 -9.9 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.750 -8.4 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.750 -6.9 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.750 -5.4 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.750 -3.9 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.750 -2.4 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0.750 -0.9 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 18.250 -0.9 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 18.250 -2.4 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 18.250 -3.9 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 18.250 -5.4 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 18.250 -6.9 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 18.250 -8.4 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 18.250 -9.9 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 18.250 -11.4 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 18.250 -12.9 90) (size 0.900 1.500) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 10.460 -6.7 90) (size 0.700 0.700) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 11.560 -6.7 90) (size 0.700 0.700) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 11.560 -7.8 90) (size 0.700 0.700) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 10.460 -7.8 90) (size 0.700 0.700) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 9.360 -7.8 90) (size 0.700 0.700) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 9.360 -6.7 90) (size 0.700 0.700) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 9.360 -5.6 90) (size 0.700 0.700) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 10.460 -5.6 90) (size 0.700 0.700) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 11.560 -5.6 90) (size 0.700 0.700) (layers F.Cu F.Paste F.Mask))
  (model ESP32-C3-WROOM-02-H4.stp
    (at (xyz 0.3740157480315 0.39370078740157 0.015748031730727))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
