(footprint "Relay_DPDT_HK19F_HUI"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Relay DPDT Schrack-RT2 RM5mm 16A 250V AC Form C http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=RT2_reflow&DocType=DS&DocLang=EN")
	(tags "Relay DPDT Schrack-RT2 RM5mm 16A 250V AC Relay")
	(property "Reference" "REF**"
		(at 12.5 -11.5 0)
		(layer "F.SilkS")
		(uuid "813d7e13-7bff-41ea-b056-5110e7ab1705")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Relay_DPDT_HK19F_HUI"
		(at 12.192 4.25 0)
		(layer "F.Fab")
		(uuid "60f6a6c4-122e-4e19-abf8-f3e9d61e2d5a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8747c589-d12e-4f54-bd80-66e15795b691")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2744d742-ad2c-4539-b4ae-934a1b60bb7e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0463430f-c3a7-4acd-b971-374a39375e11")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -2.75 1.5)
		(end -2.75 3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7c129a95-8668-4500-af1d-6c546ac568da")
	)
	(fp_line
		(start -2.75 3)
		(end -1.25 3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c42b0bac-c2e8-4969-8dc4-a267d1bc99cb")
	)
	(fp_line
		(start -2.55 -10.3)
		(end -2.55 2.8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5d93f9db-8a24-43df-a43d-59d096034ee0")
	)
	(fp_line
		(start -2.55 2.8)
		(end 19.7 2.8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "23ee4cfb-b28a-4f49-b1ca-30ab4814ed16")
	)
	(fp_line
		(start 2.54 -6.35)
		(end 2.54 -1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7aca6006-33e2-4102-a301-60c09a0b1406")
	)
	(fp_line
		(start 2.54 -2.54)
		(end 5.08 -3.81)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "001e8759-94ed-4b26-9688-9bbd87340b35")
	)
	(fp_line
		(start 2.54 -1.27)
		(end 3.81 -1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "989b5995-4923-4388-adf1-cc3625e3567b")
	)
	(fp_line
		(start 2.54 0)
		(end 3.81 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fb844c18-6e1b-4bdb-8d56-2c14bdec4c39")
	)
	(fp_line
		(start 3.81 -7.62)
		(end 2.54 -7.62)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "85e3c49f-facf-4fde-be0d-eafe86876f69")
	)
	(fp_line
		(start 3.81 -6.35)
		(end 3.81 -7.62)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ac5ee7bc-2039-4889-8f0a-2d0dfa75f850")
	)
	(fp_line
		(start 3.81 -1.27)
		(end 5.08 -1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8593ea91-da8e-4c8b-81c4-067f66437a1b")
	)
	(fp_line
		(start 3.81 0)
		(end 3.81 -1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c46f0368-487a-4c89-aba8-01176f8978d5")
	)
	(fp_line
		(start 5.08 -6.35)
		(end 2.54 -6.35)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c8134d10-172d-42a3-9f6e-cdf83173e2a8")
	)
	(fp_line
		(start 5.08 -1.27)
		(end 5.08 -6.35)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a15f10cb-bd9a-4201-b4eb-511fa13ec67e")
	)
	(fp_line
		(start 19.7 -10.3)
		(end -2.55 -10.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "81eef702-14a4-4a18-b249-38ec85adf04e")
	)
	(fp_line
		(start 19.7 2.8)
		(end 19.7 -10.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8b4b2a12-b280-405a-a846-7a7eb4d0286f")
	)
	(fp_line
		(start -2.8 -10.55)
		(end -2.8 3.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c4806428-07d2-4326-b0bf-1b5edb04ea64")
	)
	(fp_line
		(start -2.8 3.05)
		(end 19.9 3.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1d9532f3-65ad-4c77-a793-b27ee265206d")
	)
	(fp_line
		(start 19.9 -10.5)
		(end -2.8 -10.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a65c830f-ba15-4419-960c-3bac454ec7f2")
	)
	(fp_line
		(start 19.9 3.05)
		(end 19.9 -10.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1f9daffe-683a-47d1-8d0e-85119e1da8d0")
	)
	(fp_line
		(start -2.35 -10.1)
		(end -2.35 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b3934dbe-2888-4513-96b7-f9d111bfcd7b")
	)
	(fp_line
		(start -2.35 1.6)
		(end -1.35 2.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "353f6fbe-d49d-4143-b3d3-a4c2e85d8ae6")
	)
	(fp_line
		(start -1.35 2.6)
		(end 19.5 2.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "110c6cfc-ab50-4d57-ae5b-45155ac41ded")
	)
	(fp_line
		(start 0 -1.27)
		(end 0 -6.35)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0001174f-3b09-436e-b5f5-c470ed6e56ac")
	)
	(fp_line
		(start 19.5 -10.1)
		(end -2.35 -10.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e9efb4d1-08f0-49ac-ac05-851799bcba76")
	)
	(fp_line
		(start 19.5 2.6)
		(end 19.5 -10.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "864effa7-8efb-4333-880c-f9b8b3a507e2")
	)
	(fp_text user "${REFERENCE}"
		(at 12.065 -3.81 180)
		(layer "F.Fab")
		(uuid "09213bde-ad66-4f73-b5f5-3b9dac1c6c13")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "11" thru_hole oval
		(at 12.7 0 180)
		(size 2 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "63e394e7-8f62-4c9b-9c68-d0cc5eb3668a")
	)
	(pad "12" thru_hole oval
		(at 7.62 0 180)
		(size 2 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "62245da5-e3c7-4b5b-bbb4-164555e9887d")
	)
	(pad "14" thru_hole oval
		(at 17.78 0 180)
		(size 2 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b05a3acf-82f4-4cfb-b798-81940a411385")
	)
	(pad "21" thru_hole oval
		(at 12.7 -7.5 180)
		(size 2 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c5037696-0ad1-4c1e-a57c-a45d637f7562")
	)
	(pad "22" thru_hole oval
		(at 7.62 -7.5 180)
		(size 2 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "38c07c23-af31-4012-b2f4-aa5fa10a84ba")
	)
	(pad "24" thru_hole oval
		(at 17.78 -7.5 180)
		(size 2 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fef5d445-4686-40c1-ab41-1e25c3abf74e")
	)
	(pad "A1" thru_hole rect
		(at 0 0 180)
		(size 3 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c8d04df5-0d6d-486e-aa84-3097897afbf9")
	)
	(pad "A2" thru_hole oval
		(at 0 -7.62 180)
		(size 3 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ee0acf75-94f1-4711-b515-8706c4b7cdbf")
	)
	(model "${KICAD8_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_DPDT_Schrack-RT2-FormC_RM5mm.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
