(footprint "AMS1117 SOT-223"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "module CMS SOT223 4 pins")
	(tags "CMS SOT")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
		(uuid "4497a1e1-94b1-4cba-abfc-02d82a04371f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "AMS1117 SOT-223"
		(at 0 5.08 0)
		(layer "F.Fab")
		(uuid "222a057b-4f1f-481e-81c0-82276f6e2fbf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4abea311-3d5c-46ae-a6f7-53ad7d401202")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cf35375b-a35a-4ccf-b401-52356d4eb3ab")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e0b857b7-85f4-442e-9375-43b7f0b65024")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.85 -3.41)
		(end 1.91 -3.41)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "10341b74-de1d-44f8-b919-9dc7b01c77a6")
	)
	(fp_line
		(start -1.85 3.41)
		(end 1.91 3.41)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9eaaee9c-d787-4c4e-9409-486f5d803253")
	)
	(fp_line
		(start 1.91 -3.41)
		(end 1.91 -2.15)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "668bbda1-c7e1-4e23-9d62-dd4d052018b0")
	)
	(fp_line
		(start 1.91 3.41)
		(end 1.91 2.15)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7b7161b8-bc72-4822-9d67-8c4bc120433f")
	)
	(fp_poly
		(pts
			(xy -3.13 -3.31) (xy -3.37 -3.64) (xy -2.89 -3.64) (xy -3.13 -3.31)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "818bd365-7a79-40a2-b037-dacc75b8af05")
	)
	(fp_line
		(start -4.4 -3.6)
		(end -4.4 3.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1e6e1c3c-cf2e-4570-9270-1e4425f802c5")
	)
	(fp_line
		(start -4.4 3.6)
		(end 4.4 3.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fe006c7f-e9e9-42b8-94e6-7fab62e45a96")
	)
	(fp_line
		(start 4.4 -3.6)
		(end -4.4 -3.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "18a70f3a-ba6f-445d-a1d1-b2229acce0b4")
	)
	(fp_line
		(start 4.4 3.6)
		(end 4.4 -3.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1cb64177-a033-440a-bc55-482358e05d6e")
	)
	(fp_line
		(start -1.85 -2.3)
		(end -1.85 3.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2a9ca989-6b38-468d-a714-75a033988b2c")
	)
	(fp_line
		(start -1.85 -2.3)
		(end -0.8 -3.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "bcb7341f-c5b7-4cf0-ac84-66c574c5e61c")
	)
	(fp_line
		(start -1.85 3.35)
		(end 1.85 3.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c011dc66-40ad-4f1e-a34f-e251dae0cd31")
	)
	(fp_line
		(start -0.8 -3.35)
		(end 1.85 -3.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "80711826-0dce-449b-af78-388864936159")
	)
	(fp_line
		(start 1.85 -3.35)
		(end 1.85 3.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a66ee799-671f-4902-ac92-f94d39f82acf")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "184c46b5-a004-48e0-8f63-d7d63dc324be")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.12)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.15 -2.3)
		(size 2 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "ea891fee-0855-44cc-8da9-0c7b9e3b1505")
	)
	(pad "2" smd roundrect
		(at -3.15 0)
		(size 2 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "2adbaf0f-7617-4618-9438-78a8bd4ec4b2")
	)
	(pad "3" smd roundrect
		(at -3.15 2.3)
		(size 2 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "1b42a1a5-e735-42f2-b87a-1df5a461081d")
	)
	(pad "4" smd roundrect
		(at 3.15 0)
		(size 2 3.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "023f2cc5-97fb-4421-8e37-e8aa385789b4")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
