(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (title_block
    (title "Arduino UNO R4 Shield Template PCB")
    (date "2023-07-13")
    (rev "1.0")
    (company "MStackoverflow")
  )

  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "unconnected-(U1-Pad1)")
  (net 2 "unconnected-(U1-Pad2)")
  (net 3 "unconnected-(U1-Pad3)")
  (net 4 "unconnected-(U2-Pad1)")
  (net 5 "unconnected-(U2-Pad2)")
  (net 6 "unconnected-(U2-Pad3)")
  (net 7 "unconnected-(U2-Pad4)")
  (net 8 "unconnected-(U2-Pad5)")
  (net 9 "unconnected-(U2-Pad6)")
  (net 10 "unconnected-(U2-Pad7)")
  (net 11 "unconnected-(U2-Pad8)")
  (net 12 "unconnected-(U4-Pad1)")
  (net 13 "unconnected-(U4-Pad2)")
  (net 14 "unconnected-(U4-Pad3)")
  (net 15 "unconnected-(U4-Pad4)")
  (net 16 "unconnected-(U4-Pad5)")
  (net 17 "unconnected-(U4-Pad6)")
  (net 18 "unconnected-(U5-Pad1)")
  (net 19 "unconnected-(U5-Pad2)")
  (net 20 "unconnected-(U5-Pad3)")
  (net 21 "unconnected-(U5-Pad4)")
  (net 22 "unconnected-(U5-Pad5)")
  (net 23 "unconnected-(U5-Pad6)")
  (net 24 "unconnected-(U6-Pad1)")
  (net 25 "unconnected-(U6-Pad2)")
  (net 26 "unconnected-(U6-Pad3)")
  (net 27 "unconnected-(U6-Pad4)")
  (net 28 "unconnected-(U6-Pad5)")
  (net 29 "unconnected-(U6-Pad6)")
  (net 30 "unconnected-(U6-Pad7)")
  (net 31 "unconnected-(U6-Pad8)")
  (net 32 "unconnected-(U6-Pad9)")
  (net 33 "unconnected-(U6-Pad10)")
  (net 34 "unconnected-(U3-Pad9)")
  (net 35 "unconnected-(U3-Pad10)")
  (net 36 "unconnected-(U3-Pad11)")
  (net 37 "unconnected-(U3-Pad12)")
  (net 38 "unconnected-(U3-Pad13)")
  (net 39 "unconnected-(U3-Pad14)")
  (net 40 "unconnected-(U7-Pad11)")
  (net 41 "unconnected-(U7-Pad12)")
  (net 42 "unconnected-(U7-Pad13)")
  (net 43 "unconnected-(U7-Pad14)")
  (net 44 "unconnected-(U7-Pad15)")
  (net 45 "unconnected-(U7-Pad16)")
  (net 46 "unconnected-(U7-Pad17)")
  (net 47 "unconnected-(U7-Pad18)")

  (footprint "ArduinoPinSockets:Arduino_PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp 2e25bb07-6fac-4e4d-9564-79c97701c8c4)
    (at 124.47499 116.84001 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "ArduinoUnoR4Shield.kicad_sch")
    (property "Sheetname" "")
    (path "/728b8f65-9cc8-4172-9b61-68e59ce10e89")
    (attr through_hole)
    (fp_text reference "U1" (at 0 -2.33 90) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 12e15a02-3f7b-4911-8d9b-95b71f5e2fdd)
    )
    (fp_text value "OFF" (at 0 7.41 90) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0c49d04d-c026-4639-ba81-7c06a55964f3)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7d5a2529-5895-4188-a907-0db4ca55f516))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 86d4fc71-1a93-4458-a5cc-6c7c5eeb4016))
    (fp_line (start -1.33 1.27) (end -1.33 6.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 43c38f39-0f78-4c19-b31e-ef186ab79f9a))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 61fdfcdf-54bb-434b-bf2c-123d9c7e3a30))
    (fp_line (start -1.33 6.41) (end 1.33 6.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1b359939-4641-4289-9585-da971e906754))
    (fp_line (start 1.33 1.27) (end 1.33 6.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4d7bdbe4-872d-4f0d-857b-4ab34d1be85a))
    (fp_line (start -1.8 -1.8) (end -1.8 6.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 17eec74c-37fe-4eeb-b3ec-08f97ea71d64))
    (fp_line (start -1.8 6.85) (end 1.8 6.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1570e0e8-545b-4e85-b598-382009286eef))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 45d5aad0-01f8-43c9-a559-62bf5da311ca))
    (fp_line (start 1.8 6.85) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3b594fb8-be27-4daa-9343-c40781cba7f5))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e4ae77af-4272-45a2-9204-1c116b2617b1))
    (fp_line (start -1.27 6.35) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b9fafabc-9670-4624-9d78-2f8c30196df7))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fe7bd4e9-98fe-4bdb-90b1-c7a06d748b99))
    (fp_line (start 1.27 -1.27) (end 1.27 6.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e809c79b-ab2f-4ae8-b585-990483f687ac))
    (fp_line (start 1.27 6.35) (end -1.27 6.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 81c6cce9-3938-49a4-b306-9a11dd761249))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 1 "unconnected-(U1-Pad1)") (pinfunction "OFF") (pintype "input") (tstamp e0984b6e-738b-4051-b4de-e5f7bc48eb00))
    (pad "2" thru_hole circle (at 0 2.54 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 2 "unconnected-(U1-Pad2)") (pinfunction "GND") (pintype "power_out") (tstamp 801f4437-f07b-4975-8457-99342066ed28))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 3 "unconnected-(U1-Pad3)") (pinfunction "VRTC") (pintype "power_in") (tstamp aca35c14-f76f-4b9d-8b12-7510c61048a3))
    (model "${KIPRJMOD}/3DModels/pin header female 2.54mm_0.1in.STEP"
      (offset (xyz -1.3 1.3 8.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (footprint "ArduinoPinSockets:Arduino_PinSocket_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp 4c528a67-0deb-4c1b-8bcd-2e6dbf362cc6)
    (at 170.30199 88.91501)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "ArduinoUnoR4Shield.kicad_sch")
    (property "Sheetname" "")
    (path "/55cbeeb8-edbb-43d9-9bd4-158a7d52440b")
    (attr through_hole)
    (fp_text reference "U5" (at 1.27 -2.33) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 559dad08-80e0-4035-8118-99f8b699edaf)
    )
    (fp_text value "ICSP" (at 1.27 7.41) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0a9f37fb-2ab5-46e6-af68-d66d0e5f257a)
    )
    (fp_text user "${REFERENCE}" (at 1.27 2.54 90) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 988bbab1-7694-4bcf-b847-7709d8bd8cdc)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d7cfcd80-2355-4c13-b556-bfff0bab733d))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3f48164a-3742-42a3-8aed-c035f1907ca6))
    (fp_line (start -1.33 1.27) (end -1.33 6.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 451db443-7bf4-41c4-a379-085448fe9432))
    (fp_line (start -1.33 1.27) (end 1.27 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1cb0c9a1-faf9-4d7c-adc0-75985162d848))
    (fp_line (start -1.33 6.41) (end 3.87 6.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0956d93f-caeb-4d82-aba3-a93e696a35a2))
    (fp_line (start 1.27 -1.33) (end 3.87 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8128826a-6f71-441d-8674-5753d9284906))
    (fp_line (start 1.27 1.27) (end 1.27 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 15216508-fdda-4be6-bb70-1499508ffd9e))
    (fp_line (start 3.87 -1.33) (end 3.87 6.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2f89cb14-a3db-4e81-b8ae-7734b14ed6e9))
    (fp_line (start -1.8 -1.8) (end -1.8 6.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c5c99818-7bde-4c54-8569-4681abad4936))
    (fp_line (start -1.8 6.85) (end 4.35 6.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8cd4925e-3934-4296-b26f-d2e95a5957b5))
    (fp_line (start 4.35 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 11e9e4b7-663a-4ece-8c3c-aa7141a56a62))
    (fp_line (start 4.35 6.85) (end 4.35 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 358b7ca3-6912-4346-831d-eb95f1d7e417))
    (fp_line (start -1.27 0) (end 0 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aba7ac98-bd85-4499-b399-6c3310c6d02b))
    (fp_line (start -1.27 6.35) (end -1.27 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9692ecae-20df-4070-881a-07e7b6a12a4d))
    (fp_line (start 0 -1.27) (end 3.81 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6c6ab172-3ebf-464c-88be-949d282639cd))
    (fp_line (start 3.81 -1.27) (end 3.81 6.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 82c75146-6f8e-4293-a6cf-4b5c7363ec8c))
    (fp_line (start 3.81 6.35) (end -1.27 6.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dc7e0a19-ca7b-4f5f-a5d9-3a517228ab50))
    (pad "1" thru_hole circle (at 0 0) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(U5-Pad1)") (pinfunction "CIPO") (pintype "bidirectional") (tstamp a6c7471a-bc56-46fd-a33e-74799345a4f8))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(U5-Pad2)") (pinfunction "+5V") (pintype "power_out") (tstamp 2d0f3eb8-b3f3-459c-b7cc-341f7a084fcc))
    (pad "3" thru_hole circle (at 0 2.54) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(U5-Pad3)") (pinfunction "SCK") (pintype "bidirectional") (tstamp 0448d086-07a4-4ec9-9983-d195051271f6))
    (pad "4" thru_hole circle (at 2.54 2.54) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(U5-Pad4)") (pinfunction "COPI") (pintype "bidirectional") (tstamp 89fe3f60-509a-4023-b5cf-1bb62435bb88))
    (pad "5" thru_hole circle (at 0 5.08) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(U5-Pad5)") (pinfunction "RESET") (pintype "bidirectional") (tstamp 784fcb3e-9557-48d8-8dfe-c85dfe366a91))
    (pad "6" thru_hole circle (at 2.54 5.08) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(U5-Pad6)") (pinfunction "GND") (pintype "power_out") (tstamp 766ea295-e3af-47e5-82ea-76f6a2820d55))
    (model "${KIPRJMOD}/3DModels/pin header female 2.54mm_0.1in.STEP"
      (offset (xyz 1.3 1.3 -10))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -180 0))
    )
    (model "${KIPRJMOD}/3DModels/pin header female 2.54mm_0.1in.STEP"
      (offset (xyz 3.7 1.3 -10))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -180 0))
    )
  )

  (footprint "ArduinoMountingHoles:Arduino_MountingHole" (layer "F.Cu")
    (tstamp 86a3863f-0b7c-4a53-a70e-ba6164ac93a8)
    (at 172.72 83.82001)
    (property "Sheetfile" "ArduinoUnoR4Shield.kicad_sch")
    (property "Sheetname" "")
    (path "/cc690ef5-5ef2-4aa9-a8a8-2029c773ee17")
    (attr smd)
    (fp_text reference "H1" (at 0 -6.81 unlocked) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 867f78ac-e981-4553-b42d-36931958a447)
    )
    (fp_text value "MountingHole1" (at 0 -5.31 unlocked) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 405e5c24-e877-4a15-8178-ed013fee8f96)
    )
    (fp_text user "${REFERENCE}" (at 0 -3.81 unlocked) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0c752e04-b17e-4224-91e5-7141776a7a16)
    )
    (pad "" np_thru_hole circle (at 0 0) (size 3.19989 3.19989) (drill 3.19989) (layers "F&B.Cu" "*.Mask")
      (solder_mask_margin 0.5) (tstamp 1c26687a-fc0a-4400-96d3-23eb5fa5d891))
  )

  (footprint "ArduinoPinSockets:Arduino_PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp a880aa38-9cfb-49bf-89a8-ea9261606aa1)
    (at 152.39999 68.58001 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "ArduinoUnoR4Shield.kicad_sch")
    (property "Sheetname" "")
    (path "/431338ac-a7de-4b62-bdf2-eba514c80197")
    (attr through_hole)
    (fp_text reference "U7" (at 0 -2.33 90) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 39838c8b-e87f-437e-bd3f-43c336ef2bc8)
    )
    (fp_text value "Digital_2" (at 0 20.11 90) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a710ad48-66a3-480a-ad5f-a093d64d2937)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b25a1ec0-76af-4704-93f6-e2442ef60a1c)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8e8a4a9f-09da-4515-b565-74976a7abf32))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a08be0b4-38aa-4694-9a11-ffd1ea188ee2))
    (fp_line (start -1.33 1.27) (end -1.33 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1afb1e2f-7b88-4884-b637-8e2c6d0e8cf7))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d83aa256-ab48-42c7-8ce6-a1510df84ac5))
    (fp_line (start -1.33 19.11) (end 1.33 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9c7d7648-d48e-40aa-8eb9-e275e374d297))
    (fp_line (start 1.33 1.27) (end 1.33 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1a0ce42c-c060-4263-a95c-e1c866735b5e))
    (fp_line (start -1.8 -1.8) (end -1.8 19.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4a37605d-4915-4a56-bd4b-bcacd66ca770))
    (fp_line (start -1.8 19.55) (end 1.8 19.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bd614d94-e837-4af4-9f9d-fbfc89b0f486))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2f6a70e1-e3ca-4bcf-9f33-2ccb12705290))
    (fp_line (start 1.8 19.55) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3a9cfa31-ca8e-48cc-9d12-4e011094da5b))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0b5181f0-975d-4b23-b889-1b8df04bbcbc))
    (fp_line (start -1.27 19.05) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b7bd523a-7842-4a74-a3f4-7ac38ec0508c))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2e72f6d5-106e-49a8-bd60-57197caa70b4))
    (fp_line (start 1.27 -1.27) (end 1.27 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0ade8712-0b5a-4707-bf50-3093140a5c6b))
    (fp_line (start 1.27 19.05) (end -1.27 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 748c52bd-0f86-4b40-a673-0cce14b7983b))
    (pad "11" thru_hole circle (at 0 0 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 40 "unconnected-(U7-Pad11)") (pinfunction "D7") (pintype "bidirectional") (tstamp 519c7614-3827-4ac3-9801-e79dd8506283))
    (pad "12" thru_hole circle (at 0 2.54 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 41 "unconnected-(U7-Pad12)") (pinfunction "~D6") (pintype "bidirectional") (tstamp d16bea4d-4e3d-469d-a887-bed4ea7a009f))
    (pad "13" thru_hole circle (at 0 5.08 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 42 "unconnected-(U7-Pad13)") (pinfunction "~D5") (pintype "bidirectional") (tstamp fcf5b7ac-e49f-49a5-82de-78622cb7e59d))
    (pad "14" thru_hole circle (at 0 7.62 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 43 "unconnected-(U7-Pad14)") (pinfunction "D4") (pintype "bidirectional") (tstamp a1cddecb-7fef-4d50-b25f-5229903f244a))
    (pad "15" thru_hole circle (at 0 10.16 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 44 "unconnected-(U7-Pad15)") (pinfunction "~D3") (pintype "bidirectional") (tstamp 79085c5b-f782-42cd-b3cf-b05c42ee65e7))
    (pad "16" thru_hole circle (at 0 12.7 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 45 "unconnected-(U7-Pad16)") (pinfunction "D2") (pintype "bidirectional") (tstamp 52109a76-6897-4d18-8c20-609bd3f2fc14))
    (pad "17" thru_hole circle (at 0 15.24 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 46 "unconnected-(U7-Pad17)") (pinfunction "D1/TX0") (pintype "bidirectional") (tstamp cd99298e-a11d-42ff-a3a6-3158b73013aa))
    (pad "18" thru_hole circle (at 0 17.78 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 47 "unconnected-(U7-Pad18)") (pinfunction "D0/RX0") (pintype "bidirectional") (tstamp b1123e2e-ff68-41a3-8042-a49f65a101dc))
    (model "${KIPRJMOD}/3DModels/pin_header_female_2.54mm_0.1in.STEP"
      (offset (xyz 1.3 1.3 8.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )

  (footprint "ArduinoPinSockets:Arduino_PinSocket_1x10_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp b0dbd070-16c8-4e1d-88e8-491f63b11b03)
    (at 125.476 68.58 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (property "Sheetfile" "ArduinoUnoR4Shield.kicad_sch")
    (property "Sheetname" "")
    (path "/63f3422e-78b6-4e3c-b051-22b2d7c39605")
    (attr through_hole)
    (fp_text reference "U6" (at 0 -2.33 90) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c1d883e5-2277-4099-ab06-2f4788f4556b)
    )
    (fp_text value "Digital_1" (at 0 25.19 90) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 70ba6d6a-0390-483a-b763-bc4b9a418fa2)
    )
    (fp_text user "${REFERENCE}" (at 0 11.43) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 89b1b19e-af98-4c8a-9e0f-b88ba130fb92)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bddc253a-a35e-452b-a515-5db2c69ee1f2))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4592b101-88cb-4d41-9200-4fc933412045))
    (fp_line (start -1.33 1.27) (end -1.33 24.19)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ff970091-ab2e-4802-9be5-d9fedc6390a4))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e72b2ba0-f728-4671-be56-b5f66d995854))
    (fp_line (start -1.33 24.19) (end 1.33 24.19)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 11cc56b0-ad8c-48c6-a7c5-1503da2ba290))
    (fp_line (start 1.33 1.27) (end 1.33 24.19)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 12ebd8b2-39f3-4656-8a38-5fe7b280195c))
    (fp_line (start -1.8 -1.8) (end -1.8 24.65)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6019bf38-a286-4537-a253-3eba72e027be))
    (fp_line (start -1.8 24.65) (end 1.8 24.65)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1c24921e-f029-4ccc-9469-348e6f75556b))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0c2252bb-4e9c-4b60-8364-047e9fb1d4ca))
    (fp_line (start 1.8 24.65) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e7fe7b20-8c1f-4a5d-b26c-934dac285a27))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 016a9045-f7cd-470d-b339-6ecbbaa51b88))
    (fp_line (start -1.27 24.13) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ec4b7e20-e872-406d-87c2-a6c3169b3582))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cdc41618-a29e-45bf-8669-dd3cba432f27))
    (fp_line (start 1.27 -1.27) (end 1.27 24.13)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 538c69cf-c12e-431b-809b-5396efb287a3))
    (fp_line (start 1.27 24.13) (end -1.27 24.13)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d87812f4-3d1f-4aea-9058-8da88952426d))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(U6-Pad1)") (pinfunction "SCL") (pintype "bidirectional") (tstamp 9e6ad6e1-568a-4fcf-a8b9-72d8b85223b9))
    (pad "2" thru_hole circle (at 0 2.54 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(U6-Pad2)") (pinfunction "SDA") (pintype "bidirectional") (tstamp 3cb1c82b-91e6-4bd9-bde3-b4acf771ed67))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(U6-Pad3)") (pinfunction "AREF") (pintype "output") (tstamp 7f77da50-a0ba-4d03-ac5c-71afcbd55ef7))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(U6-Pad4)") (pinfunction "GND") (pintype "power_out") (tstamp f33e6970-6110-4cb4-8030-457bc1d4ea51))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(U6-Pad5)") (pinfunction "D13/SCK/CANRX0") (pintype "bidirectional") (tstamp be4ce2da-4d54-426d-a8fa-bdb1215dc480))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 29 "unconnected-(U6-Pad6)") (pinfunction "D12/CIPO") (pintype "bidirectional") (tstamp 313cda3f-f38f-4f18-beb5-292828cb48cf))
    (pad "7" thru_hole circle (at 0 15.24 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 30 "unconnected-(U6-Pad7)") (pinfunction "~D11/COPI") (pintype "bidirectional") (tstamp f765b4ff-f5c6-4f6b-9bfa-23e78b86d0db))
    (pad "8" thru_hole circle (at 0 17.78 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 31 "unconnected-(U6-Pad8)") (pinfunction "~D10/CS/CANTX0") (pintype "bidirectional") (tstamp 8172942f-8ee2-4769-a494-be5420297383))
    (pad "9" thru_hole circle (at 0 20.32 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 32 "unconnected-(U6-Pad9)") (pinfunction "~D9") (pintype "bidirectional") (tstamp 76488d93-0e2c-4493-92e7-7d4a28b62f62))
    (pad "10" thru_hole circle (at 0 22.86 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 33 "unconnected-(U6-Pad10)") (pinfunction "D8") (pintype "bidirectional") (tstamp b69334c5-b5cb-4f53-8c94-e05fd6649be0))
    (model "${KIPRJMOD}/3DModels/1x10.STEP"
      (offset (xyz -1.2 1.3 8.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (footprint "ArduinoMountingHoles:Arduino_MountingHole" (layer "F.Cu")
    (tstamp b1131b2c-7436-448d-be4a-099c268296e5)
    (at 120.65 116.84)
    (property "Sheetfile" "ArduinoUnoR4Shield.kicad_sch")
    (property "Sheetname" "")
    (path "/484f0239-84f5-49d9-b84d-554adc0db3d6")
    (attr smd)
    (fp_text reference "H4" (at 0 -6.81 unlocked) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 55a767f8-9fd6-4144-af01-93108ac17402)
    )
    (fp_text value "MountingHole4" (at 0 -5.31 unlocked) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e44d6763-406b-4634-9bce-6e9cf33e4d25)
    )
    (fp_text user "${REFERENCE}" (at 0 -3.81 unlocked) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c9e692a6-1172-422c-8d75-1a6b650c1ce9)
    )
    (pad "" np_thru_hole circle (at 0 0) (size 3.19989 3.19989) (drill 3.19989) (layers "F&B.Cu" "*.Mask")
      (solder_mask_margin 0.5) (tstamp 95601110-d968-4a7a-99e6-5181d05f6f41))
  )

  (footprint "ArduinoPinSockets:Arduino_PinSocket_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp bc917419-74c7-496b-81b1-45e19e4a36f9)
    (at 157.48 116.84 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "ArduinoUnoR4Shield.kicad_sch")
    (property "Sheetname" "")
    (path "/63007821-d794-4b28-94a8-9262a646d27d")
    (attr through_hole)
    (fp_text reference "U3" (at 0 -2.33 90) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 94923efe-4e89-4a4f-bb26-882a91f75e66)
    )
    (fp_text value "Analog_2" (at 0 15.03 90) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bff4f213-571b-47ae-a716-812b38fba289)
    )
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 893d1186-8698-473a-9963-0ea76feb878a)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ee486d56-2835-4fe4-8ce9-6936c2a853d4))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5a435456-b075-4219-a260-59067f4c954f))
    (fp_line (start -1.33 1.27) (end -1.33 14.03)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0d7c66a6-9fbd-4570-8938-5ec4464715be))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 54634143-04a8-4255-8a0c-66c7c3d9e8ba))
    (fp_line (start -1.33 14.03) (end 1.33 14.03)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 46a4c262-9384-42b0-a378-37f45982b677))
    (fp_line (start 1.33 1.27) (end 1.33 14.03)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d6d308c3-9aaf-4dea-8d75-34fa2ea51255))
    (fp_line (start -1.8 -1.8) (end -1.8 14.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 912d9b49-7170-4340-9030-575d64d94b42))
    (fp_line (start -1.8 14.5) (end 1.8 14.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bdfb919e-6311-46d3-8a03-2b194408e4c6))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a6d63524-df2a-4da7-9b8d-f803d4a15f54))
    (fp_line (start 1.8 14.5) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 38f450ea-a81c-4353-be64-774d7fa7df53))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0ffd2c69-493c-44ea-be56-5f2c054b03c0))
    (fp_line (start -1.27 13.97) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cdbb6373-d3a2-4e8a-91f5-0df2688c522d))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4b428c3e-78fe-423d-a1d3-d5def6f394cb))
    (fp_line (start 1.27 -1.27) (end 1.27 13.97)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 11e73308-73ec-4c3e-a9c3-860fa251ef4d))
    (fp_line (start 1.27 13.97) (end -1.27 13.97)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 65871039-7c0d-480b-8500-612c4b211f64))
    (pad "9" thru_hole circle (at 0 0 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 34 "unconnected-(U3-Pad9)") (pinfunction "A0") (pintype "bidirectional") (tstamp b274da14-92a7-4b86-864a-ad57b7d536c6))
    (pad "10" thru_hole circle (at 0 2.54 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 35 "unconnected-(U3-Pad10)") (pinfunction "A1") (pintype "bidirectional") (tstamp 24ea1f7f-f601-49fc-a8b1-7b9508a74fcd))
    (pad "11" thru_hole circle (at 0 5.08 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 36 "unconnected-(U3-Pad11)") (pinfunction "A2") (pintype "bidirectional") (tstamp 461b546b-93d7-4add-9c5c-4443c1be20b8))
    (pad "12" thru_hole circle (at 0 7.62 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 37 "unconnected-(U3-Pad12)") (pinfunction "A3") (pintype "bidirectional") (tstamp ad72ae46-89cd-4037-8c40-b1ffa34975c1))
    (pad "13" thru_hole circle (at 0 10.16 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 38 "unconnected-(U3-Pad13)") (pinfunction "A4") (pintype "bidirectional") (tstamp aaff15d2-1e25-4b32-8859-5cfabaca500c))
    (pad "14" thru_hole circle (at 0 12.7 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 39 "unconnected-(U3-Pad14)") (pinfunction "A5") (pintype "bidirectional") (tstamp 4d5b7c80-9d78-48b0-996f-cc3a0476894c))
    (model "${KIPRJMOD}/3DModels/1x6.STEP"
      (offset (xyz -1.3 1.3 8.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (footprint "ArduinoPinSockets:Arduino_PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp bce48327-225e-4c0f-95c6-69415511efa7)
    (at 134.62 116.84 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "ArduinoUnoR4Shield.kicad_sch")
    (property "Sheetname" "")
    (path "/b239170f-efa2-4070-8687-fa7a47427091")
    (attr through_hole)
    (fp_text reference "U2" (at 0 -2.33 90) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 16a8fcde-6945-47ed-b093-85510c2114a8)
    )
    (fp_text value "Analog_1" (at 0 20.11 90) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 95dc0131-c3fe-4d9e-a4e8-59878b331ced)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 398016ae-5549-4348-90d4-a2293b1178b9)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cdf3fca7-6ccd-4e0b-b6d9-7580e713188a))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b32ae90f-4b10-42e2-8666-239bc1f15ee9))
    (fp_line (start -1.33 1.27) (end -1.33 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f76cb197-44ff-4848-8cd8-6eff94873524))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d5061507-a4cb-40dd-bc88-82568d549551))
    (fp_line (start -1.33 19.11) (end 1.33 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 12fcec91-9651-444f-88ea-cedc59222460))
    (fp_line (start 1.33 1.27) (end 1.33 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f1c615d9-1c24-4d54-b245-be1257a1a37d))
    (fp_line (start -1.8 -1.8) (end -1.8 19.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 892fd2ba-2200-472e-98fc-256e1b17e7fc))
    (fp_line (start -1.8 19.55) (end 1.8 19.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 60368f3a-03c1-40f0-a16d-4d70c54b91cd))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8c1f7fb5-125a-4ee3-91ed-c312528006f4))
    (fp_line (start 1.8 19.55) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9b3fa32b-c6a0-4377-a9f6-983b2d8c61e1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7f4464cb-7f0e-47d1-9de9-4c045c4438c0))
    (fp_line (start -1.27 19.05) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2d298c38-dd52-489b-b0cd-c98421284cd8))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 70fa328b-8461-4dc7-9bf9-341ef0bfbf96))
    (fp_line (start 1.27 -1.27) (end 1.27 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 09c1132c-2c9e-4c33-a892-6004e1344402))
    (fp_line (start 1.27 19.05) (end -1.27 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2b44db68-acd6-4a6b-af65-0450bb13b7f3))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 4 "unconnected-(U2-Pad1)") (pinfunction "BOOT") (pintype "input") (tstamp 2d7d0027-8f4b-463e-ae7d-a19ae98a2704))
    (pad "2" thru_hole circle (at 0 2.54 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 5 "unconnected-(U2-Pad2)") (pinfunction "IOREF") (pintype "power_out") (tstamp 39aa136a-49ce-4513-9d3b-fddb1fdf88a5))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 6 "unconnected-(U2-Pad3)") (pinfunction "Reset") (pintype "input") (tstamp 21ef6bf5-df81-439d-bf00-76db09af6e90))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 7 "unconnected-(U2-Pad4)") (pinfunction "+3V3") (pintype "power_out") (tstamp b22ea22b-9410-4d87-86c0-b3c9da7e6571))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 8 "unconnected-(U2-Pad5)") (pinfunction "+5V") (pintype "power_out") (tstamp 7646d43b-d38b-43ef-a455-ee1bb4334592))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(U2-Pad6)") (pinfunction "GND") (pintype "power_out") (tstamp 31a12b0b-1ed0-401c-a6da-214cf408f534))
    (pad "7" thru_hole circle (at 0 15.24 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(U2-Pad7)") (pinfunction "GND") (pintype "power_out") (tstamp 0f971533-f91d-487a-a14e-89e5b8d7de71))
    (pad "8" thru_hole circle (at 0 17.78 90) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(U2-Pad8)") (pinfunction "VIN") (pintype "power_out") (tstamp 29af5d8d-f755-4b3f-8cf7-d54e70a87df3))
    (model "${KIPRJMOD}/3DModels/pin_header_female_2.54mm_0.1in.STEP"
      (offset (xyz 1.3 1.3 8.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )

  (footprint "ArduinoMountingHoles:Arduino_MountingHole" (layer "F.Cu")
    (tstamp e04389c5-0b54-4b52-92cc-19f23b6db214)
    (at 121.91999 68.58001)
    (property "Sheetfile" "ArduinoUnoR4Shield.kicad_sch")
    (property "Sheetname" "")
    (path "/cae81823-456a-4007-89b0-a70abec1758b")
    (attr smd)
    (fp_text reference "H2" (at 0 -6.81 unlocked) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bee7306b-758a-4ac8-bb3b-8e70f92c927c)
    )
    (fp_text value "MountingHole2" (at 0 -5.31 unlocked) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8e07b4b8-17b2-47c0-96e8-90a89a5db670)
    )
    (fp_text user "${REFERENCE}" (at 0 -3.81 unlocked) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d72f1ce0-7fca-40ca-82c7-ac690d929b44)
    )
    (pad "" np_thru_hole circle (at 0 0) (size 3.19989 3.19989) (drill 3.19989) (layers "F&B.Cu" "*.Mask")
      (solder_mask_margin 0.5) (tstamp e6644aa4-62cf-499a-b512-2e696f56d2f7))
  )

  (footprint "ArduinoPinSockets:Arduino_PinSocket_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp fbb7c789-9bc8-4866-8646-feb35f2def7f)
    (at 128.016 76.1492 -90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "ArduinoUnoR4Shield.kicad_sch")
    (property "Sheetname" "")
    (path "/6ca0b600-55b8-480e-86ab-70d33f64e0f6")
    (attr through_hole)
    (fp_text reference "U4" (at 1.27 -2.33 90) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 548749a2-aefa-4f3b-bc78-c3064f87d776)
    )
    (fp_text value "ESP32-S3" (at 1.27 7.41 90) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5a0dab3e-05d9-4e9f-8e1b-91ee6370c027)
    )
    (fp_text user "${REFERENCE}" (at 1.27 2.54) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3b2c838f-188b-48a0-87ab-4ab394dffad1)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5fcee3ef-4ee7-44ad-abd8-3d1e54af3307))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c9a032cd-bf5f-45d3-92e1-2a808e49fc44))
    (fp_line (start -1.33 1.27) (end -1.33 6.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0c55f4bf-b899-470a-b0e3-ec473f402e9a))
    (fp_line (start -1.33 1.27) (end 1.27 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0c2fedd7-bcbb-4be6-b36e-d3d6555db5aa))
    (fp_line (start -1.33 6.41) (end 3.87 6.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4eb6875e-49c0-4ec8-9919-b1eb74f4e35a))
    (fp_line (start 1.27 -1.33) (end 3.87 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 53f37a80-667b-45de-b216-5aaf56cdf6ac))
    (fp_line (start 1.27 1.27) (end 1.27 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8f034c35-7787-47a1-9c20-d19d3fdbe33a))
    (fp_line (start 3.87 -1.33) (end 3.87 6.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 52750fa5-aaf4-417b-b5a7-569d2cab4e29))
    (fp_line (start -1.8 -1.8) (end -1.8 6.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 11af1ed1-9ea1-4c3f-a8a0-1fcc2b0cc2e1))
    (fp_line (start -1.8 6.85) (end 4.35 6.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 406417e4-5dee-4534-af76-6eb854f4402d))
    (fp_line (start 4.35 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 95f23054-be86-411d-ad7c-cb32684f91e1))
    (fp_line (start 4.35 6.85) (end 4.35 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5c786a18-baac-42eb-ac95-40c980d9d642))
    (fp_line (start -1.27 0) (end 0 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 82059a18-b40d-4906-a618-dc34a4ef1d3c))
    (fp_line (start -1.27 6.35) (end -1.27 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fa0a60fa-73cf-4295-a85b-14e77df7ef41))
    (fp_line (start 0 -1.27) (end 3.81 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bbf0b7b4-61a5-4990-bf45-bf89873fc67a))
    (fp_line (start 3.81 -1.27) (end 3.81 6.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4f81e8dd-2ca5-4736-aeb2-1ad509913a1d))
    (fp_line (start 3.81 6.35) (end -1.27 6.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b6d82da2-7419-455e-a601-91d847db3518))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(U4-Pad1)") (pinfunction "GPIO42") (pintype "bidirectional") (tstamp 0d2158f2-bcd9-4265-8e29-7544701a08f8))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(U4-Pad2)") (pinfunction "GPIO41") (pintype "bidirectional") (tstamp a576d9d4-16c2-4db9-aa78-0c194d69ef4e))
    (pad "3" thru_hole circle (at 0 2.54 270) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 14 "unconnected-(U4-Pad3)") (pinfunction "GPIO43/TXD0") (pintype "bidirectional") (tstamp 33f671a5-43de-41bc-bc96-b6f720d9402f))
    (pad "4" thru_hole circle (at 2.54 2.54 270) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 15 "unconnected-(U4-Pad4)") (pinfunction "GPIO0/DOWNLOAD") (pintype "bidirectional") (tstamp 2a5557f5-b80e-4485-b89a-c8f87d465ff0))
    (pad "5" thru_hole circle (at 0 5.08 270) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(U4-Pad5)") (pinfunction "GPIO44/RXD0") (pintype "bidirectional") (tstamp bbf86fdb-ecb2-4ea1-9130-f7347e278f24))
    (pad "6" thru_hole circle (at 2.54 5.08 270) (size 1.422 1.422) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(U4-Pad6)") (pinfunction "GND") (pintype "power_out") (tstamp 3f1bc9f4-c1de-4e69-b97f-05675c98fc7d))
    (model "${KIPRJMOD}/3DModels/pin header female 2.54mm_0.1in.STEP"
      (offset (xyz 1.3 1.3 -10))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -180 0))
    )
    (model "${KIPRJMOD}/3DModels/pin header female 2.54mm_0.1in.STEP"
      (offset (xyz 3.7 1.3 -10))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -180 0))
    )
  )

  (footprint "ArduinoMountingHoles:Arduino_MountingHole" (layer "F.Cu")
    (tstamp fff9768b-b734-4ecd-98e9-1bdddd5e91ed)
    (at 172.72 111.76)
    (property "Sheetfile" "ArduinoUnoR4Shield.kicad_sch")
    (property "Sheetname" "")
    (path "/e0808123-e8b3-42ae-ba8a-c117a3e25098")
    (attr smd)
    (fp_text reference "H3" (at 0 -6.81 unlocked) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 64ee44fc-9a0f-46b2-805f-1a33e6d221b2)
    )
    (fp_text value "MountingHole3" (at 0 -5.31 unlocked) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0a95f9dd-fe92-455d-8076-51e100c8feff)
    )
    (fp_text user "${REFERENCE}" (at 0 -3.81 unlocked) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a5e340d6-b59e-45fa-8e55-c98d1da68da0)
    )
    (pad "" np_thru_hole circle (at 0 0) (size 3.19989 3.19989) (drill 3.19989) (layers "F&B.Cu" "*.Mask")
      (solder_mask_margin 0.5) (tstamp d64476c6-2d53-42ed-a325-18685bacfa2a))
  )

  (gr_line (start 171.196 66.04) (end 172.72 67.564)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 0b37582e-4aef-4a1d-b02e-836cae36f933))
  (gr_arc (start 107.696 119.38) (mid 106.97758 119.08242) (end 106.68 118.364)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 17507f6b-bff5-4605-aac5-ef23dd746e7d))
  (gr_line (start 172.72 78.994) (end 175.26 81.534)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 367697cd-a0ea-4570-83fb-fe5c7beca341))
  (gr_arc (start 172.72 118.364) (mid 172.42242 119.08242) (end 171.704 119.38)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 3aa08e6c-c487-4cdd-ae01-99db0b3cf1e8))
  (gr_line (start 175.26 81.534) (end 175.26 114.3)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 4153c0ef-c0ab-4590-bd4e-a048d96ce045))
  (gr_line (start 171.704 119.38) (end 107.696 119.38)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 41fca45b-32a7-4b07-9f98-b94af6335026))
  (gr_line (start 175.26 114.3) (end 172.72 116.84)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 6e1d066f-da0c-4958-a2f0-ca88bfc5f94e))
  (gr_line (start 172.72 67.564) (end 172.72 78.994)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 737df77a-2d62-4118-b6c1-e814a97aba2b))
  (gr_arc (start 106.68 67.056) (mid 106.97758 66.33758) (end 107.696 66.04)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 94dd7856-a8a5-4136-babc-b7a35866cdfe))
  (gr_line (start 172.72 116.84) (end 172.72 118.364)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp aa072add-5e43-4c26-9cc7-44a5a7d8e5f9))
  (gr_line (start 107.696 66.04) (end 171.196 66.04)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp dc908eb8-6d74-403f-9238-1166597aa959))
  (gr_line (start 106.68 118.364) (end 106.68 67.056)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp fe5da4d8-2c3f-4c43-ae6a-212b2c32df7d))

)
