(footprint "SW_Slide-03_7.3x2.5x2.5_P2.54mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Wuerth, WS-SLTV, 450301014042, https://www.we-online.com/components/products/datasheet/450301014042.pdf")
	(tags "switch single-pole double-throw SPDT würth wurth")
	(property "Reference" "REF**"
		(at 0 -2.54 0)
		(layer "F.SilkS")
		(uuid "91f8e7c5-1ab9-4140-873f-919408a983c5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SW_Slide-03_7.3x2.5x2.5_P2.54mm"
		(at 0 3.81 0)
		(layer "F.Fab")
		(uuid "0188cd0c-0317-45bc-8596-298ac8ec5a93")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4b1113a5-9095-463c-ac64-d0f5196bf183")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "dd0996dc-2584-4f0a-969c-7a83aa7f0321")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f0dd8ead-c29e-4913-b689-efe416fb9c16")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -4.11 -1.36)
		(end 3.86 1.36)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "e6c50bbc-8805-4f65-a52d-c390e7f2c366")
	)
	(fp_rect
		(start -4.25 -1.5)
		(end 4 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "f2252ff2-2d7e-412c-a62f-2302e4645acb")
	)
	(fp_rect
		(start -4 -1.25)
		(end 3.75 1.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "0dd6af52-a073-45ff-97f3-a7d515e3e150")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.54 0)
		(layer "F.Fab")
		(uuid "0551fa7c-a19d-4a21-adcf-80a77a655ee9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5edfecf2-dfb6-48da-8ec1-ce45c3dada6f")
	)
	(pad "2" thru_hole circle
		(at -2.54 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "009fb3af-d41e-46f4-bdd4-5c0efa4823c6")
	)
	(pad "3" thru_hole circle
		(at 2.54 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7b8be690-e896-4d08-9607-3e21c1a974a8")
	)
	(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_Slide-03_Wuerth-WS-SLTV_10x2.5x6.4_P2.54mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
