
(footprint RESCAXS127P508X320X70-8N (layer F.Cu) (tedit 66EF3CF1)
  (descr "")
  (attr smd)
  (fp_text reference REF** (at -0.378 -3.5264 0) (layer F.SilkS)
    (effects (font (size 0.64 0.64) (thickness 0.15)))
  )
  (fp_text value RESCAXS127P508X320X70-8N (at 7.3436 3.5264 0) (layer F.Fab)
    (effects (font (size 0.64 0.64) (thickness 0.15)))
  )
  (pad 8 smd roundrect (roundrect_rratio 0.1) (at 1.59 -2.005) (size 1.14 1.13) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 1 smd roundrect (roundrect_rratio 0.1) (at -1.59 -2.005) (size 1.14 1.13) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 2 smd roundrect (roundrect_rratio 0.1) (at -1.59 -0.635) (size 1.14 0.93) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 3 smd roundrect (roundrect_rratio 0.1) (at -1.59 0.635) (size 1.14 0.93) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 4 smd roundrect (roundrect_rratio 0.1) (at -1.59 2.005) (size 1.14 1.13) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 5 smd roundrect (roundrect_rratio 0.1) (at 1.59 2.005) (size 1.14 1.13) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 6 smd roundrect (roundrect_rratio 0.1) (at 1.59 0.635) (size 1.14 0.93) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 7 smd roundrect (roundrect_rratio 0.1) (at 1.59 -0.635) (size 1.14 0.93) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (fp_line (start 1.6 -2.54) (end -1.6 -2.54) (layer F.Fab) (width 0.127))
  (fp_line (start -1.6 -2.54) (end -1.6 2.54) (layer F.Fab) (width 0.127))
  (fp_line (start -1.6 2.54) (end 1.6 2.54) (layer F.Fab) (width 0.127))
  (fp_line (start 1.6 2.54) (end 1.6 -2.54) (layer F.Fab) (width 0.127))
  (fp_line (start -0.7 -2.54) (end 0.7 -2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start -0.7 2.54) (end 0.7 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start -2.41 -2.82) (end -2.41 2.82) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.41 2.82) (end 2.41 2.82) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.41 2.82) (end 2.41 -2.82) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.41 -2.82) (end -2.41 -2.82) (layer F.CrtYd) (width 0.05))
  (fp_circle (center -2.89 -2.005) (end -2.79 -2.005) (layer F.SilkS) (width 0.2))
  (fp_circle (center -2.89 -2.005) (end -2.79 -2.005) (layer F.Fab) (width 0.2))
)