
(footprint XCVR_ESP32-S3-WROOM-2-N32R8V (layer F.Cu) (tedit 67049FAC)
  (descr "")
  (attr smd)
  (fp_text reference REF** (at -6.575 -14.135 0) (layer F.SilkS)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (fp_text value XCVR_ESP32-S3-WROOM-2-N32R8V (at 8.03 14.365 0) (layer F.Fab)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (pad 41_1 smd rect (at -1.36 0.09) (size 1.0 1.0) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 1 smd rect (at -8.75 -5.26) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 41_2 smd rect (at -2.86 0.09) (size 1.0 1.0) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 41_3 smd rect (at 0.14 0.09) (size 1.0 1.0) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 41_4 smd rect (at -2.86 1.59) (size 1.0 1.0) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 41_5 smd rect (at -1.36 1.59) (size 1.0 1.0) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 41_6 smd rect (at 0.14 1.59) (size 1.0 1.0) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 41_7 smd rect (at -2.86 -1.41) (size 1.0 1.0) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 41_8 smd rect (at -1.36 -1.41) (size 1.0 1.0) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 41_9 smd rect (at 0.14 -1.41) (size 1.0 1.0) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 41_10 thru_hole circle (at -1.36 -0.66) (size 0.3 0.3) (drill 0.2) (layers *.Cu))
  (pad 41_11 thru_hole circle (at -2.86 -0.66) (size 0.3 0.3) (drill 0.2) (layers *.Cu))
  (pad 41_12 thru_hole circle (at 0.14 -0.66) (size 0.3 0.3) (drill 0.2) (layers *.Cu))
  (pad 41_13 thru_hole circle (at -2.86 0.84) (size 0.3 0.3) (drill 0.2) (layers *.Cu))
  (pad 41_14 thru_hole circle (at -1.36 0.84) (size 0.3 0.3) (drill 0.2) (layers *.Cu))
  (pad 41_15 thru_hole circle (at 0.14 0.84) (size 0.3 0.3) (drill 0.2) (layers *.Cu))
  (pad 41_16 thru_hole circle (at -2.11 -1.41) (size 0.3 0.3) (drill 0.2) (layers *.Cu))
  (pad 41_17 thru_hole circle (at -0.61 -1.41) (size 0.3 0.3) (drill 0.2) (layers *.Cu))
  (pad 41_18 thru_hole circle (at -2.11 0.09) (size 0.3 0.3) (drill 0.2) (layers *.Cu))
  (pad 41_19 thru_hole circle (at -0.61 0.09) (size 0.3 0.3) (drill 0.2) (layers *.Cu))
  (pad 41_20 thru_hole circle (at -2.11 1.59) (size 0.3 0.3) (drill 0.2) (layers *.Cu))
  (pad 41_21 thru_hole circle (at -0.61 1.59) (size 0.3 0.3) (drill 0.2) (layers *.Cu))
  (pad 2 smd rect (at -8.75 -3.99) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 3 smd rect (at -8.75 -2.72) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 4 smd rect (at -8.75 -1.45) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 5 smd rect (at -8.75 -0.18) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 6 smd rect (at -8.75 1.09) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 7 smd rect (at -8.75 2.36) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 8 smd rect (at -8.75 3.63) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 9 smd rect (at -8.75 4.9) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 10 smd rect (at -8.75 6.17) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 11 smd rect (at -8.75 7.44) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 12 smd rect (at -8.75 8.71) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 13 smd rect (at -8.75 9.98) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 14 smd rect (at -8.75 11.25) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 15 smd rect (at -6.985 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 27 smd rect (at 8.75 11.25) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 28 smd rect (at 8.75 9.98) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 29 smd rect (at 8.75 8.71) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 30 smd rect (at 8.75 7.44) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 31 smd rect (at 8.75 6.17) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 32 smd rect (at 8.75 4.9) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 33 smd rect (at 8.75 3.63) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 34 smd rect (at 8.75 2.36) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 35 smd rect (at 8.75 1.09) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 36 smd rect (at 8.75 -0.18) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 37 smd rect (at 8.75 -1.45) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 38 smd rect (at 8.75 -2.72) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 39 smd rect (at 8.75 -3.99) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 40 smd rect (at 8.75 -5.26) (size 1.5 0.9) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 16 smd rect (at -5.715 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 17 smd rect (at -4.445 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 18 smd rect (at -3.175 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 19 smd rect (at -1.905 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 20 smd rect (at -0.635 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 21 smd rect (at 0.635 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 22 smd rect (at 1.905 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 23 smd rect (at 3.175 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 24 smd rect (at 4.445 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 25 smd rect (at 5.715 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 26 smd rect (at 6.985 12.5) (size 0.9 1.5) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (fp_line (start -9.0 -12.75) (end 9.0 -12.75) (layer F.Fab) (width 0.127))
  (fp_line (start 9.0 -12.75) (end 9.0 -6.75) (layer F.Fab) (width 0.127))
  (fp_line (start 9.0 -6.75) (end 9.0 12.75) (layer F.Fab) (width 0.127))
  (fp_line (start 9.0 12.75) (end -9.0 12.75) (layer F.Fab) (width 0.127))
  (fp_line (start -9.0 12.75) (end -9.0 -6.75) (layer F.Fab) (width 0.127))
  (fp_line (start -9.0 -6.75) (end -9.0 -12.75) (layer F.Fab) (width 0.127))
  (fp_line (start -9.0 -6.75) (end 9.0 -6.75) (layer F.Fab) (width 0.127))
  (fp_text user "ANTENNA" (at -4.5 -9.5) (layer F.Fab)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (fp_line (start -9.75 13.5) (end -9.75 -13.0) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.75 -13.0) (end 9.75 -13.0) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.75 -13.0) (end 9.75 13.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.75 13.5) (end 9.75 13.5) (layer F.CrtYd) (width 0.05))
  (fp_circle (center -10.2 -5.26) (end -10.1 -5.26) (layer F.Fab) (width 0.2))
  (fp_line (start -9.0 -12.75) (end 9.0 -12.75) (layer F.SilkS) (width 0.127))
  (fp_line (start 9.0 -12.75) (end 9.0 -6.03) (layer F.SilkS) (width 0.127))
  (fp_line (start -9.0 -6.03) (end -9.0 -12.75) (layer F.SilkS) (width 0.127))
  (fp_circle (center -10.2 -5.26) (end -10.1 -5.26) (layer F.SilkS) (width 0.2))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -9.0 -12.75)
        (xy 9.0 -12.75)
        (xy 9.0 -6.75)
        (xy -9.0 -6.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -9.0 -12.75)
        (xy 9.0 -12.75)
        (xy 9.0 -6.75)
        (xy -9.0 -6.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -9.0 -12.75)
        (xy 9.0 -12.75)
        (xy 9.0 -6.75)
        (xy -9.0 -6.75)
      )
    )
  )
  (fp_line (start -9.0 12.02) (end -9.0 12.75) (layer F.SilkS) (width 0.127))
  (fp_line (start -9.0 12.75) (end -7.755 12.75) (layer F.SilkS) (width 0.127))
  (fp_line (start 9.0 12.02) (end 9.0 12.75) (layer F.SilkS) (width 0.127))
  (fp_line (start 9.0 12.75) (end 7.755 12.75) (layer F.SilkS) (width 0.127))
)