(footprint "ESP32-C3-WROOM-02-H4"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -6.575 -11.085 0)
		(layer "F.SilkS")
		(uuid "c1ef7f4f-d8a5-44f4-ad1d-4b2aec7eccf5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "ESP32-C3-WROOM-02-H4"
		(at 7.395 11.085 0)
		(layer "F.Fab")
		(uuid "b181fa74-d9b4-4804-9bc1-b081e6bde4bb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "15536f93-f33c-4864-9d98-6e178b43b039")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7dfa6719-3fd2-4897-bc0d-ec5e75a775dd")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "9a131e6a-a466-4751-94ad-e5721b8264e5")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -9 -10)
		(end -9 -3.67)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0076f9b1-81b5-4285-abb4-62faf899b121")
	)
	(fp_line
		(start -9 10)
		(end -9 9.87)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "193a1fe4-1544-4f0a-a331-baad59e749fc")
	)
	(fp_line
		(start -9 10)
		(end 9 10)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e3d811e3-865c-4318-9fe1-1cba1633accd")
	)
	(fp_line
		(start 9 -10)
		(end -9 -10)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2f7ccea0-b14d-4f41-9967-771d65b5ea14")
	)
	(fp_line
		(start 9 -3.67)
		(end 9 -10)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "34a1d457-851b-4c77-b352-0988e5fbe50d")
	)
	(fp_line
		(start 9 10)
		(end 9 9.87)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "999f0b2b-d2bd-44aa-8d78-3240b5b1c47b")
	)
	(fp_circle
		(center -10.5 -2.9)
		(end -10.4 -2.9)
		(stroke
			(width 0.2)
			(type solid)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "cd47654d-a52c-422c-8e77-eae4d78f69f4")
	)
	(fp_line
		(start -9.75 -10.25)
		(end -9.75 10.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "172387b9-ba7a-4395-a875-36d8319536fa")
	)
	(fp_line
		(start -9.75 10.25)
		(end 9.75 10.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "07a472d3-b3b4-48a8-92c5-11b84169a55b")
	)
	(fp_line
		(start 9.75 -10.25)
		(end -9.75 -10.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2af17463-a6d8-4a6a-85bf-7a4abc35fe63")
	)
	(fp_line
		(start 9.75 10.25)
		(end 9.75 -10.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4c08169c-2bb8-4f43-8692-d32e478139b3")
	)
	(fp_line
		(start -9 -10)
		(end -9 -4)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "81588b9a-c83a-4bc7-ba7a-167b90fc3fdd")
	)
	(fp_line
		(start -9 -4)
		(end -9 10)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "67974f64-51a9-4e67-9a68-00e668e6c344")
	)
	(fp_line
		(start -9 10)
		(end 9 10)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5c37b9a1-b972-4c2b-a47c-76444bfcece7")
	)
	(fp_line
		(start 9 -10)
		(end -9 -10)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e78db179-c8bb-4496-8101-cb63044d88f9")
	)
	(fp_line
		(start 9 -4)
		(end -9 -4)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "41282e0d-9a18-4120-b9bd-655e8effafd8")
	)
	(fp_line
		(start 9 -4)
		(end 9 -10)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "91151eb1-8a2c-498f-bb58-b95a6358faa4")
	)
	(fp_line
		(start 9 10)
		(end 9 -4)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "22f16326-4c43-4f12-97bd-c64200effc3c")
	)
	(fp_circle
		(center -10.5 -2.9)
		(end -10.4 -2.9)
		(stroke
			(width 0.2)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "cc470171-7a85-46f0-942b-31d5aac30266")
	)
	(pad "1" smd rect
		(at -8.75 -2.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "4f2cf8cd-63a0-4c4d-a2fc-30401d4d579d")
	)
	(pad "2" smd rect
		(at -8.75 -1.4)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "2d7bde91-885b-4e75-96aa-3a220aea7933")
	)
	(pad "3" smd rect
		(at -8.75 0.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "f71a33f4-b981-4849-a326-fe0eb98aa681")
	)
	(pad "4" smd rect
		(at -8.75 1.6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "1b987018-93b0-4de0-8271-a4673148f422")
	)
	(pad "5" smd rect
		(at -8.75 3.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "0a1b99dc-6f53-4dae-93f8-c1c147265d2f")
	)
	(pad "6" smd rect
		(at -8.75 4.6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "d9ba1da5-7148-4d31-bf5c-683c0bd8595a")
	)
	(pad "7" smd rect
		(at -8.75 6.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "3cf28dcf-d765-4dbe-8bf3-7bca177e725b")
	)
	(pad "8" smd rect
		(at -8.75 7.6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "df872d06-3e39-4375-bc22-ef3bb3d1b1b6")
	)
	(pad "9" smd rect
		(at -8.75 9.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "19431822-d50b-4e77-a015-065108c192f0")
	)
	(pad "10" smd rect
		(at 8.75 9.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "9f193b3b-31f5-404c-bf3c-70e85a9dffde")
	)
	(pad "11" smd rect
		(at 8.75 7.6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "06bd1478-6895-4d06-9e7c-f38386483dc7")
	)
	(pad "12" smd rect
		(at 8.75 6.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "b61ccca8-29cd-479e-93e0-82b8fc376640")
	)
	(pad "13" smd rect
		(at 8.75 4.6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "5e26cebb-1376-4f2d-85a0-663e3d89c305")
	)
	(pad "14" smd rect
		(at 8.75 3.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "051e7207-9b08-4f18-bf50-d3eb8d8a0eaf")
	)
	(pad "15" smd rect
		(at 8.75 1.6)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "6de2f8c7-78a2-4f9f-86bf-44bc3d928dbb")
	)
	(pad "16" smd rect
		(at 8.75 0.1)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "36396bbc-12de-4a0e-964d-54fb454c4e00")
	)
	(pad "17" smd rect
		(at 8.75 -1.4)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "915268c9-6d26-4efe-9a23-a01ec54b2d33")
	)
	(pad "18" smd rect
		(at 8.75 -2.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "ca71375e-d35c-4f9e-9aae-637df1a557c2")
	)
	(pad "19" smd rect
		(at -0.14 2.2)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "385b5496-6d73-41a6-af62-a1475a34a52f")
	)
	(pad "20" smd rect
		(at 0.96 2.2)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "8fafad51-c486-44eb-8e9f-1c70644eeaa3")
	)
	(pad "21" smd rect
		(at 2.06 2.2)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "89f4dcce-d1b6-47ed-a960-49ee0ea49182")
	)
	(pad "22" smd rect
		(at -0.14 3.3)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "cf5f9572-6ac2-4561-a9e9-38441368ff44")
	)
	(pad "23" smd rect
		(at 0.96 3.3)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "dd536341-59e7-4ec1-b803-5207f361bdd3")
	)
	(pad "24" smd rect
		(at 2.06 3.3)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "7f4a1e09-9261-40e2-9e68-a32b10a467e7")
	)
	(pad "25" smd rect
		(at -0.14 4.4)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "8733727d-1033-49d3-af6e-2f32f6d3a3d5")
	)
	(pad "26" smd rect
		(at 0.96 4.4)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "24de7862-16fc-4700-aa17-48387ff3c2e1")
	)
	(pad "27" smd rect
		(at 2.06 4.4)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
		(uuid "e08912de-8924-4b1b-9ef5-8acffb9f1eb7")
	)
	(pad "28" thru_hole circle
		(at 0.41 2.2)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "e92f3fbd-680c-404a-9731-81d18b0d1160")
	)
	(pad "29" thru_hole circle
		(at 1.51 2.2)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "76f7b757-fea9-4212-a976-bfb2e8e6ad7d")
	)
	(pad "30" thru_hole circle
		(at -0.14 2.75)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "ff4649c9-87af-40f8-857c-ce33a08cebc9")
	)
	(pad "31" thru_hole circle
		(at 0.96 2.75)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "78c7a6ee-6de2-4034-8333-107691cb871e")
	)
	(pad "32" thru_hole circle
		(at 2.06 2.75)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "36c35b0c-23ef-47f7-b22f-13a0a2a03658")
	)
	(pad "33" thru_hole circle
		(at 0.41 3.3)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "1db95e42-0600-4c5f-89fe-895929074861")
	)
	(pad "34" thru_hole circle
		(at 1.51 3.3)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "93aa8f8f-dc4a-4913-a4ac-27ec72a30846")
	)
	(pad "35" thru_hole circle
		(at -0.14 3.85)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "629decbb-bf92-41dc-aeab-d7f59202750a")
	)
	(pad "36" thru_hole circle
		(at 0.96 3.85)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "1fa7fe60-609e-4366-926d-91f44ba27f58")
	)
	(pad "37" thru_hole circle
		(at 2.06 3.85)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "bc3acfb6-52b0-45ca-81b6-2d184b9afe85")
	)
	(pad "38" thru_hole circle
		(at 0.41 4.4)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "3f7d3459-139d-4fdb-8e48-0c7e980d52b5")
	)
	(pad "39" thru_hole circle
		(at 1.51 4.4)
		(size 0.4 0.4)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
		(uuid "34f87634-3531-4b8b-8137-238797db8d16")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "862083ce-f31d-451b-b600-797268f6d971")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9 -10) (xy 9 -10) (xy 9 -4) (xy -9 -4)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu")
		(uuid "23faee98-3437-4126-b9e6-da16c18b2d7e")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9 -10) (xy 9 -10) (xy 9 -4) (xy -9 -4)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(uuid "a1808f18-e0f9-4b1a-a307-741746e8d492")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9 -10) (xy 9 -10) (xy 9 -4) (xy -9 -4)
			)
		)
	)
	(model "C:/Users/alex/github/KiCAD-Libraries/ESP32-C3-WROOM-02-N4.step"
		(offset
			(xyz 0 0.01 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
