(footprint "BME280_BMP280_I2C"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Temperature, Humidity and Pressure sensor")
	(tags "BME BMP 280 sensor")
	(property "Reference" "REF**"
		(at 0 -0.6 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b2f73bb8-4683-4ee9-8ab3-b6ce16dac6d2")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "BME(P)280"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "fff12e2f-d528-4335-990a-e4a0482935fc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ad329f2a-2a43-45ce-94c5-a84992e49cbb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ba517ac1-53c2-43d6-aa10-be76758929c8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Temperature, Humidity and Pressure sensor; I2C interface"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e2235702-6933-4ccd-92be-eab4fc07ff6f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start 0 0)
		(end 13 10)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "ae20fa2a-e81e-43f9-ab3a-0a7440443314")
	)
	(fp_circle
		(center 11.2 1.8)
		(end 12.3 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "692e882c-c4a3-4699-ba13-bfc83c56ad4b")
	)
	(fp_rect
		(start 0 0)
		(end 13 10)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "196d99dd-ca23-4891-a5a9-102dc2a2d12d")
	)
	(fp_text user "BME(P) 280"
		(at 6.8 5 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "d0814df1-988f-493a-936b-4823a83db662")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "d88c27f7-7ef8-4b84-894e-4c9c27ced838")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 1.3 1.22)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c4b77e8c-9597-467f-896c-0a3b58f9df68")
	)
	(pad "2" thru_hole circle
		(at 1.3 3.76)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d946b919-5c59-4166-b126-d3697e239817")
	)
	(pad "3" thru_hole circle
		(at 1.3 6.3)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "376baac8-5abd-4ea7-abe7-e45a43c37a64")
	)
	(pad "4" thru_hole circle
		(at 1.3 8.84)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "27e65202-1f5a-4e17-a7d2-3f2bf667346c")
	)
)