(footprint "MOSFET-NP-SSF6670-SOP-8_3.9x4.9mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "SOP SO")
	(property "Reference" "REF**"
		(at 0 -3.4 0)
		(layer "F.SilkS")
		(uuid "b99f5d35-59a1-4175-b193-54d5d5093ec7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "MOSFET-NP-SSF6670-SOP-8_3.9x4.9mm"
		(at 0 3.4 0)
		(layer "F.Fab")
		(uuid "dd214028-f121-4488-858e-2dd07ee98d39")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ad8b8ddb-2375-4f51-91dd-43f9070ac183")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "087ba4aa-f5be-40f3-85bd-6f4e75715d1c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4c1e94e1-46cb-43ef-9364-c7b6c181bcd8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0 -2.56)
		(end -1.95 -2.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0fdd37b4-7583-4023-b00b-343be215c754")
	)
	(fp_line
		(start 0 -2.56)
		(end 1.95 -2.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4af88de5-4327-4de0-9bf2-e5fa2903768a")
	)
	(fp_line
		(start 0 2.56)
		(end -1.95 2.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ee0bc5e3-6fd2-43bf-8067-5c90c0892cd4")
	)
	(fp_line
		(start 0 2.56)
		(end 1.95 2.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "07499253-7034-4f5c-a311-82b2cd7f93da")
	)
	(fp_poly
		(pts
			(xy -2.7 -2.465) (xy -2.94 -2.795) (xy -2.46 -2.795) (xy -2.7 -2.465)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "599a0b9c-648b-4957-9c20-78d6813190bf")
	)
	(fp_line
		(start -3.7 -2.7)
		(end -3.7 2.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5e61c401-1747-46a1-9f90-cb098256e865")
	)
	(fp_line
		(start -3.7 2.7)
		(end 3.7 2.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9e83a82a-da2c-46da-9cfb-31132ec38c6e")
	)
	(fp_line
		(start 3.7 -2.7)
		(end -3.7 -2.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d9eede71-ab2a-4ae8-bf88-d925899052bf")
	)
	(fp_line
		(start 3.7 2.7)
		(end 3.7 -2.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7a1d2a77-18d3-4ec0-995e-4112b46d6fab")
	)
	(fp_line
		(start -1.95 -1.475)
		(end -0.975 -2.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f016fa6e-cbd1-45d6-876a-904fd49110d9")
	)
	(fp_line
		(start -1.95 2.45)
		(end -1.95 -1.475)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9a69d119-ac5f-403d-a3eb-986ada33ac50")
	)
	(fp_line
		(start -0.975 -2.45)
		(end 1.95 -2.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f5f70270-25ed-404b-98c5-870b56f44048")
	)
	(fp_line
		(start 1.95 -2.45)
		(end 1.95 2.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ae53cb9f-e256-419c-bfae-3b564eae4c5c")
	)
	(fp_line
		(start 1.95 2.45)
		(end -1.95 2.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "58185606-4db9-454e-8141-0499192d33c2")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "77bcc5ce-5e6f-4c0f-94f2-4d2cca1d887d")
		(effects
			(font
				(size 0.98 0.98)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.625 -1.905)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "c721f725-e542-4d49-8377-e105c221f466")
	)
	(pad "2" smd roundrect
		(at -2.625 -0.635)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "4c648e66-569a-4144-b2a2-70f76e094333")
	)
	(pad "3" smd roundrect
		(at -2.625 0.635)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "1195948b-a670-48fd-af6f-8761a7451ed4")
	)
	(pad "4" smd roundrect
		(at -2.625 1.905)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "459aaaed-4db9-45d0-a625-816cfd061663")
	)
	(pad "5" smd roundrect
		(at 2.625 1.905)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "eef84009-3aef-4df7-b116-33d05b8f0c05")
	)
	(pad "6" smd roundrect
		(at 2.625 0.635)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "380872b4-0579-4a51-a861-1cdc33248143")
	)
	(pad "7" smd roundrect
		(at 2.625 -0.635)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "6ac88393-3ba7-45fe-a4c3-c4f33e158878")
	)
	(pad "8" smd roundrect
		(at 2.625 -1.905)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "69a6a3ed-a8f8-47e1-aef6-5f58b4b86b0e")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOP-8_3.9x4.9mm_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
