(footprint "ESP32-C3_SuperMini"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "ESP32 C3 Super Mini")
	(tags "ESP32 C3")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "cee1dcb7-49d6-47bf-afb1-c5247cf191bf")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "ESP32-C3_SuperMini"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b699cd6c-c89b-47f3-ace3-24c02047a611")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Alexander Footprint Library:ESP32-C3_SuperMini"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6f412b33-4d27-4658-9f7e-6d4eb7572bd6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0c4ada2c-e3c2-48fb-841a-1685ffc1aa17")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "ESP32 C3 Super Mini"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6521eb37-600e-4181-a5c2-ca9bf5df9738")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a6afda93-6dfa-4e1c-8d97-7ebeb08412d1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at 0 -20.32)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0)
		(chamfer_ratio 0.25)
		(chamfer top_left)
		(uuid "88ca3259-c5e7-4bcf-9215-328098ae68f1")
	)
	(pad "2" thru_hole oval
		(at 0 -17.78)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8c140aba-7566-4ddd-916a-cab44138c547")
	)
	(pad "3" thru_hole oval
		(at 0 -15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c10b09f4-456d-4ee2-be5f-6677d0655e20")
	)
	(pad "4" thru_hole oval
		(at 0 -12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3a41051d-8d83-4ecf-a0fa-72d7fc1d996b")
	)
	(pad "5" thru_hole oval
		(at 0 -10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f19f2195-9c00-468f-9de8-9745f441c5f1")
	)
	(pad "6" thru_hole oval
		(at 0 -7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e55a397f-24d1-4084-aae7-597dc7bdb61e")
	)
	(pad "7" thru_hole oval
		(at 0 -5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6bb8895d-524f-474d-af5b-fff5a0176362")
	)
	(pad "8" thru_hole oval
		(at 0 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "eb9be630-9229-4013-91b5-d84cdbe76cdd")
	)
	(pad "9" thru_hole oval
		(at 15.24 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cb45ea7e-7497-47ef-9761-819dbecf7429")
	)
	(pad "10" thru_hole oval
		(at 15.24 -5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0b1721de-dd2b-4ba0-bdbe-5e2fc35a9619")
	)
	(pad "11" thru_hole oval
		(at 15.24 -7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "145c1d75-a850-44c3-b26a-8fb0beb996a8")
	)
	(pad "12" thru_hole oval
		(at 15.24 -10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ab38707c-89f1-41f6-b0b4-dedb69ce8089")
	)
	(pad "13" thru_hole oval
		(at 15.24 -12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c4abde78-23fb-4741-a3f9-fadfad94de81")
	)
	(pad "14" thru_hole oval
		(at 15.24 -15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e9ae96d8-f9d5-4ba7-bb02-08f7ae4e46a1")
	)
	(pad "15" thru_hole rect
		(at 15.24 -17.78)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a54e90cb-40b5-462c-86f8-49f9f869de47")
	)
	(pad "16" thru_hole oval
		(at 15.24 -20.32)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fb09284c-c15b-4c1b-87e3-a063b223dfc3")
	)
)
