(footprint "ESP32-S2mini-Weemos"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "ESP32-S2mini Weemos")
	(tags "ESP32 S2")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "85e67103-2dc8-492b-8760-8ded1cab9887")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "ESP32-S2mini"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b748e87d-3c4f-4d5e-93bd-32f2f113c773")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "93e57a27-3b74-437b-8e93-819e4506da6f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c4dd62ad-f165-4859-876f-0f44159e121e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a0e2ca00-57f4-4895-8adf-07d0ba1a8982")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -2.54 6)
		(end -2.54 -26.94)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "2feefd70-2dbb-433b-a692-2cd7dcc92424")
	)
	(fp_line
		(start -1.54 -27.94)
		(end 24.4 -27.94)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "80c9e49b-1184-4876-a0e3-03b438177d93")
	)
	(fp_line
		(start 24.4 7)
		(end -1.54 7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "dcc24b01-ee61-4355-a234-183ab4c2c1a5")
	)
	(fp_line
		(start 25.4 -26.94)
		(end 25.4 6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "9d385446-09ba-429b-b698-1435b02ca15b")
	)
	(fp_arc
		(start -2.54 -26.94)
		(mid -2.247107 -27.647107)
		(end -1.54 -27.94)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "7b67c202-51f7-404c-8e95-4fc959a1f4b2")
	)
	(fp_arc
		(start -1.54 7)
		(mid -2.247107 6.707107)
		(end -2.54 6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "6e5ceaa9-7738-4816-8163-35cb8a9c572d")
	)
	(fp_arc
		(start 24.4 -27.94)
		(mid 25.107107 -27.647107)
		(end 25.4 -26.94)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "a4504e82-a3c0-44b6-bbd4-d31deed26c77")
	)
	(fp_arc
		(start 25.4 6)
		(mid 25.107107 6.707107)
		(end 24.4 7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "d38c390d-ad7d-4332-9e74-c069788c16ca")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "1d0f991e-c1ee-44bc-8da9-d711b62b66fd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 2.54 -20.32)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "76ae043d-d892-46f0-be5e-787cb9fc22a4")
	)
	(pad "2" thru_hole roundrect
		(at 0 -20.32)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0)
		(chamfer_ratio 0.25)
		(chamfer top_left)
		(uuid "b23eb19d-81d8-4fac-bf2f-51da830a94d9")
	)
	(pad "3" thru_hole circle
		(at 2.54 -17.78)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "97232564-a6d3-4f4f-bb30-2b4d0a4e0043")
	)
	(pad "4" thru_hole circle
		(at 0 -17.78)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f5db6b1f-5dad-45cc-b68e-bcf65a9e9edf")
	)
	(pad "5" thru_hole circle
		(at 2.54 -15.24)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "faa404c0-3fd6-46a1-be04-98747d0657c9")
	)
	(pad "6" thru_hole circle
		(at 0 -15.24)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4635bf8d-98d2-41c7-baaa-8ab7902ab92e")
	)
	(pad "7" thru_hole circle
		(at 2.54 -12.7)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f68478af-a5ea-42c6-ae23-6606b7def362")
	)
	(pad "8" thru_hole circle
		(at 0 -12.7)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f0d8c34d-f538-4061-a43b-a340cfd2b4d1")
	)
	(pad "9" thru_hole circle
		(at 2.54 -10.16)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bbdff238-87a0-4188-8d3c-716f3f311ce2")
	)
	(pad "10" thru_hole circle
		(at 0 -10.16)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "88a9484c-82a7-4865-86bb-378aa87a1180")
	)
	(pad "11" thru_hole circle
		(at 2.54 -7.62)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0a5017bb-848b-43fa-ae9d-7da85af8d181")
	)
	(pad "12" thru_hole circle
		(at 0 -7.62)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "22b311e8-4ffd-4629-8cfd-a9e31a4a3195")
	)
	(pad "13" thru_hole circle
		(at 2.54 -5.08)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "96faa1d1-d8ae-422d-bd15-cace204a0c63")
	)
	(pad "14" thru_hole circle
		(at 0 -5.08)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fdf4b7bb-2dcf-4166-a4e9-0834f8f1ca71")
	)
	(pad "15" thru_hole circle
		(at 2.54 -2.54)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "60ac0410-b862-4315-9711-81a5f21b2d09")
	)
	(pad "16" thru_hole circle
		(at 0 -2.54)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "526e3c5e-523a-4fe4-80b2-128d6de1fb15")
	)
	(pad "17" thru_hole circle
		(at 22.86 -20.32)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5e13b752-a375-4cd0-ab52-1255fac70f9e")
	)
	(pad "18" thru_hole circle
		(at 20.32 -20.32)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d55e37f4-0d9f-4f01-8b67-60cd5fdab85f")
	)
	(pad "19" thru_hole circle
		(at 22.86 -17.78)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "701ef938-9d4d-41d4-9f8f-bd53a4f5f42e")
	)
	(pad "20" thru_hole circle
		(at 20.32 -17.78)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c2dccc32-eb41-4fa1-ba75-10f765d56d4e")
	)
	(pad "21" thru_hole circle
		(at 22.86 -15.24)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "737782ef-69fd-4622-9a88-5568be9c57c6")
	)
	(pad "22" thru_hole circle
		(at 20.32 -15.24)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ed79534a-86c7-4bb3-bed0-522cf83c453b")
	)
	(pad "23" thru_hole circle
		(at 22.86 -12.7)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8a301d13-c8ec-4099-baee-46b2ef2be750")
	)
	(pad "24" thru_hole circle
		(at 20.32 -12.7)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1b54d5dd-67db-4fb5-bc83-0a657f57eb92")
	)
	(pad "25" thru_hole circle
		(at 22.86 -10.16)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "672cdf15-6045-4eb0-8b3f-0f6d48114f2f")
	)
	(pad "26" thru_hole circle
		(at 20.32 -10.16)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8850b74d-9d07-49a2-88d6-d72adeff12ec")
	)
	(pad "27" thru_hole circle
		(at 22.86 -7.62)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4602d319-acfc-4f8c-a66e-3f6809c34eb3")
	)
	(pad "28" thru_hole circle
		(at 20.32 -7.62)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c8d9c509-f6a4-40cb-8b01-8282afc2ea59")
	)
	(pad "29" thru_hole rect
		(at 22.86 -5.08)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "dd634ae5-f4ab-4307-bfea-29ed2ad8226e")
	)
	(pad "30" thru_hole rect
		(at 20.32 -5.08)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1d70c0ff-c109-4e63-9694-c5ae2bb2bf27")
	)
	(pad "31" thru_hole circle
		(at 22.86 -2.54)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6a4f2b3a-c39b-4042-8e47-e66174997851")
	)
	(pad "32" thru_hole circle
		(at 20.32 -2.54)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "95bb7757-bc42-4354-8286-a07f9348d96e")
	)
)
