
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "TXB0108PWR" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -12.7 23.86 0.0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "TXB0108PWR" (id 1) (at -12.7 -21.78 0.0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "TXB0108PWR:SOP65P640X120-20N" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "H" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Texas Instruments" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.2mm" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "IPC-7351B" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "TXB0108PWR_0_0"
      (rectangle (start -12.7 -17.78) (end 12.7 22.86)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin bidirectional line (at -17.78 7.62 0) (length 5.08)
        (name "A1"
          (effects (font (size 1.016 1.016)))
        )
        (number "1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 5.08 0) (length 5.08)
        (name "A2"
          (effects (font (size 1.016 1.016)))
        )
        (number "3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 2.54 0) (length 5.08)
        (name "A3"
          (effects (font (size 1.016 1.016)))
        )
        (number "4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 0.0 0) (length 5.08)
        (name "A4"
          (effects (font (size 1.016 1.016)))
        )
        (number "5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 7.62 180.0) (length 5.08)
        (name "B1"
          (effects (font (size 1.016 1.016)))
        )
        (number "20"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 5.08 180.0) (length 5.08)
        (name "B2"
          (effects (font (size 1.016 1.016)))
        )
        (number "18"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 2.54 180.0) (length 5.08)
        (name "B3"
          (effects (font (size 1.016 1.016)))
        )
        (number "17"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 0.0 180.0) (length 5.08)
        (name "B4"
          (effects (font (size 1.016 1.016)))
        )
        (number "16"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -17.78 12.7 0) (length 5.08)
        (name "OE"
          (effects (font (size 1.016 1.016)))
        )
        (number "10"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 20.32 180.0) (length 5.08)
        (name "VCCA"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 17.78 180.0) (length 5.08)
        (name "VCCB"
          (effects (font (size 1.016 1.016)))
        )
        (number "19"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 -2.54 0) (length 5.08)
        (name "A5"
          (effects (font (size 1.016 1.016)))
        )
        (number "6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 -5.08 0) (length 5.08)
        (name "A6"
          (effects (font (size 1.016 1.016)))
        )
        (number "7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 -7.62 0) (length 5.08)
        (name "A7"
          (effects (font (size 1.016 1.016)))
        )
        (number "8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 -10.16 0) (length 5.08)
        (name "A8"
          (effects (font (size 1.016 1.016)))
        )
        (number "9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 -2.54 180.0) (length 5.08)
        (name "B5"
          (effects (font (size 1.016 1.016)))
        )
        (number "15"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 -5.08 180.0) (length 5.08)
        (name "B6"
          (effects (font (size 1.016 1.016)))
        )
        (number "14"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 -7.62 180.0) (length 5.08)
        (name "B7"
          (effects (font (size 1.016 1.016)))
        )
        (number "13"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 -10.16 180.0) (length 5.08)
        (name "B8"
          (effects (font (size 1.016 1.016)))
        )
        (number "12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -15.24 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "11"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)