(footprint "Conn_I2C_3" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 8060404d-7584-4986-83fc-8fdc66016fdb)
  )
  (fp_text value "Conn_I2C_3" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ba0e9860-90bb-4e1f-9729-155a34948ea8)
  )
  (fp_text user "Vcc" (at 7.62 10.16 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp 1d40c77c-7a15-463f-9f12-f62fa4b0ab23)
  )
  (fp_text user "#2" (at 2.54 5.08 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)) (justify top))
    (tstamp 1f3f1931-c15b-4ffd-9c0b-d3e649c4cf93)
  )
  (fp_text user "GND" (at 7.62 7.62 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp 2a847be3-42ad-45f3-a9f3-dc3305ba8db4)
  )
  (fp_text user "SCL" (at 7.62 15.24 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp 9f723913-5272-492a-bac8-6af4ca2a8f3b)
  )
  (fp_text user "SDA" (at 7.62 12.7 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp b55ebb0d-085f-4d5c-a341-963f34825691)
  )
  (fp_text user "#1" (at 0 5.08 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)) (justify top))
    (tstamp c733450b-6d87-4e3c-8fd2-a1f03dc40109)
  )
  (fp_text user "#3" (at 5.08 5.08 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)) (justify top))
    (tstamp fa438551-b005-47cf-b59d-623d10a0e488)
  )
  (fp_text user "I2C" (at 2.54 17.78 unlocked) (layer "F.SilkS" knockout)
      (effects (font (size 1 1) (thickness 0.2) bold) (justify bottom))
    (tstamp fc487470-f46c-45ca-a9f1-5b449c30c807)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 66068ab2-a7ec-4899-a895-f04295fcf364)
  )
  (pad "GND" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 5b9c140e-084a-4b77-8d8c-d049a53630cf))
  (pad "GND" thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 7851c28d-6063-4548-834b-a845eadc7638))
  (pad "GND" thru_hole oval (at 5.08 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp ec6760b1-789a-4ea9-ab25-f4073c461766))
  (pad "SCL" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 1ebdfecc-7c29-46ed-a0e0-dd467f86b5c3))
  (pad "SCL" thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 4cb829c8-512c-46e2-b9f8-0a0b134921ca))
  (pad "SCL" thru_hole oval (at 5.08 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 8606ae3a-d8a3-4bb0-b892-0f8b85472fa6))
  (pad "SDA" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 5849b506-291c-413b-9309-1ebc8bc1ef39))
  (pad "SDA" thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 8f667479-820f-445f-a9f0-b3ba84a02d4a))
  (pad "SDA" thru_hole oval (at 5.08 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 2823a1cf-7bf9-4fa1-aada-44b1492883b9))
  (pad "Vcc" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp a0190172-0af1-482f-9650-9ba3dde28d4d))
  (pad "Vcc" thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp af03e0fd-7431-4705-8356-859609fc800c))
  (pad "Vcc" thru_hole oval (at 5.08 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 868e6d34-b5a5-4e1e-a5bf-2e0c1b1a4d11))
)
