(footprint "CONN-ESP32-WROOM-Adapter-Legacy-v3"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "ESP32-WROOM-Adapter")
	(tags "ESP32-D0WD Espressif ESP32-WROOM")
	(property "Reference" "ESP32-D**"
		(at -10.61 3.7 90)
		(layer "F.SilkS")
		(uuid "daa5e4ac-a759-4bcc-b120-37e70b41461b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "CONN-ESP32-WROOM-Adapter-Legacy-v3"
		(at 0 11.5 0)
		(layer "F.Fab")
		(uuid "8233f24a-c962-47f7-beb1-dee7c612f0ea")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2b0bccdf-3ef3-409e-a1af-bcb355114cf3")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "1d10067e-286c-484a-9226-7fe741c3b86a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "06672e7a-21d6-4e58-bafb-e24e7d07ac77")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -17.6 -10.6854)
		(end -17.6 20.9)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0a5e460b-de19-42b6-bcac-037b78af5b1b")
	)
	(fp_line
		(start -9.12 -15.86)
		(end -9.12 -9.445)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "245b6f59-030f-4a95-b2db-9d20824f7753")
	)
	(fp_line
		(start -9.12 -15.86)
		(end 9.12 -15.86)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "45b06861-f57b-4b05-9a2c-93d1fadf1aa1")
	)
	(fp_line
		(start -9.12 -9.445)
		(end -9.5 -9.445)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "de643e0e-0faf-407a-9aa9-a15486adb340")
	)
	(fp_line
		(start -9.12 9.1)
		(end -9.12 9.88)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6a5e67ae-5958-415f-a0b8-ff4814232f23")
	)
	(fp_line
		(start -9.12 9.88)
		(end -8.12 9.88)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e97b2722-bbcc-4ed4-bb20-d121b8b394ff")
	)
	(fp_line
		(start 9.12 -15.86)
		(end 9.12 -9.445)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "746a8915-b328-4245-bfb5-7dae79585cdf")
	)
	(fp_line
		(start 9.12 9.1)
		(end 9.12 9.88)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "458bcbae-8b74-4755-9861-38d895e5d533")
	)
	(fp_line
		(start 9.12 9.88)
		(end 8.12 9.88)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9cdeb24d-f07f-449a-bdb0-40dceec536d8")
	)
	(fp_line
		(start 15.8854 22.6)
		(end -15.7 22.6)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "fd0c8750-064d-457d-a15d-fd53d0ef4f67")
	)
	(fp_line
		(start 17.5 -10.8)
		(end 17.5 20.7854)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "07f30f64-77ce-445e-8d9c-994b101d21d4")
	)
	(fp_arc
		(start -17.6 -10.6854)
		(mid -15.117897 -12.365818)
		(end -14.527166 -9.427166)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b884fea9-2931-4d8d-ab4f-e5eebcf3ccda")
	)
	(fp_arc
		(start -15.700001 22.60263)
		(mid -17.00953 22.080265)
		(end -17.6 20.8)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "4ed29c57-0495-40d3-ac5d-49740d1d3614")
	)
	(fp_arc
		(start 14.595841 -9.495841)
		(mid 15.10238 -12.253486)
		(end 17.499999 -10.8)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6ba210ad-ca96-4c06-80c5-907290cae3e6")
	)
	(fp_arc
		(start 17.5 20.7854)
		(mid 17.071898 22.033759)
		(end 15.880748 22.601944)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "65de2f07-f35c-46e0-82d3-9720c3538b79")
	)
	(fp_line
		(start -17.8054 20.86)
		(end -17.8054 -10.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "6442d147-51f3-46dd-8770-abb230e77bb9")
	)
	(fp_line
		(start -15.8054 -12.7)
		(end 15.78 -12.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "87cbd564-0194-4d71-ba0c-189e22774748")
	)
	(fp_line
		(start 15.78 22.86)
		(end -15.8054 22.86)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "fdf15341-cbcc-4be7-a434-def43bdc71e7")
	)
	(fp_line
		(start 17.78 -10.7)
		(end 17.78 20.86)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "3a249ad1-2f9f-4e73-817e-e19e386bb2c7")
	)
	(fp_arc
		(start -17.8054 -10.7)
		(mid -17.219614 -12.114214)
		(end -15.8054 -12.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "5e3c13f1-3c66-42e7-aa53-8dcddcd437b4")
	)
	(fp_arc
		(start -15.8054 22.86)
		(mid -17.219614 22.274214)
		(end -17.8054 20.86)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "f2af26eb-f516-4aaa-9655-5e7c978dee9a")
	)
	(fp_arc
		(start 15.78 -12.7)
		(mid 17.194214 -12.114214)
		(end 17.78 -10.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "7f5cf0a8-0b1a-49bb-8c1e-cbeb2769ab19")
	)
	(fp_arc
		(start 17.78 20.86)
		(mid 17.194214 22.274214)
		(end 15.78 22.86)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "92bf65ae-96d4-47b4-9dc9-0a8f10a74e44")
	)
	(fp_circle
		(center -15.805401 -10.700001)
		(end -14.805401 -10.700001)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "Edge.Cuts")
		(uuid "90cab467-7a34-4cd4-8a71-104ab03b815b")
	)
	(fp_circle
		(center -15.805401 20.860001)
		(end -14.805401 20.860001)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "Edge.Cuts")
		(uuid "979f6e03-94bc-481d-b671-5d7448ad2c74")
	)
	(fp_circle
		(center 15.78 -10.7)
		(end 16.78 -10.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "Edge.Cuts")
		(uuid "a78d0663-30a3-4ceb-b52d-62fe15cd0ee3")
	)
	(fp_circle
		(center 15.78 20.86)
		(end 16.78 20.86)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "Edge.Cuts")
		(uuid "590f40e9-fa75-4847-ab31-8cf44d94d18d")
	)
	(fp_text user "! 3.3V ONLY !"
		(at 0.1 15.6 0)
		(unlocked yes)
		(layer "B.SilkS")
		(uuid "50bab6ac-4dc5-44ec-9738-2a3a19e7e060")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
			(justify mirror)
		)
	)
	(fp_text user "2024-07-24"
		(at 0 22 0)
		(unlocked yes)
		(layer "B.SilkS")
		(uuid "8fb6ce15-ec65-4102-915f-c9995943391f")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify bottom mirror)
		)
	)
	(fp_text user "by: Alexander Bobkov"
		(at -2 2 -45)
		(unlocked yes)
		(layer "B.SilkS")
		(uuid "cb9c6598-a0a9-4a8d-a250-9581ef5249b3")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify mirror)
		)
	)
	(fp_text user "ESP32-WROOM Legacy Adapter v3"
		(at 0 20 0)
		(unlocked yes)
		(layer "B.SilkS")
		(uuid "d6d33bcd-ae52-426e-a6cc-389840c16844")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify bottom mirror)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "0bb61328-94b0-4200-94ed-ff0b1fe2f817")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at -15.24 -7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c45ebe57-e6a1-48ed-82e9-d85a7e3d9183")
	)
	(pad "2" thru_hole circle
		(at -12.7 -7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5af1219a-7de4-45c7-baef-65bd13f10950")
	)
	(pad "3" thru_hole circle
		(at -15.24 -5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9f5d6520-35da-4d3d-9b97-f30248e1aab6")
	)
	(pad "4" thru_hole circle
		(at -12.7 -5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "494912f4-a3e1-41f1-b26d-3bae2c057fac")
	)
	(pad "5" thru_hole circle
		(at -15.24 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "eb7c2c4d-49cb-49c1-94f9-2237cf11208b")
	)
	(pad "6" thru_hole circle
		(at -12.7 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "449fd6ba-6438-4d50-ad14-d12a2d165149")
	)
	(pad "7" thru_hole circle
		(at -15.24 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "99458874-47b7-4093-8294-c3c8efa08a79")
	)
	(pad "8" thru_hole circle
		(at -12.7 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4dcef257-226c-4872-88c1-51513558ce76")
	)
	(pad "9" thru_hole circle
		(at -15.24 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1312447d-12be-4802-90bb-c49735fc43a7")
	)
	(pad "10" thru_hole circle
		(at -12.7 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7f186338-bf65-4204-a67d-9a6b5e81014a")
	)
	(pad "11" thru_hole circle
		(at -15.24 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "76e241f8-07d3-4f70-884b-1131ce586b1b")
	)
	(pad "12" thru_hole circle
		(at -12.7 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cbb0efd9-335e-4e61-a55e-e6613c350c3c")
	)
	(pad "13" thru_hole circle
		(at -15.24 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "dc815df4-c4e8-4659-9ee6-fcb18e012f23")
	)
	(pad "14" thru_hole circle
		(at -12.7 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3a2543d3-1bbd-4c49-9f26-b400f7ce92d4")
	)
	(pad "15" thru_hole circle
		(at -10.16 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "acdbb381-8dc6-4902-ae61-804129178435")
	)
	(pad "16" thru_hole circle
		(at -7.62 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "faaf0cae-4f14-4f21-a8f9-fe1add4fb828")
	)
	(pad "17" thru_hole circle
		(at -5.08 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1be5bc3f-d96f-48dd-84f6-357a7ad781f3")
	)
	(pad "18" thru_hole circle
		(at -2.54 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "58639f95-41b1-4323-8be0-a7044e29023e")
	)
	(pad "19" thru_hole circle
		(at 0 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "08558148-5847-4e26-9bad-10edc3894cc0")
	)
	(pad "20" thru_hole circle
		(at 2.54 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5fdefa29-7d44-4658-8dec-ad90950cc1e6")
	)
	(pad "21" thru_hole circle
		(at 5.08 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b5041c29-e488-4dfd-b266-d3f157f92fce")
	)
	(pad "22" thru_hole circle
		(at 7.62 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a1f27f14-7a30-4887-8ca3-526d79d8032c")
	)
	(pad "23" thru_hole circle
		(at 10.16 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "379aac43-3756-44b3-8970-ef0cc6bc7a5c")
	)
	(pad "24" thru_hole circle
		(at 12.7 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6bb65553-1cc3-41c1-9533-6ebe08f6dc00")
	)
	(pad "25" thru_hole circle
		(at 12.7 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "00a83e5f-c179-4f74-93b9-f946db4fffeb")
	)
	(pad "25" thru_hole circle
		(at 15.24 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3a22c102-467d-45f1-b10f-34f65bf14d4b")
	)
	(pad "26" thru_hole circle
		(at 12.7 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bcb7df82-3ab6-48dc-8b29-d99e00bf8ac7")
	)
	(pad "27" thru_hole circle
		(at 15.24 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fd348198-59e5-4c8f-8f8e-cf49b57f89bb")
	)
	(pad "28" thru_hole circle
		(at 12.7 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "46b70e9e-8b46-4dc4-9c6b-5830ce38e486")
	)
	(pad "29" thru_hole circle
		(at 15.24 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9b7267e3-8859-4a0c-a0e7-0068ed9d947e")
	)
	(pad "30" thru_hole circle
		(at 12.7 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3e010dcc-3008-44e3-91c2-d7d4d6fbd230")
	)
	(pad "31" thru_hole circle
		(at 15.24 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a1484b20-4e4e-4b59-bfc6-865b836b2a4e")
	)
	(pad "32" thru_hole circle
		(at 12.7 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0fa97bae-07e6-4b92-963a-cbe479f9ffc0")
	)
	(pad "33" thru_hole circle
		(at 15.24 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5ce89063-05dd-41df-95f5-3ee9b2d2e56a")
	)
	(pad "34" thru_hole circle
		(at 12.7 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "31ba038b-702a-477f-a295-a53867991cee")
	)
	(pad "35" thru_hole circle
		(at 15.24 -5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3cbf4e31-c0e2-4e73-aa44-86d5c84e984e")
	)
	(pad "36" thru_hole circle
		(at 12.7 -5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a2cbf51c-a5bb-4e37-a25a-66322236c1e5")
	)
	(pad "37" thru_hole circle
		(at 15.24 -7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b71a6f32-6bee-4ce4-8412-0d3ba9cf856d")
	)
	(pad "38" thru_hole circle
		(at 12.7 -7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3d9846de-9c93-4df2-8e1f-1d14d705a288")
	)
	(pad "38" thru_hole circle
		(at 15.24 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "00d2ce8b-53ea-45c9-bd1e-fb557e73837c")
	)
	(model "${KICAD6_3DMODEL_DIR}/RF_Module.3dshapes/ESP32-WROOM-32D.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "C:/Users/alex/github/KiCAD-Libraries/ESP32-WROOM-32UE-N16.STEP"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
