(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "217175-0001" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 29.21 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "217175-0001" (at 29.21 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "2171750001" (at 29.21 -94.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://www.molex.com/pdm_docs/sd/2171750001_sd.pdf" (at 29.21 -194.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "Connector USB Type C Female 6Positions 0.5mm Right Angle SMT Embossed T/R - Tape and Reel" (at 29.21 -294.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "3.46" (at 29.21 -394.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "Molex" (at 29.21 -494.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "217175-0001" (at 29.21 -594.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "538-217175-0001" (at 29.21 -694.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Molex/217175-0001?qs=DRkmTr78QARWJMiqNnldSg%3D%3D" (at 29.21 -794.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Part Number" "" (at 29.21 -894.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Price/Stock" "" (at 29.21 -994.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 2.54)
      (end 27.94 -12.7)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "CC1" (effects (font (size 1.27 1.27))))
      (number "A5" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "VBUS_1" (effects (font (size 1.27 1.27))))
      (number "A9" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "GND_1" (effects (font (size 1.27 1.27))))
      (number "A12" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "CC2" (effects (font (size 1.27 1.27))))
      (number "B5" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -10.16 0) (length 5.08)
      (name "VBUS_2" (effects (font (size 1.27 1.27))))
      (number "B9" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 0 180) (length 5.08)
      (name "GND_2" (effects (font (size 1.27 1.27))))
      (number "B12" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -2.54 180) (length 5.08)
      (name "MH1" (effects (font (size 1.27 1.27))))
      (number "MH1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -5.08 180) (length 5.08)
      (name "MH2" (effects (font (size 1.27 1.27))))
      (number "MH2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -7.62 180) (length 5.08)
      (name "MH3" (effects (font (size 1.27 1.27))))
      (number "MH3" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 33.02 -10.16 180) (length 5.08)
      (name "MH4" (effects (font (size 1.27 1.27))))
      (number "MH4" (effects (font (size 1.27 1.27))))
    )
  )
)
