(footprint "Conn_I2C"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "8060404d-7584-4986-83fc-8fdc66016fdb")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Conn_I2C"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "ba0e9860-90bb-4e1f-9729-155a34948ea8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8e8a42fe-9e40-4832-a4aa-7e5928aac47e")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1497f289-eb66-4470-86c0-feeda8b3c785")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "30f318fc-d15e-4738-b6f7-0b91b39702d5")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr through_hole)
	(fp_text user "SCL"
		(at 2.54 15.24 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "1a795a35-b22a-43f3-a486-b1063021684d")
		(effects
			(font
				(size 0.8 1)
				(thickness 0.1)
			)
		)
	)
	(fp_text user "SDA"
		(at 2.54 12.7 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "8a205637-b83e-48fc-91ad-62a29ce98930")
		(effects
			(font
				(size 0.8 1)
				(thickness 0.1)
			)
		)
	)
	(fp_text user "GND"
		(at 2.54 7.62 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "9008a3ab-7c09-42ca-a8fd-38edf4f42cfa")
		(effects
			(font
				(size 0.8 1)
				(thickness 0.1)
			)
		)
	)
	(fp_text user "Vcc"
		(at 2.54 10.16 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "f6169012-cb39-4d0e-b154-87889a874df6")
		(effects
			(font
				(size 0.8 1)
				(thickness 0.1)
			)
		)
	)
	(fp_text user "I2C"
		(at 0 17.78 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
		(uuid "fc487470-f46c-45ca-a9f1-5b449c30c807")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "66068ab2-a7ec-4899-a895-f04295fcf364")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "GND" thru_hole rect
		(at 0 7.62)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5c41aac6-f663-494d-a0f4-636d0c39bea1")
	)
	(pad "SCL" thru_hole circle
		(at 0 15.24)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2c743884-b986-4e77-bf71-8d8c8664b7a4")
	)
	(pad "SDA" thru_hole circle
		(at 0 12.7)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c26bce4f-7c1b-4a87-92f9-aba6c298f7db")
	)
	(pad "Vcc" thru_hole circle
		(at 0 10.16)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "09c4c65c-17f1-4721-bfd6-fa35f3058def")
	)
)