(footprint "Conn_ESP32_WROOM-DevKit"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "ESP32 DevBoard 38 pins")
	(tags "ESP32 DevBoard 38")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b402446d-1b7a-401c-b7a8-b751312eca93")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Conn_ESP32_WROOM-DevKit"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "83dc45d7-073a-4439-ad4e-af6f67e174d7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d74e5f70-57c2-4394-8381-0bb5b483160b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "43789d1f-6fe6-45a8-921f-6c30beb72c22")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "ESP32 DevBoard 38 pins"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6f9c5a9d-5651-41cd-927e-347ef1c66b59")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -2.54 -50.8)
		(end 2.54 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "e0741dfb-0c23-4b69-8b45-371e45b772d7")
	)
	(fp_rect
		(start 7.62 -50.8)
		(end 17.78 -48.26)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "828f0772-bddb-48c3-b4f9-ed96987ae6a3")
	)
	(fp_rect
		(start 22.86 -50.8)
		(end 27.94 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "87043fcf-24c3-4370-a43d-a8189f433afc")
	)
	(fp_rect
		(start -2.54 -50.8)
		(end 27.94 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "Edge.Cuts")
		(uuid "0c55cdcc-7d7f-482a-91c9-34e51e4bb97c")
	)
	(fp_rect
		(start -2.54 -50.8)
		(end 2.54 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "Margin")
		(uuid "e46f453a-665f-487b-ae6a-533f5f24aaec")
	)
	(fp_rect
		(start 22.86 -50.8)
		(end 27.94 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "Margin")
		(uuid "d4e4cb92-84ba-4b86-a40b-084f62c4c27c")
	)
	(fp_rect
		(start -2.54 -50.8)
		(end 27.94 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "01479acf-8df2-427a-a135-b782eb53fd01")
	)
	(fp_text user "USB"
		(at 12.7 -48.26 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "c72c1f94-9e06-4cfc-92fa-0ccda1d39ad4")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "287892f0-6b80-4e42-a2ea-213c0741645d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 -48.26)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b1fd2bdb-d928-4ae6-9a54-c15fb98a28f7")
	)
	(pad "2" thru_hole circle
		(at 0 -45.72)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1dcb9034-ea2d-46c1-92a7-0cf495881989")
	)
	(pad "3" thru_hole circle
		(at 0 -43.18)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "68bbd01c-2871-4c06-b625-0aae35094dd5")
	)
	(pad "4" thru_hole circle
		(at 0 -40.64)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a91351a4-5128-4c49-b9a9-65e97713b7b0")
	)
	(pad "5" thru_hole circle
		(at 0 -38.1)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "21a3e36e-c9a3-45b5-b802-bf30a0c6ccaa")
	)
	(pad "6" thru_hole circle
		(at 0 -35.56)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c99ead02-21ae-487d-960c-804be85b5460")
	)
	(pad "7" thru_hole circle
		(at 0 -33.02)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "83e9a5c1-7b2b-42b9-9edf-4af0c07538ca")
	)
	(pad "8" thru_hole circle
		(at 0 -30.48)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7466d4b0-3525-408c-9f45-d4c22d3fb135")
	)
	(pad "9" thru_hole circle
		(at 0 -27.94)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "765e2cea-fad7-435a-9145-e621cea13261")
	)
	(pad "10" thru_hole circle
		(at 0 -25.4)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4681cff6-0a7a-4c1d-bd21-725a62cb2791")
	)
	(pad "11" thru_hole circle
		(at 0 -22.86)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a5540c1e-b0f0-49d5-bc57-79e03af0e9f5")
	)
	(pad "12" thru_hole circle
		(at 0 -20.32)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "522de160-1cf6-48c2-8e89-6b9e8e33a3c7")
	)
	(pad "13" thru_hole circle
		(at 0 -17.78)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3a5823f1-717f-410b-afda-bf30eff2280e")
	)
	(pad "14" thru_hole circle
		(at 0 -15.24)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "51dfe943-0014-49f9-95f0-92fca967b9bc")
	)
	(pad "15" thru_hole circle
		(at 0 -12.7)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f6a1dc90-684b-4321-a759-b04743b9adbb")
	)
	(pad "16" thru_hole circle
		(at 0 -10.16)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f1ff8040-2215-4a2d-973e-34e9e511095b")
	)
	(pad "17" thru_hole circle
		(at 0 -7.62)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b294be77-90e0-4ee7-baf0-6a238cb72c80")
	)
	(pad "18" thru_hole circle
		(at 0 -5.08)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2e7b1810-c9ac-45a7-b7d0-9b62dde5eaae")
	)
	(pad "19" thru_hole circle
		(at 0 -2.54)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b4fd9c88-1f14-4431-a5ae-84a8d811d928")
	)
	(pad "20" thru_hole circle
		(at 25.4 -2.54)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b0ca4a31-4efb-4f20-bd6b-8e5784b20033")
	)
	(pad "21" thru_hole circle
		(at 25.4 -5.08)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1ff77abc-768b-41e3-9eb6-4a46e72a59c4")
	)
	(pad "22" thru_hole circle
		(at 25.4 -7.62)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a40e4634-2f3c-4730-bf2e-7a604bb344f6")
	)
	(pad "23" thru_hole circle
		(at 25.4 -10.16)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a39aeba0-1aea-4ec2-a5fb-18bc3c40fca0")
	)
	(pad "24" thru_hole circle
		(at 25.4 -12.7)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5264d910-51c7-4b34-8730-fbeacd858f53")
	)
	(pad "25" thru_hole circle
		(at 25.4 -15.24)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "864fca95-a77e-4c56-a565-a90c9920fe0d")
	)
	(pad "26" thru_hole circle
		(at 25.4 -17.78)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5411152c-e7d0-45c4-b5a2-d08b842d6e32")
	)
	(pad "27" thru_hole circle
		(at 25.4 -20.32)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ddfce733-f66a-41d5-8fb5-5b03d3c1d05f")
	)
	(pad "28" thru_hole circle
		(at 25.4 -22.86)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bf331f1f-97e8-4e8b-b5a0-d80d8e5cbc32")
	)
	(pad "29" thru_hole circle
		(at 25.4 -25.4)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7f13fa12-e2c3-48b3-90d0-03dc21f7858b")
	)
	(pad "30" thru_hole circle
		(at 25.4 -27.94)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "92f6a64b-8397-4498-ad3d-66dde1d56ee4")
	)
	(pad "31" thru_hole circle
		(at 25.4 -30.48)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "364644f8-c29e-4b6a-a46f-5922e8f6cf0f")
	)
	(pad "32" thru_hole circle
		(at 25.4 -33.02)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "adfdbf32-6e29-4e86-9491-794ee9cbe3cb")
	)
	(pad "33" thru_hole circle
		(at 25.4 -35.56)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "642d1db4-a414-45f4-bb44-4821eee71ae0")
	)
	(pad "34" thru_hole circle
		(at 25.4 -38.1)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "69c515bd-1bb6-4247-bf1c-d32a1a8c270f")
	)
	(pad "35" thru_hole circle
		(at 25.4 -40.64)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "61f611a1-a301-4736-bffc-c826e2ff638b")
	)
	(pad "36" thru_hole circle
		(at 25.4 -43.18)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "231d73bf-85ca-4470-88b2-808a3b8a883d")
	)
	(pad "37" thru_hole circle
		(at 25.4 -45.72)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7e679ad3-dd31-4d74-a98e-bdeb1c1f6294")
	)
	(pad "38" thru_hole circle
		(at 25.4 -48.26)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0156ee9a-586e-40b8-bb69-5e4dd7c6efd3")
	)
)