(footprint "SW_SPST_6x3"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(tags "SPST button tactile switch")
	(property "Reference" "REF**"
		(at 0 -4 0)
		(layer "F.SilkS")
		(uuid "ac46ecd6-c91a-4697-9867-f96e29e4f26b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SW_SPST_6x3"
		(at 0 3 0)
		(layer "F.Fab")
		(uuid "7941cf56-4e7e-427e-a7f8-1a95b943068a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a85283e7-d45e-493c-be43-75d2ecac0afc")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b546b94d-58ff-41a0-a38d-9ba6224e33d3")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "SPST button tactile switch"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "469e19ea-e1a3-410a-8c20-09cfa4c0197f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3.06 -1.81)
		(end 3.06 -1.81)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "44f60bfd-f7f6-4f0e-9fb5-b246a542426c")
	)
	(fp_line
		(start -3.06 1.81)
		(end -3.06 -1.81)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b11f6328-00f6-4e24-b419-a862c2f5381b")
	)
	(fp_line
		(start 3.06 -1.81)
		(end 3.06 1.81)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "efac0af3-3387-4112-8164-229d2a0a1786")
	)
	(fp_line
		(start 3.06 1.81)
		(end -3.06 1.81)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e009832c-d058-4e34-960c-764f9ec75851")
	)
	(fp_line
		(start -5.95 -2)
		(end -5.95 2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d24074a6-cbe0-4400-92f8-95e5a5e1c0af")
	)
	(fp_line
		(start -5.95 -2)
		(end 5.95 -2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "eefb9e6e-f288-4c7c-ba6c-215f4b19047c")
	)
	(fp_line
		(start -5.95 2)
		(end 5.95 2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "659a6da1-bdaf-4895-959b-0d0427369fa3")
	)
	(fp_line
		(start 5.95 -2)
		(end 5.95 2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3128de98-d55a-42bc-84b0-eccbc3670429")
	)
	(fp_line
		(start -3 -1.75)
		(end -3 1.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9a5e5743-4779-410a-852d-a31067d08eed")
	)
	(fp_line
		(start -3 -1.75)
		(end 3 -1.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d7154d3c-b401-411c-bfc5-ddcab6c95d30")
	)
	(fp_line
		(start -3 1.75)
		(end 3 1.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "64cc5d4d-ce68-420f-9407-1cf938a340e2")
	)
	(fp_line
		(start -1.75 -1)
		(end 1.75 -1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "45336baf-c305-4036-964d-5c5ce6180c3d")
	)
	(fp_line
		(start -1.75 1)
		(end -1.75 -1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "36b7d042-07b1-4a12-87be-b8af13cc6e98")
	)
	(fp_line
		(start -1.5 -0.8)
		(end -1.5 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ee24a63b-8b49-4127-b37c-8bc10b140a4f")
	)
	(fp_line
		(start -1.5 -0.8)
		(end 1.5 -0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8ed2fb8c-88cd-4bf6-9934-2366a1be9ceb")
	)
	(fp_line
		(start -1.5 0.8)
		(end 1.5 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f185f4c9-eed7-4dc4-8232-152341f5088f")
	)
	(fp_line
		(start 1.5 -0.8)
		(end 1.5 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ffc3b6fb-0bb8-48ad-bb8c-5264c960ae9e")
	)
	(fp_line
		(start 1.75 -1)
		(end 1.75 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "bb4cfb6f-1db2-4694-b194-060041562a7c")
	)
	(fp_line
		(start 1.75 1)
		(end -1.75 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "88c019c9-ebc4-4554-8a3d-72fedfa38fd3")
	)
	(fp_line
		(start 3 -1.75)
		(end 3 1.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "69002332-c242-4dd5-b10c-1a1021a85689")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.6 0)
		(layer "F.Fab")
		(uuid "666ba2b8-0fd0-40eb-9ee7-3d675db72415")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -4.59 0)
		(size 2.18 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "15a9016f-fab5-4f6e-911b-c6b27c5a8562")
	)
	(pad "2" smd rect
		(at 4.59 0)
		(size 2.18 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "32e4f653-9a48-444f-990e-41eabf874034")
	)
	(model "${KICAD8_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_FSMSM.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
