(footprint "Conn_ESP32_WROOM-DevKit-38pins"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "ESP32 DevBoard 38 pins")
	(tags "ESP32 DevBoard 38")
	(property "Reference" "REF**"
		(at 0 0.25 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b402446d-1b7a-401c-b7a8-b751312eca93")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Conn_ESP32_WROOM-DevKit-38pins"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "83dc45d7-073a-4439-ad4e-af6f67e174d7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d74e5f70-57c2-4394-8381-0bb5b483160b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "43789d1f-6fe6-45a8-921f-6c30beb72c22")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "ESP32 DevBoard 38 pins"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6f9c5a9d-5651-41cd-927e-347ef1c66b59")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.33 -46.99)
		(end -1.33 -1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "81b22ad0-7ff9-4219-a48e-bffaa647716f")
	)
	(fp_line
		(start -1.33 -46.99)
		(end 1.33 -46.99)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b8c74aa6-3241-4f5b-8880-2ba0eab471fd")
	)
	(fp_line
		(start -1.33 -1.21)
		(end 1.33 -1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "672f7535-cd12-4515-a7e2-bdd345b4fa88")
	)
	(fp_line
		(start 0 -49.59)
		(end 1.33 -49.59)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4d5645b8-b525-485e-9659-645fc426f12d")
	)
	(fp_line
		(start 1.33 -49.59)
		(end 1.33 -48.26)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "47521411-2387-4459-a790-743d02eb8624")
	)
	(fp_line
		(start 1.33 -46.99)
		(end 1.33 -1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "514125e7-3605-48b6-9032-e268f996ab3c")
	)
	(fp_line
		(start 24.07 -1.21)
		(end 26.73 -1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8af5594f-efce-4bd3-9daa-01df91fa9830")
	)
	(fp_line
		(start 24.075 -49.6)
		(end 24.07 -1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f6881115-e779-4960-9c15-389754d6c25f")
	)
	(fp_line
		(start 24.075 -49.6)
		(end 26.675 -49.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e6106870-f0c4-4eb4-8854-2e06ad7a32fa")
	)
	(fp_line
		(start 26.675 -49.6)
		(end 26.73 -1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f871e0b9-2d1c-4394-95a6-19b6c64e7cf4")
	)
	(fp_rect
		(start -1.75 -50)
		(end 1.75 -0.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "e0741dfb-0c23-4b69-8b45-371e45b772d7")
	)
	(fp_rect
		(start 9.92 -50)
		(end 15.18 -47.86)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "828f0772-bddb-48c3-b4f9-ed96987ae6a3")
	)
	(fp_rect
		(start 23.75 -50)
		(end 27 -0.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "87043fcf-24c3-4370-a43d-a8189f433afc")
	)
	(fp_line
		(start -1.8 -50.06)
		(end 1.75 -50.06)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "af8796f4-cfe2-4805-8980-2a5654be8515")
	)
	(fp_line
		(start -1.8 -0.76)
		(end -1.8 -50.06)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "63a4b27e-13a8-4e8a-943d-f8cb5efdc81d")
	)
	(fp_line
		(start 1.75 -50.06)
		(end 1.75 -0.76)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d9c67c54-bf5f-4755-9121-33e4565c4e56")
	)
	(fp_line
		(start 1.75 -0.76)
		(end -1.8 -0.76)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "99df5db0-0bb3-41bb-b2ee-e61b9fc35a8c")
	)
	(fp_line
		(start 23.6 -50.06)
		(end 27.15 -50.06)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c0fd0227-21fb-450f-9970-89f6de57ebe0")
	)
	(fp_line
		(start 23.6 -0.76)
		(end 23.6 -50.06)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "46c6913f-63c1-4989-a5c1-b6ae02b5bed2")
	)
	(fp_line
		(start 27.15 -50.06)
		(end 27.15 -0.76)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5a40440d-ea22-43a2-bca6-63f4bcbc9069")
	)
	(fp_line
		(start 27.15 -0.76)
		(end 23.6 -0.76)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "eafeb8d4-1ea1-4188-9b17-0d4a0877d369")
	)
	(fp_line
		(start -1.27 -49.53)
		(end 0.635 -49.53)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b182f215-310f-4bdb-94fc-f3e950ae5eec")
	)
	(fp_line
		(start -1.27 -1.27)
		(end -1.27 -49.53)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d4d51883-7af2-4363-b9a2-2d893bec0992")
	)
	(fp_line
		(start 0.635 -49.53)
		(end 1.27 -48.895)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c2650ce7-6082-405c-a1d7-4211ce2bf2f6")
	)
	(fp_line
		(start 1.27 -48.895)
		(end 1.27 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1bb77174-43e0-4062-b703-13f37f0c66f4")
	)
	(fp_line
		(start 1.27 -1.27)
		(end -1.27 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7b730dde-bebc-4857-8f99-4f4e8c67fb05")
	)
	(fp_line
		(start 24.13 -49.53)
		(end 26.035 -49.53)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5f289aee-81cc-4fc7-9ca3-aab191b8005a")
	)
	(fp_line
		(start 24.13 -1.27)
		(end 24.13 -49.53)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b00e1b43-bd31-4a4e-bb67-c1157a88f2f4")
	)
	(fp_line
		(start 26.67 -48.895)
		(end 26.67 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4e9a3ce2-d3ab-4369-ab5d-c3bff7ffcdf8")
	)
	(fp_line
		(start 26.67 -1.27)
		(end 24.13 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e4764241-584b-4e29-9fe5-9f6cf7a26e62")
	)
	(fp_text user "GND"
		(at -3 -2.5 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
		(uuid "021b492e-364b-4cfa-9fad-29dc062f947c")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.2)
				(bold yes)
			)
			(justify right)
		)
	)
	(fp_text user "5V"
		(at 28 -48.2 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
		(uuid "78894cdf-67d0-478a-8895-77a80e852bb9")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.2)
				(bold yes)
			)
			(justify left)
		)
	)
	(fp_text user "3V3"
		(at 28 -2.6 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
		(uuid "81203640-3bac-46c1-9d72-c4c13a848f11")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.2)
				(bold yes)
			)
			(justify left)
		)
	)
	(fp_text user "GND"
		(at 28 -35.5 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
		(uuid "c0f61a3c-02ea-4df6-b1af-16d3a9abadb5")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.2)
				(bold yes)
			)
			(justify left)
		)
	)
	(fp_text user "USB"
		(at 12.55 -48.26 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "c72c1f94-9e06-4cfc-92fa-0ccda1d39ad4")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(fp_text user "5V"
		(at -4.7 -17.7 0)
		(unlocked yes)
		(layer "F.SilkS" knockout)
		(uuid "d58ff46d-d1ff-4d8a-bdeb-965a3af76f6d")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.2)
				(bold yes)
			)
			(justify left)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 3 -25.4 90)
		(layer "F.Fab")
		(uuid "017315f1-05b8-44e7-8d42-467d1c73ad21")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "287892f0-6b80-4e42-a2ea-213c0741645d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 25.4 -25.4 90)
		(layer "F.Fab")
		(uuid "3b6718b2-ff6c-4ff3-9ed4-860171bc610a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 -48.26)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "76e2bcc7-bd44-4642-b826-9a0b0abb409d")
	)
	(pad "2" thru_hole oval
		(at 0 -45.72)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "645c146f-2025-425b-a7b1-624f935cff8c")
	)
	(pad "3" thru_hole oval
		(at 0 -43.18)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8f346474-b23f-40c6-b078-e6f697bc7d74")
	)
	(pad "4" thru_hole oval
		(at 0 -40.64)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d157bfae-799f-4809-8a35-7d80e82408a2")
	)
	(pad "5" thru_hole oval
		(at 0 -38.1)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4234b3ac-ae04-41b2-a11b-cc39d51f4089")
	)
	(pad "6" thru_hole oval
		(at 0 -35.56)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f59fb152-877c-47db-b973-bf7e29350b35")
	)
	(pad "7" thru_hole oval
		(at 0 -33.02)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2a1344db-ae99-4696-8417-4b25e00a87b3")
	)
	(pad "8" thru_hole oval
		(at 0 -30.48)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a376f260-52b9-4ff2-bfb8-9d671e25820b")
	)
	(pad "9" thru_hole oval
		(at 0 -27.94)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "575d844e-a830-46fe-901f-02c1c3db2e11")
	)
	(pad "10" thru_hole oval
		(at 0 -25.4)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8b241345-c1c4-4d61-b170-99be111906e0")
	)
	(pad "11" thru_hole oval
		(at 0 -22.86)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fb334b88-be17-42fe-a374-716b9347e0ce")
	)
	(pad "12" thru_hole oval
		(at 0 -20.32)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "44771395-55d0-449f-afb7-1fc3d82410cf")
	)
	(pad "13" thru_hole oval
		(at 0 -17.78)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6bd1be63-bf5a-41dd-83b6-ce70dd16a8b9")
	)
	(pad "14" thru_hole oval
		(at 0 -15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d658f2f0-121a-44bc-b0b4-aa4f0a51d804")
	)
	(pad "15" thru_hole oval
		(at 0 -12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "84550160-a4a1-41d0-9756-6d355a2b413b")
	)
	(pad "16" thru_hole oval
		(at 0 -10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a1996dc5-27de-4a0e-9a3e-b4f451f83e95")
	)
	(pad "17" thru_hole oval
		(at 0 -7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "82db1716-c441-4453-a3ed-40c22f2b1cd8")
	)
	(pad "18" thru_hole oval
		(at 0 -5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8d458aba-623e-43d5-ab03-879261374fe5")
	)
	(pad "19" thru_hole oval
		(at 0 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8595753b-55e4-4fc4-a2d7-6462f2129746")
	)
	(pad "20" thru_hole oval
		(at 25.4 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "421c4c5a-feb1-4e57-b751-74e36e8a0f76")
	)
	(pad "21" thru_hole oval
		(at 25.4 -5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c0b0e139-49d9-4e4c-b1f9-6ea3ce883b63")
	)
	(pad "22" thru_hole oval
		(at 25.4 -7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fae9d3b5-03d0-4cc0-8d62-68538bc7708f")
	)
	(pad "23" thru_hole oval
		(at 25.4 -10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1cfaf6c0-2f6c-49f4-82e7-6c6179bb477b")
	)
	(pad "24" thru_hole oval
		(at 25.4 -12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "31d6ef3f-dfda-4da1-a9b7-babf047c2db7")
	)
	(pad "25" thru_hole oval
		(at 25.4 -15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e5d45eca-2d3c-4e47-80a6-6da6deaf6a13")
	)
	(pad "26" thru_hole oval
		(at 25.4 -17.78)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "edc30946-6903-4e38-8c89-110fe70a5d17")
	)
	(pad "27" thru_hole oval
		(at 25.4 -20.32)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "69d45fa9-6e4e-426c-820a-9544be5517dc")
	)
	(pad "28" thru_hole oval
		(at 25.4 -22.86)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3b2e94ec-8f3c-4214-8095-3fa33422bf1f")
	)
	(pad "29" thru_hole oval
		(at 25.4 -25.4)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0841f9a8-32a0-4b18-8384-ec70917feff0")
	)
	(pad "30" thru_hole oval
		(at 25.4 -27.94)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7b4a1a0f-63b5-455f-8ea6-811de153b21c")
	)
	(pad "31" thru_hole oval
		(at 25.4 -30.48)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "feb8faae-a66d-4fd7-b095-7a51039ea6a3")
	)
	(pad "32" thru_hole oval
		(at 25.4 -33.02)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ae6f6648-09c0-457c-94c4-651013ff773d")
	)
	(pad "33" thru_hole oval
		(at 25.4 -35.56)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "497c7cb9-4216-43e3-bff8-67978f9d57ba")
	)
	(pad "34" thru_hole oval
		(at 25.4 -38.1)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2841b3ed-15a1-4595-a1c3-5cdb4580ebd6")
	)
	(pad "35" thru_hole oval
		(at 25.4 -40.64)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cc3d9fb3-da7b-48e7-9219-59c3032060bf")
	)
	(pad "36" thru_hole oval
		(at 25.4 -43.18)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cb8b559e-fec7-4a25-abeb-e10873bf36c8")
	)
	(pad "37" thru_hole oval
		(at 25.4 -45.72)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e1938432-62fd-434e-b884-3dd0d0d0f593")
	)
	(pad "38" thru_hole oval
		(at 25.4 -48.15)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e2d19b84-7e59-4824-813e-a81e32f76520")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x19_P2.54mm_Vertical.wrl1"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
