
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "CX60-24S-UNIT" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -15.24 16.51 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "CX60-24S-UNIT" (id 1) (at -15.24 -26.67 0.0)
      (effects (font (size 1.27 1.27)) (justify top left))
    )
    (property "Footprint" "CX60-24S-UNIT:HIROSE_CX60-24S-UNIT" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "5" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "2.6 mm" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Hirose" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "CX60-24S-UNIT_0_0"
      (rectangle (start -15.24 -25.4) (end 15.24 15.24)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin bidirectional line (at -20.32 7.62 0) (length 5.08)
        (name "TX1+"
          (effects (font (size 1.016 1.016)))
        )
        (number "A2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -20.32 5.08 0) (length 5.08)
        (name "TX1-"
          (effects (font (size 1.016 1.016)))
        )
        (number "A3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -20.32 12.7 0) (length 5.08)
        (name "VBUS_A"
          (effects (font (size 1.016 1.016)))
        )
        (number "A4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -20.32 2.54 0) (length 5.08)
        (name "CC"
          (effects (font (size 1.016 1.016)))
        )
        (number "A5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -20.32 0.0 0) (length 5.08)
        (name "D+"
          (effects (font (size 1.016 1.016)))
        )
        (number "A6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -20.32 -2.54 0) (length 5.08)
        (name "D-"
          (effects (font (size 1.016 1.016)))
        )
        (number "A7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -20.32 -5.08 0) (length 5.08)
        (name "SBU1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -20.32 -7.62 0) (length 5.08)
        (name "RX2-"
          (effects (font (size 1.016 1.016)))
        )
        (number "A10"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -20.32 -10.16 0) (length 5.08)
        (name "RX2+"
          (effects (font (size 1.016 1.016)))
        )
        (number "A11"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -20.32 -12.7 0) (length 5.08)
        (name "GNDA"
          (effects (font (size 1.016 1.016)))
        )
        (number "A1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 20.32 7.62 180.0) (length 5.08)
        (name "RX1+"
          (effects (font (size 1.016 1.016)))
        )
        (number "B11"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 20.32 5.08 180.0) (length 5.08)
        (name "RX1-"
          (effects (font (size 1.016 1.016)))
        )
        (number "B10"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 20.32 12.7 180.0) (length 5.08)
        (name "VBUS_B"
          (effects (font (size 1.016 1.016)))
        )
        (number "B4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 20.32 2.54 180.0) (length 5.08)
        (name "SBU2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 20.32 -5.08 180.0) (length 5.08)
        (name "VCONN"
          (effects (font (size 1.016 1.016)))
        )
        (number "B5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 20.32 -7.62 180.0) (length 5.08)
        (name "TX2-"
          (effects (font (size 1.016 1.016)))
        )
        (number "B3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 20.32 -10.16 180.0) (length 5.08)
        (name "TX2+"
          (effects (font (size 1.016 1.016)))
        )
        (number "B2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 20.32 -12.7 180.0) (length 5.08)
        (name "GNDB"
          (effects (font (size 1.016 1.016)))
        )
        (number "B1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -20.32 -20.32 0) (length 5.08)
        (name "SHIELD1"
          (effects (font (size 1.016 1.016)))
        )
        (number "S1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at 20.32 -20.32 180.0) (length 5.08)
        (name "SHIELD2"
          (effects (font (size 1.016 1.016)))
        )
        (number "S3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -20.32 10.16 0) (length 5.08)
        (name "VBUS_A__1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -20.32 -15.24 0) (length 5.08)
        (name "GNDA__1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -20.32 -22.86 0) (length 5.08)
        (name "SHIELD1__1"
          (effects (font (size 1.016 1.016)))
        )
        (number "S2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 20.32 10.16 180.0) (length 5.08)
        (name "VBUS_B__1"
          (effects (font (size 1.016 1.016)))
        )
        (number "B9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 20.32 -15.24 180.0) (length 5.08)
        (name "GNDB__1"
          (effects (font (size 1.016 1.016)))
        )
        (number "B12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at 20.32 -22.86 180.0) (length 5.08)
        (name "SHIELD2__1"
          (effects (font (size 1.016 1.016)))
        )
        (number "S4"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)