(footprint "Conn_ePaper" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Connector for Waveshare 4.2\" e-Paper")
  (tags "ePaper")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 47c0de8e-fd2e-4b8a-9640-ac2f6a98654c)
  )
  (fp_text value "Conn_ePaper" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 91208d68-1471-4cf1-83ae-8a320dbe857a)
  )
  (fp_text user "CLK" (at 2.54 12.7 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp 148ecb74-f7d9-4183-9a56-e51c07233b42)
  )
  (fp_text user "Vcc" (at 2.54 5.08 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp 2ccd2f16-4b56-44ee-9cc1-94f31d7c977a)
  )
  (fp_text user "CS" (at 2.54 15.24 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp 3e3e6f4e-b41a-4b8c-a3b9-a6e7d73a2772)
  )
  (fp_text user "BSY" (at 2.54 22.86 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp 69106f81-4875-4873-aba9-3dd558a850e6)
  )
  (fp_text user "RST" (at 2.54 20.32 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp 859f3ef2-ca79-4da9-a5ff-accb3467eec4)
  )
  (fp_text user "GND" (at 2.54 7.62 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp c056fffb-def1-4534-8d86-edd415e568d0)
  )
  (fp_text user "DC" (at 2.54 17.78 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp c572b78c-694e-4be1-9d5d-8bcde8e3eb71)
  )
  (fp_text user "e-Paper" (at 0 25.4 unlocked) (layer "F.SilkS" knockout)
      (effects (font (size 1 1) (thickness 0.2) bold))
    (tstamp cffac2d2-b0fe-436e-9db8-eba98ee7def6)
  )
  (fp_text user "DIN" (at 2.54 10.16 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp f4153077-210e-4e5a-b7a6-cd9e416c94f0)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2f7d6680-ce9e-4916-8717-e28c22650c16)
  )
  (pad "BUSY" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp d93dc8d9-17e4-470b-81e2-f01e717b2f24))
  (pad "CLK" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp e09bf378-db43-4d10-9155-0d04785cb718))
  (pad "CS" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp a0bd0d68-3e72-4152-99c7-7c928d9a3bdf))
  (pad "DC" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp f0974ada-ddf4-4307-a4ab-04000fecb6bc))
  (pad "DIN" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 3b1c7174-b668-4db1-b53c-a403e5c82cc6))
  (pad "GND" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 53e54d7c-f401-49e3-83cc-34d06c3c8139))
  (pad "RST" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp c0c84827-7e41-49db-97a3-73a5e092425f))
  (pad "Vcc" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 170f761b-9cfc-4864-974f-811c70880c5d))
)
