(footprint "Conn_ESP32-C3-WROOM-02"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -9.035 -14.585 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "c1ef7f4f-d8a5-44f4-ad1d-4b2aec7eccf5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Conn_ESP32-C3-WROOM-02"
		(at 0 20.32 0)
		(layer "F.Fab")
		(uuid "b181fa74-d9b4-4804-9bc1-b081e6bde4bb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at -2.46 -3.5 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "15536f93-f33c-4864-9d98-6e178b43b039")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at -2.46 -3.5 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7dfa6719-3fd2-4897-bc0d-ec5e75a775dd")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at -2.46 -3.5 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "9a131e6a-a466-4751-94ad-e5721b8264e5")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -17.78 -5.08)
		(end -17.78 15.24)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "714c0d54-5e95-430b-86e1-11d11dc4e131")
	)
	(fp_line
		(start -15.24 -7.62)
		(end 10.16 -7.62)
		(stroke
			(width 0.25)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9cc96d90-71da-48bc-acc9-8a33371f4475")
	)
	(fp_line
		(start -15.24 17.78)
		(end 10.16 17.78)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "bb76cd0f-c6d5-4451-90b0-6f2b8e909eeb")
	)
	(fp_line
		(start 12.7 -5.08)
		(end 12.7 15.24)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ab64e8e2-b014-483c-b7cb-35736f8c456e")
	)
	(fp_arc
		(start -17.78 -5.08)
		(mid -17.036051 -6.876051)
		(end -15.24 -7.62)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8a8bb993-9351-414b-92a5-5052904c4071")
	)
	(fp_arc
		(start -15.24 17.78)
		(mid -17.036051 17.036051)
		(end -17.78 15.24)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a03c8451-9aa3-480c-9bbf-21589f90d370")
	)
	(fp_arc
		(start 10.16 -7.62)
		(mid 11.956051 -6.876051)
		(end 12.7 -5.08)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6d8db259-cc08-4998-875c-b7fbd6689735")
	)
	(fp_arc
		(start 12.7 15.24)
		(mid 11.956051 17.036051)
		(end 10.16 17.78)
		(stroke
			(width 0.5)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ec2cf4bf-1779-4400-a505-d3d4a4722a5b")
	)
	(fp_line
		(start -17.78 15.24)
		(end -17.78 -5.08)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "dc0a399e-86b7-4726-a038-1e7730e7ae22")
	)
	(fp_line
		(start -15.24 -7.62)
		(end 10.16 -7.62)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "b1751c00-b900-4b60-91a0-bce747457d36")
	)
	(fp_line
		(start 10.16 17.78)
		(end -15.24 17.78)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "2a50c0b5-62e8-4153-a44e-58b5bab18ebe")
	)
	(fp_line
		(start 12.7 -5.08)
		(end 12.7 15.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "9d82ace1-7e1d-408e-a12b-aeebf47444b8")
	)
	(fp_arc
		(start -17.78 -5.08)
		(mid -17.036051 -6.876051)
		(end -15.24 -7.62)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "65a3d21f-c77e-40a3-b422-39e8b720edd5")
	)
	(fp_arc
		(start -15.24 17.78)
		(mid -17.036051 17.036051)
		(end -17.78 15.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "9840c1a7-2040-4d6e-854d-cb28239d748c")
	)
	(fp_arc
		(start 10.16 -7.62)
		(mid 11.956051 -6.876051)
		(end 12.7 -5.08)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "28231675-c752-460a-91ab-d51cf7dbf7dd")
	)
	(fp_arc
		(start 12.7 15.24)
		(mid 11.956051 17.036051)
		(end 10.16 17.78)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "1eaa7d5e-f35f-40bc-b477-7c8cf2f081e6")
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(uuid "36c075c2-27a0-4fb3-bed3-b03d913725de")
		(pts
			(xy 10.16 17.78) (xy 10.16 -7.62)
		)
		(height 15.24)
		(gr_text "25.4000 mm"
			(at 24.25 5.08 90)
			(layer "Cmts.User")
			(uuid "36c075c2-27a0-4fb3-bed3-b03d913725de")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(uuid "5cda490b-8368-4605-99a9-6bf898d6235b")
		(pts
			(xy -15.24 -5.08) (xy 10.16 -5.08)
		)
		(height -20.32)
		(gr_text "25.4000 mm"
			(at -2.54 -26.55 0)
			(layer "Cmts.User")
			(uuid "5cda490b-8368-4605-99a9-6bf898d6235b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(uuid "e2f57b15-561b-4cc4-a3e4-2a6e23c062fa")
		(pts
			(xy -17.78 15.24) (xy 12.7 15.24)
		)
		(height 12.7)
		(gr_text "30.4800 mm"
			(at -2.54 26.79 0)
			(layer "Cmts.User")
			(uuid "e2f57b15-561b-4cc4-a3e4-2a6e23c062fa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(pad "1" thru_hole rect
		(at -15.24 -5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1fc9f2e5-39c7-426e-b123-548378da993a")
	)
	(pad "2" thru_hole circle
		(at -15.24 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6774307e-1ae8-4563-a337-105bbc7e0497")
	)
	(pad "3" thru_hole circle
		(at -15.24 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5d64747d-a852-42e6-b321-385dd43d0959")
	)
	(pad "4" thru_hole circle
		(at -15.24 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "51d4b505-3fa6-47e7-aab5-47bf622cd946")
	)
	(pad "5" thru_hole circle
		(at -15.24 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4da34b95-ba12-41a8-b201-9026c516407c")
	)
	(pad "6" thru_hole circle
		(at -15.24 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5a056539-f712-4018-8e26-7fb3d287f69c")
	)
	(pad "7" thru_hole circle
		(at -15.24 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cd777b65-609a-464f-a49e-4890fd059058")
	)
	(pad "8" thru_hole circle
		(at -15.24 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4fee6c49-0bdd-44fb-80ce-58a1f7b9d8e6")
	)
	(pad "9" thru_hole roundrect
		(at -15.24 15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0)
		(chamfer_ratio 0.3)
		(chamfer top_left bottom_right)
		(uuid "f6c3d963-487a-4e0e-b670-4b0433679f97")
	)
	(pad "10" thru_hole circle
		(at 10.16 15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "edab94a2-f3bc-438a-b3c2-aca260e231bd")
	)
	(pad "11" thru_hole circle
		(at 10.16 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9b9d0460-b01f-4d5d-8f38-61e52eb2ca93")
	)
	(pad "12" thru_hole circle
		(at 10.16 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f55b6177-83ad-45d4-8abc-316506e463ab")
	)
	(pad "13" thru_hole circle
		(at 10.16 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "af34ec01-ae4e-40fc-99f4-97654eb3e89b")
	)
	(pad "14" thru_hole circle
		(at 10.16 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f9aae237-f5e9-47e8-9be4-7eb18ef51010")
	)
	(pad "15" thru_hole circle
		(at 10.16 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1b9e7da7-379d-4543-add7-65ed2a1b5475")
	)
	(pad "16" thru_hole circle
		(at 10.16 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "899b639f-b0b5-499e-a3e6-5a76f0a3cd9d")
	)
	(pad "17" thru_hole circle
		(at 10.16 -2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f49b1057-0d1b-4c88-a911-6e285f4844ea")
	)
	(pad "18" thru_hole circle
		(at 10.16 -5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a192418f-dfe2-4b90-87fc-c77ddb8982c7")
	)
)
