(footprint "Conn_Terminal_5mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "8060404d-7584-4986-83fc-8fdc66016fdb")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Conn_Terminal_5mm"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "ba0e9860-90bb-4e1f-9729-155a34948ea8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "305dbe99-1b34-408d-9fe6-6e967b23caba")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "ffc24033-fd91-4e62-943a-a9215680e46e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "45eb5cea-0c1c-4aaa-9f6c-e90668d6b41d")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -2.54 5.08)
		(end -2.54 15.24)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "119e0d40-353f-47d1-98b5-88ff8db40a5f")
	)
	(fp_line
		(start -2.54 5.08)
		(end 5.08 5.08)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f51a2e25-189f-4179-b395-72dc5f427040")
	)
	(fp_line
		(start -2.54 15.24)
		(end 5.08 15.24)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "db790cd0-98bc-4595-a2d9-31df01c040a9")
	)
	(fp_line
		(start 0 10.17)
		(end 5.08 10.16)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "68c91e74-9234-42ab-9616-03dc4916c5a2")
	)
	(fp_line
		(start 2.54 5.08)
		(end -2.54 5.08)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "304b08d3-eac7-40bd-bc66-1057698c855d")
	)
	(fp_line
		(start 2.54 15.24)
		(end 2.54 5.08)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "bf0ddac2-0edb-4a23-b41b-ee1977e69b88")
	)
	(fp_line
		(start 5.08 15.24)
		(end 5.08 5.08)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c91234bb-069b-4581-9303-8bcb3d09bd83")
	)
	(fp_line
		(start -2.54 5.08)
		(end -2.54 15.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "732c8e15-78df-40c2-99f9-bd335ea3b5ea")
	)
	(fp_line
		(start -2.54 15.24)
		(end 5.08 15.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "de404b78-4786-4c16-bec1-11b1d877d0be")
	)
	(fp_line
		(start 5.08 5.08)
		(end -2.54 5.08)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "474f1c4e-8d9a-407f-8759-bf79e698274a")
	)
	(fp_line
		(start 5.08 15.24)
		(end 5.08 5.08)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2b9c4258-2f29-4247-8c0a-3d7c71959999")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "66068ab2-a7ec-4899-a895-f04295fcf364")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole oval
		(at 0 7.62 90)
		(size 2 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "be90548e-ff38-4168-9bc0-eeec75a49830")
	)
	(pad "2" thru_hole oval
		(at 0 12.7 90)
		(size 2 3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6f70d812-2e00-4800-a122-272793c65c50")
	)
)
