
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "ESP32-C3-WROOM-02U-N4" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -12.7 18.542 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "ESP32-C3-WROOM-02U-N4" (id 1) (at -12.7 -43.18 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "ESP32-C3-WROOM-02U-N4:XCVR_ESP32-C3-WROOM-02U-N4" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "1.3" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.35mm" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Espressif Systems" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "ESP32-C3-WROOM-02U-N4_0_0"
      (rectangle (start -12.7 -40.64) (end 12.7 17.78)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin power_in line (at 17.78 15.24 180.0) (length 5.08)
        (name "3V3"
          (effects (font (size 1.016 1.016)))
        )
        (number "1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -17.78 10.16 0) (length 5.08)
        (name "EN"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -15.24 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 5.08 0) (length 5.08)
        (name "IO0"
          (effects (font (size 1.016 1.016)))
        )
        (number "18"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 2.54 0) (length 5.08)
        (name "IO1"
          (effects (font (size 1.016 1.016)))
        )
        (number "17"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 0.0 0) (length 5.08)
        (name "IO2"
          (effects (font (size 1.016 1.016)))
        )
        (number "16"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 -2.54 0) (length 5.08)
        (name "IO3"
          (effects (font (size 1.016 1.016)))
        )
        (number "15"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 -5.08 0) (length 5.08)
        (name "IO4"
          (effects (font (size 1.016 1.016)))
        )
        (number "3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 -7.62 0) (length 5.08)
        (name "IO5"
          (effects (font (size 1.016 1.016)))
        )
        (number "4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 -10.16 0) (length 5.08)
        (name "IO6"
          (effects (font (size 1.016 1.016)))
        )
        (number "5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 10.16 180.0) (length 5.08)
        (name "IO7"
          (effects (font (size 1.016 1.016)))
        )
        (number "6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 7.62 180.0) (length 5.08)
        (name "IO8"
          (effects (font (size 1.016 1.016)))
        )
        (number "7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 5.08 180.0) (length 5.08)
        (name "IO9"
          (effects (font (size 1.016 1.016)))
        )
        (number "8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 2.54 180.0) (length 5.08)
        (name "IO10"
          (effects (font (size 1.016 1.016)))
        )
        (number "10"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 0.0 180.0) (length 5.08)
        (name "IO18"
          (effects (font (size 1.016 1.016)))
        )
        (number "13"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 -2.54 180.0) (length 5.08)
        (name "IO19"
          (effects (font (size 1.016 1.016)))
        )
        (number "14"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 -10.16 180.0) (length 5.08)
        (name "TXD/IO21"
          (effects (font (size 1.016 1.016)))
        )
        (number "12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 -7.62 180.0) (length 5.08)
        (name "RXD/IO20"
          (effects (font (size 1.016 1.016)))
        )
        (number "11"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -17.78 180.0) (length 5.08)
        (name "GND__1"
          (effects (font (size 1.016 1.016)))
        )
        (number "19_1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -20.32 180.0) (length 5.08)
        (name "GND__2"
          (effects (font (size 1.016 1.016)))
        )
        (number "19_2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -22.86 180.0) (length 5.08)
        (name "GND__3"
          (effects (font (size 1.016 1.016)))
        )
        (number "19_3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -25.4 180.0) (length 5.08)
        (name "GND__4"
          (effects (font (size 1.016 1.016)))
        )
        (number "19_4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -27.94 180.0) (length 5.08)
        (name "GND__5"
          (effects (font (size 1.016 1.016)))
        )
        (number "19_5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -30.48 180.0) (length 5.08)
        (name "GND__6"
          (effects (font (size 1.016 1.016)))
        )
        (number "19_6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -33.02 180.0) (length 5.08)
        (name "GND__7"
          (effects (font (size 1.016 1.016)))
        )
        (number "19_7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -35.56 180.0) (length 5.08)
        (name "GND__8"
          (effects (font (size 1.016 1.016)))
        )
        (number "19_8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -38.1 180.0) (length 5.08)
        (name "GND__9"
          (effects (font (size 1.016 1.016)))
        )
        (number "19_9"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)