(footprint "PinSocket_1x02_P2.54"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5e1403aa-0d62-459b-897f-8756eca026e5")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "PinSocket_1x02_P2.54"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "f2a9e1eb-308f-4035-bb26-aea054e2d6d5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5433eafd-fdba-4f21-8dbd-d3e3c908cb66")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "89bcbbe6-2da0-4ade-b337-b071f7d8fe78")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "89600bac-db47-4ed3-a7c1-8ef89229b0ce")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -0.12 -3.84)
		(end -0.12 -1.24)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "07686343-f33c-4296-be79-23cbc9df9485")
	)
	(fp_line
		(start -0.12 -3.84)
		(end 2.54 -3.84)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8ff6f42b-349d-4d4c-a44d-6c0456369cdc")
	)
	(fp_line
		(start -0.12 -1.24)
		(end 2.54 -1.24)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2c755848-5439-41f3-a6d1-949f3383ad1e")
	)
	(fp_line
		(start 1.21 -6.44)
		(end 2.54 -6.44)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "87fc2b51-c120-4656-b2dc-8080faf0f860")
	)
	(fp_line
		(start 2.54 -6.44)
		(end 2.54 -5.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "488e366b-31d0-4101-96d1-6865dd95071c")
	)
	(fp_line
		(start 2.54 -3.84)
		(end 2.54 -1.24)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "444d2ece-5db7-4945-b1e2-23fd6fcf043f")
	)
	(fp_line
		(start -0.59 -6.91)
		(end 2.96 -6.91)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c45af91a-a919-4ef1-baa9-b148f92887a6")
	)
	(fp_line
		(start -0.59 -0.81)
		(end -0.59 -6.91)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ef818971-7a6c-4a28-8653-c514fa0d39ad")
	)
	(fp_line
		(start 2.96 -6.91)
		(end 2.96 -0.81)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d6ad637e-6a91-408d-9658-de211c1150ab")
	)
	(fp_line
		(start 2.96 -0.81)
		(end -0.59 -0.81)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b169fb2e-1b37-4885-a667-64fa30c5dcfc")
	)
	(fp_line
		(start -0.06 -6.38)
		(end 1.845 -6.38)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ca62df82-d570-46e9-a313-3b451d06c4ae")
	)
	(fp_line
		(start -0.06 -1.3)
		(end -0.06 -6.38)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e0c637cc-e96d-4403-ac15-84c514a7628e")
	)
	(fp_line
		(start 1.845 -6.38)
		(end 2.48 -5.745)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f92f131b-4eda-476c-8094-9acc5d23c936")
	)
	(fp_line
		(start 2.48 -5.745)
		(end 2.48 -1.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6c53f148-e5c2-483f-9502-ea841154dcc8")
	)
	(fp_line
		(start 2.48 -1.3)
		(end -0.06 -1.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5c8c7790-d84e-42e7-ba12-d7aa875b9ff9")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "1fafa1bc-1e59-4f3f-bd93-4879d3c80f32")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 1.21 -5.11)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4f7075f7-8254-4131-a9f9-92d49c23bbe1")
	)
	(pad "2" thru_hole oval
		(at 1.21 -2.57)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "856af50b-1830-4709-9f6b-48298035b569")
	)
)