
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "2171750001" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -12.7 13.2842 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "2171750001" (id 1) (at -12.7 -15.24 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "2171750001:MOLEX_2171750001" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "A1" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "OPTION" "MOLEX_CONFIG" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.26mm" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Molex" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "2171750001_0_0"
      (rectangle (start -12.7 -12.7) (end 12.7 12.7)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin power_in line (at 17.78 5.08 180.0) (length 5.08)
        (name "GND1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -17.78 5.08 0) (length 5.08)
        (name "VBUS1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 10.16 0) (length 5.08)
        (name "CC1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 2.54 180.0) (length 5.08)
        (name "GND2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -17.78 2.54 0) (length 5.08)
        (name "VBUS2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 10.16 180.0) (length 5.08)
        (name "CC2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at 17.78 -2.54 180.0) (length 5.08)
        (name "SHIELD1"
          (effects (font (size 1.016 1.016)))
        )
        (number "SH1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at 17.78 -5.08 180.0) (length 5.08)
        (name "SHIELD2"
          (effects (font (size 1.016 1.016)))
        )
        (number "SH2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at 17.78 -7.62 180.0) (length 5.08)
        (name "SHIELD3"
          (effects (font (size 1.016 1.016)))
        )
        (number "SH3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at 17.78 -10.16 180.0) (length 5.08)
        (name "SHIELD4"
          (effects (font (size 1.016 1.016)))
        )
        (number "SH4"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)