(footprint "ESP32_PADS_VN-VP" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp dc70ac50-b0f1-462d-896e-1d04deceae9a)
  )
  (fp_text value "ESP32_PADS_VN-VP" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d0830e06-4bf8-4cc9-a2bc-adb5c90ccfb1)
  )
  (fp_text user "VP" (at 2.54 -7.62 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 02334255-ab51-409d-81f1-30cbd5194c78)
  )
  (fp_text user "VN" (at 2.54 -5.08 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 1d0964f5-7f9d-40ed-85d1-6778eb0bd574)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2f7db317-3357-4890-abaa-711856b4f3b6)
  )
  (pad "4" thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask") (tstamp 56ec86d3-5ed2-4b55-be5d-0c1f364bfdf8))
  (pad "5" thru_hole circle (at 0 -5.08) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask") (tstamp a2538358-7e6e-4664-a08b-d11869db182f))
)
