(footprint "Conn_UART" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 8060404d-7584-4986-83fc-8fdc66016fdb)
  )
  (fp_text value "Conn_UART" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ba0e9860-90bb-4e1f-9729-155a34948ea8)
  )
  (fp_text user "RXD" (at 2.54 15.24 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp 1a795a35-b22a-43f3-a486-b1063021684d)
  )
  (fp_text user "TXD" (at 2.54 12.7 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp 8a205637-b83e-48fc-91ad-62a29ce98930)
  )
  (fp_text user "GND" (at 2.54 7.62 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp 9008a3ab-7c09-42ca-a8fd-38edf4f42cfa)
  )
  (fp_text user "3V3" (at 2.54 10.16 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 1) (thickness 0.1)))
    (tstamp f6169012-cb39-4d0e-b154-87889a874df6)
  )
  (fp_text user "UART" (at 0 17.78 unlocked) (layer "F.SilkS" knockout)
      (effects (font (size 1 1) (thickness 0.2) bold) (justify bottom))
    (tstamp fc487470-f46c-45ca-a9f1-5b449c30c807)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 66068ab2-a7ec-4899-a895-f04295fcf364)
  )
  (pad "3V3" thru_hole circle (at 0 10.16) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask") (tstamp 09c4c65c-17f1-4721-bfd6-fa35f3058def))
  (pad "GND" thru_hole circle (at 0 7.62) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask") (tstamp 5c41aac6-f663-494d-a0f4-636d0c39bea1))
  (pad "RXD" thru_hole circle (at 0 15.24) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask") (tstamp 2c743884-b986-4e77-bf71-8d8c8664b7a4))
  (pad "TXD" thru_hole circle (at 0 12.7) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask") (tstamp c26bce4f-7c1b-4a87-92f9-aba6c298f7db))
)
